smartctl 7.2 2021-09-14 r5236 [FreeBSD 13.0-STABLE amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Toshiba 2.5" HDD MK..55GSX
Device Model:     TOSHIBA MK1655GSX
Serial Number:    --
LU WWN Device Id: 5 000039 ...
Firmware Version: FG010D
User Capacity:    160,041,885,696 bytes [160 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA8-ACS (minor revision not indicated)
SATA Version is:  SATA 2.6, 3.0 Gb/s
Local Time is:    Thu Mar 24 21:09:50 2022 EDT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM level is:     128 (quiet), recommended: 254
APM level is:     128 (minimum power consumption without standby)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  120) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  74) minutes.
SCT capabilities: 	       (0x0039)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 128
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     PO-R--   100   100   050    -    0
  3 Spin_Up_Time            POS--K   100   100   001    -    1007
  5 Reallocated_Sector_Ct   PO--CK   100   100   050    -    391
  9 Power_On_Hours          -O--CK   090   090   000    -    263576
 12 Power_Cycle_Count       -O--CK   100   100   000    -    2078
191 G-Sense_Error_Rate      -O--CK   100   100   000    -    830
192 Power-Off_Retract_Count -O--CK   100   100   000    -    48
193 Load_Cycle_Count        -O--CK   096   096   000    -    46080
194 Temperature_Celsius     -O---K   100   100   000    -    32 (Min/Max 0/58)
199 UDMA_CRC_Error_Count    -O--CK   100   100   000    -    35452817
200 Multi_Zone_Error_Rate   -O--CK   100   100   000    -    81459060
240 Head_Flying_Hours       -O--CK   092   092   000    -    200978
241 Total_LBAs_Written      -O--CK   100   100   000    -    7966498490
242 Total_LBAs_Read         -O--CK   100   100   000    -    13034000713
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O     51  Comprehensive SMART error log
0x03       GPL     R/O     64  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (64 sectors)
Device Error Count: 2667 (device log contains only the most recent 256 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 2667 [106] occurred at disk power-on lifetime: 4377 hours (182 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 41 00 02 00 00 01 c9 f9 1f 61 00  Error: UNC at LBA = 0x01c9f91f = 30013727

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 08 00 00 00 00 01 c9 f9 18 40 08     00:10:45.775  READ FPDMA QUEUED
  ef 00 10 00 02 a1 9e af 00 00 00 a0 00     00:10:45.774  SET FEATURES [Enable SATA feature]
  27 00 00 00 00 00 00 00 00 00 00 e0 00     00:10:45.774  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 03 00 45 00 00 00 00 00 00 00 a0 00     00:10:45.773  IDENTIFY DEVICE
  ef 10 03 02 45 00 00 00 00 00 00 a0 00     00:10:45.773  SET FEATURES [Set transfer mode]

Error 2666 [105] occurred at disk power-on lifetime: 4377 hours (182 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 41 00 02 00 00 01 c9 f9 1f 61 00  Error: UNC at LBA = 0x01c9f91f = 30013727

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 08 00 00 00 00 01 c9 f9 18 40 08     00:10:41.941  READ FPDMA QUEUED
  60 00 08 00 00 00 00 01 d5 77 88 40 08     00:10:41.940  READ FPDMA QUEUED
  60 00 08 00 00 00 00 01 d5 77 80 40 08     00:10:41.940  READ FPDMA QUEUED
  60 00 08 00 00 00 00 01 d5 77 78 40 08     00:10:41.932  READ FPDMA QUEUED
  60 00 08 00 00 00 00 01 c9 fa b8 40 08     00:10:41.932  READ FPDMA QUEUED

Error 2665 [104] occurred at disk power-on lifetime: 4377 hours (182 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 41 00 02 00 00 01 c9 f9 1f 61 00  Error: UNC at LBA = 0x01c9f91f = 30013727

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 08 00 00 00 00 01 c9 f9 18 40 08     00:10:34.429  READ FPDMA QUEUED
  ef 00 10 00 02 a1 9e af 00 00 00 a0 00     00:10:34.429  SET FEATURES [Enable SATA feature]
  27 00 00 00 00 00 00 00 00 00 00 e0 00     00:10:34.429  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 03 00 45 00 00 00 00 00 00 00 a0 00     00:10:34.428  IDENTIFY DEVICE
  ef 10 03 02 45 00 00 00 00 00 00 a0 00     00:10:34.428  SET FEATURES [Set transfer mode]

Error 2664 [103] occurred at disk power-on lifetime: 4377 hours (182 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 41 00 02 00 00 01 c9 f9 1f 61 00  Error: UNC at LBA = 0x01c9f91f = 30013727

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 08 00 00 00 00 01 c9 f9 18 40 08     00:10:30.584  READ FPDMA QUEUED
  ef 00 10 00 02 a1 9e af 00 00 00 a0 00     00:10:30.584  SET FEATURES [Enable SATA feature]
  27 00 00 00 00 00 00 00 00 00 00 e0 00     00:10:30.584  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 03 00 45 00 00 00 00 00 00 00 a0 00     00:10:30.583  IDENTIFY DEVICE
  ef 10 03 02 45 00 00 00 00 00 00 a0 00     00:10:30.583  SET FEATURES [Set transfer mode]

Error 2663 [102] occurred at disk power-on lifetime: 4377 hours (182 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 41 00 02 00 00 01 c9 f9 1f 61 00  Error: UNC at LBA = 0x01c9f91f = 30013727

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 08 00 00 00 00 01 c9 f9 18 40 08     00:10:26.739  READ FPDMA QUEUED
  ef 00 10 00 02 a1 9e af 00 00 00 a0 00     00:10:26.739  SET FEATURES [Enable SATA feature]
  27 00 00 00 00 00 00 00 00 00 00 e0 00     00:10:26.739  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 03 00 45 00 00 00 00 00 00 00 a0 00     00:10:26.739  IDENTIFY DEVICE
  ef 10 03 02 45 00 00 00 00 00 00 a0 00     00:10:26.739  SET FEATURES [Set transfer mode]

Error 2662 [101] occurred at disk power-on lifetime: 4377 hours (182 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 41 00 02 00 00 01 c9 f9 1f 61 00  Error: UNC at LBA = 0x01c9f91f = 30013727

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 01 00 00 00 00 00 01 c9 f8 d8 40 08     00:10:22.911  READ FPDMA QUEUED
  60 00 18 00 00 00 00 01 c3 78 c8 40 08     00:10:22.898  READ FPDMA QUEUED
  60 01 00 00 00 00 00 01 c9 c0 d8 40 08     00:10:22.896  READ FPDMA QUEUED
  60 01 00 00 00 00 00 01 c9 bf d8 40 08     00:10:22.885  READ FPDMA QUEUED
  60 00 18 00 00 00 00 01 60 5e a8 40 08     00:10:22.868  READ FPDMA QUEUED

Error 2661 [100] occurred at disk power-on lifetime: 4366 hours (181 days + 22 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 41 00 d2 00 00 02 9b 3f f3 62 00  Error: WP at LBA = 0x029b3ff3 = 43728883

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 01 00 00 e0 00 00 0e b2 6a a8 40 00     03:34:59.122  WRITE FPDMA QUEUED
  61 01 00 00 d8 00 00 0e b2 69 a8 40 00     03:34:59.122  WRITE FPDMA QUEUED
  60 00 20 00 d0 00 00 02 9b 3f e0 40 00     03:34:59.122  READ FPDMA QUEUED
  61 01 00 00 c8 00 00 0e b2 68 a8 40 00     03:34:59.122  WRITE FPDMA QUEUED
  61 01 00 00 c0 00 00 0e b2 67 a8 40 00     03:34:59.122  WRITE FPDMA QUEUED

Error 2660 [99] occurred at disk power-on lifetime: 4366 hours (181 days + 22 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 41 00 ea 00 00 02 9b 3f f3 62 00  Error: WP at LBA = 0x029b3ff3 = 43728883

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 08 00 58 00 00 00 5f 02 c0 40 00     03:34:55.612  WRITE FPDMA QUEUED
  61 00 40 00 50 00 00 00 5f b5 e8 40 00     03:34:55.612  WRITE FPDMA QUEUED
  61 00 50 00 48 00 00 0e b2 5e 58 40 00     03:34:55.020  WRITE FPDMA QUEUED
  61 01 00 00 40 00 00 0e b2 5d 58 40 00     03:34:55.020  WRITE FPDMA QUEUED
  61 00 20 00 38 00 00 09 77 ac e0 40 00     03:34:54.967  WRITE FPDMA QUEUED

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%      4383         -
# 2  Short offline       Completed without error       00%      3204         -
# 3  Short offline       Completed without error       00%      2942         -
# 4  Short offline       Completed without error       00%      2941         -
# 5  Short offline       Interrupted (host reset)      20%       155         -
# 6  Short offline       Completed without error       00%         1         -
# 7  Short offline       Completed without error       00%         1         -
# 8  Short offline       Completed without error       00%         1         -
# 9  Short offline       Completed without error       00%         1         -
#10  Short offline       Completed without error       00%         0         -
#11  Short offline       Completed without error       00%         0         -
#12  Short offline       Completed without error       00%         0         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  2
SCT Version (vendor specific):       1 (0x0001)
Device State:                        Active (0)
Current Temperature:                    32 Celsius
Power Cycle Min/Max Temperature:     25/35 Celsius
Lifetime    Min/Max Temperature:      0/58 Celsius
Specified Max Operating Temperature:    37 Celsius
Under/Over Temperature Limit Count:  25/0

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        10 minutes
Min/Max recommended Temperature:     15/55 Celsius
Min/Max Temperature Limit:           10/60 Celsius
Temperature History Size (Index):    478 (260)

SCT Error Recovery Control:
           Read: Disabled
          Write: Disabled

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  4            0  Command failed due to ICRC error
0x0002  4            0  R_ERR response for data FIS
0x0003  4            0  R_ERR response for device-to-host data FIS
0x0004  4            0  R_ERR response for host-to-device data FIS
0x0005  4            0  R_ERR response for non-data FIS
0x0006  4            0  R_ERR response for device-to-host non-data FIS
0x0007  4            0  R_ERR response for host-to-device non-data FIS
0x0008  4            0  Device-to-host non-data FIS retries
0x0009  4            5  Transition from drive PhyRdy to drive PhyNRdy
0x000a  4            5  Device-to-host register FISes sent due to a COMRESET
0x000b  4            0  CRC errors within host-to-device FIS
0x000d  4            0  Non-CRC errors within host-to-device FIS
0x000f  4            0  R_ERR response for host-to-device data FIS, CRC
0x0010  4            0  R_ERR response for host-to-device data FIS, non-CRC
0x0012  4            0  R_ERR response for host-to-device non-data FIS, CRC
0x0013  4            0  R_ERR response for host-to-device non-data FIS, non-CRC

