smartctl 7.1 2019-12-30 r5022 [x86_64-unknown-openbsd6.8] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Crucial/Micron RealSSD m4/C400/P400
Device Model:     M4-CT064M4SSD2
Serial Number:    --
LU WWN Device Id: 5 00a075 ...
Firmware Version: 070H
User Capacity:    64,023,257,088 bytes [64.0 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
Form Factor:      2.5 inches
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ACS-2, ATA8-ACS T13/1699-D revision 6
SATA Version is:  SATA 3.0, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Fri Jun 11 00:45:48 2021 CEST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  295) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (   4) minutes.
Conveyance self-test routine
recommended polling time: 	 (   3) minutes.
SCT capabilities: 	       (0x003d)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  1 Raw_Read_Error_Rate     0x002f   100   100   050    Pre-fail  Always       -       0
  5 Reallocated_Sector_Ct   0x0033   100   100   010    Pre-fail  Always       -       0
  9 Power_On_Hours          0x0032   100   100   001    Old_age   Always       -       18683
 12 Power_Cycle_Count       0x0032   100   100   001    Old_age   Always       -       3980
170 Grown_Failing_Block_Ct  0x0033   100   100   010    Pre-fail  Always       -       0
171 Program_Fail_Count      0x0032   100   100   001    Old_age   Always       -       0
172 Erase_Fail_Count        0x0032   100   100   001    Old_age   Always       -       0
173 Wear_Leveling_Count     0x0033   097   097   010    Pre-fail  Always       -       104
174 Unexpect_Power_Loss_Ct  0x0032   100   100   001    Old_age   Always       -       1512
181 Non4k_Aligned_Access    0x0022   100   100   001    Old_age   Always       -       938 217 721
183 SATA_Iface_Downshift    0x0032   100   100   001    Old_age   Always       -       0
184 End-to-End_Error        0x0033   100   100   050    Pre-fail  Always       -       0
187 Reported_Uncorrect      0x0032   100   100   001    Old_age   Always       -       0
188 Command_Timeout         0x0032   100   100   001    Old_age   Always       -       0
189 Factory_Bad_Block_Ct    0x000e   100   100   001    Old_age   Always       -       50
194 Temperature_Celsius     0x0022   100   100   000    Old_age   Always       -       0
195 Hardware_ECC_Recovered  0x003a   100   100   001    Old_age   Always       -       0
196 Reallocated_Event_Count 0x0032   100   100   001    Old_age   Always       -       0
197 Current_Pending_Sector  0x0032   100   100   001    Old_age   Always       -       0
198 Offline_Uncorrectable   0x0030   100   100   001    Old_age   Offline      -       0
199 UDMA_CRC_Error_Count    0x0032   100   100   001    Old_age   Always       -       1
202 Perc_Rated_Life_Used    0x0018   097   097   001    Old_age   Offline      -       3
206 Write_Error_Rate        0x000e   100   100   001    Old_age   Always       -       0

SMART Error Log Version: 1
Warning: ATA error count 0 inconsistent with error log pointer 1

ATA Error Count: 0
	CR = Command Register [HEX]
	FR = Features Register [HEX]
	SC = Sector Count Register [HEX]
	SN = Sector Number Register [HEX]
	CL = Cylinder Low Register [HEX]
	CH = Cylinder High Register [HEX]
	DH = Device/Head Register [HEX]
	DC = Device Command Register [HEX]
	ER = Error register [HEX]
	ST = Status register [HEX]
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 0 occurred at disk power-on lifetime: 14336 hours (597 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  00 50 00 28 5a 89 40   at LBA = 0x00895a28 = 9001512

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  61 00 00 28 a0 8a 40 00      19:32:32.448  WRITE FPDMA QUEUED
  61 00 00 28 9a 89 40 00      19:32:32.448  WRITE FPDMA QUEUED
  61 00 00 28 90 89 40 00      19:32:32.448  WRITE FPDMA QUEUED
  61 00 00 28 8a 89 40 00      19:32:32.448  WRITE FPDMA QUEUED
  61 00 00 28 80 89 40 00      19:32:32.448  WRITE FPDMA QUEUED

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Aborted by host               00%      6871         -
# 2  Short offline       Aborted by host               00%      6871         -
# 3  Short offline       Aborted by host               00%      6868         -
# 4  Short offline       Aborted by host               00%      6854         -
# 5  Short offline       Aborted by host               00%      6843         -
# 6  Short offline       Aborted by host               00%      6833         -
# 7  Short offline       Aborted by host               00%      6823         -
# 8  Short offline       Aborted by host               00%      6823         -
# 9  Short offline       Aborted by host               00%      6823         -
#10  Short offline       Aborted by host               00%      6823         -
#11  Short offline       Aborted by host               00%      6823         -
#12  Short offline       Aborted by host               00%      6822         -
#13  Short offline       Aborted by host               00%      6822         -
#14  Short offline       Aborted by host               00%      6822         -
#15  Short offline       Aborted by host               00%      6808         -
#16  Short offline       Aborted by host               00%      6783         -
#17  Short offline       Aborted by host               00%      6782         -
#18  Short offline       Aborted by host               00%      6781         -
#19  Short offline       Aborted by host               00%      6781         -
#20  Short offline       Aborted by host               00%      6758         -
#21  Short offline       Aborted by host               00%      6757         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

