smartctl 7.1 2019-12-30 r5022 [FreeBSD 12.1-STABLE i386] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Western Digital Caviar
Device Model:     WDC WD800BB-00HEA0
Serial Number:    --
Firmware Version: 13.03G13
User Capacity:    80,026,361,856 bytes [80.0 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA/ATAPI-6 (minor revision not indicated)
Local Time is:    Sun Oct  4 21:30:13 2020 EEST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM level is:     254 (maximum performance), recommended: 128
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED
See vendor-specific Attribute list for marginal Attributes.

General SMART Values:
Offline data collection status:  (0x84)	Offline data collection activity
					was suspended by an interrupting command from host.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		( 2460) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					No General Purpose Logging support.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  35) minutes.
Conveyance self-test routine
recommended polling time: 	 (   5) minutes.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     PO-R--   200   200   051    -    10794
  3 Spin_Up_Time            POS---   100   100   021    -    2375
  4 Start_Stop_Count        -O--CK   097   097   040    -    3528
  5 Reallocated_Sector_Ct   PO--CK   197   197   140    -    20
  7 Seek_Error_Rate         PO-R--   200   200   051    -    0
  9 Power_On_Hours          -O--CK   001   001   000    -    103742
 10 Spin_Retry_Count        PO--C-   100   100   051    -    0
 11 Calibration_Retry_Count PO--C-   100   100   051    -    0
 12 Power_Cycle_Count       -O--CK   098   098   000    -    2493
194 Temperature_Celsius     -O---K   112   010   000    -    31
196 Reallocated_Event_Count -O--CK   199   199   000    -    1
197 Current_Pending_Sector  -O--C-   200   151   000    -    0
198 Offline_Uncorrectable   -O--C-   200   149   000    -    0
199 UDMA_CRC_Error_Count    -O-R--   200   001   000    -    11711
200 Multi_Zone_Error_Rate   P--R--   200   001   051    Past 0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

Read SMART Log Directory failed: Input/output error

General Purpose Log Directory not supported

SMART Extended Comprehensive Error Log (GP Log 0x03) not supported

SMART Error Log Version: 1
Warning: ATA error count 15969 inconsistent with error log pointer 5

ATA Error Count: 15969 (device log contains only the most recent five errors)
	CR = Command Register [HEX]
	FR = Features Register [HEX]
	SC = Sector Count Register [HEX]
	SN = Sector Number Register [HEX]
	CL = Cylinder Low Register [HEX]
	CH = Cylinder High Register [HEX]
	DH = Device/Head Register [HEX]
	DC = Device Command Register [HEX]
	ER = Error register [HEX]
	ST = Status register [HEX]
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 15969 occurred at disk power-on lifetime: 2732 hours (113 days + 20 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 01 7b f6 ad f1  Error: UNC 1 sectors at LBA = 0x01adf67b = 28178043

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 02 7a f6 ad 01 51   5d+14:51:29.500  READ DMA
  c8 00 02 7a f6 ad 01 51   5d+14:51:27.560  READ DMA
  c8 00 02 7a f6 ad 01 51   5d+14:51:25.650  READ DMA
  c8 00 02 7a f6 ad 01 51   5d+14:51:23.720  READ DMA
  c8 00 02 7a f6 ad 01 51   5d+14:51:21.805  READ DMA

Error 15968 occurred at disk power-on lifetime: 2732 hours (113 days + 20 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 01 7b f6 ad f1  Error: UNC 1 sectors at LBA = 0x01adf67b = 28178043

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 02 7a f6 ad 01 51   5d+14:51:27.560  READ DMA
  c8 00 02 7a f6 ad 01 51   5d+14:51:25.650  READ DMA
  c8 00 02 7a f6 ad 01 51   5d+14:51:23.720  READ DMA
  c8 00 02 7a f6 ad 01 51   5d+14:51:21.805  READ DMA
  c8 00 02 78 f6 ad 01 51   5d+14:51:21.800  READ DMA

Error 15967 occurred at disk power-on lifetime: 2732 hours (113 days + 20 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 01 7b f6 ad f1  Error: UNC 1 sectors at LBA = 0x01adf67b = 28178043

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 02 7a f6 ad 01 51   5d+14:51:25.650  READ DMA
  c8 00 02 7a f6 ad 01 51   5d+14:51:23.720  READ DMA
  c8 00 02 7a f6 ad 01 51   5d+14:51:21.805  READ DMA
  c8 00 02 78 f6 ad 01 51   5d+14:51:21.800  READ DMA
  c8 00 02 76 f6 ad 01 51   5d+14:51:21.800  READ DMA

Error 15966 occurred at disk power-on lifetime: 2732 hours (113 days + 20 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 01 7b f6 ad f1  Error: UNC 1 sectors at LBA = 0x01adf67b = 28178043

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 02 7a f6 ad 01 51   5d+14:51:23.720  READ DMA
  c8 00 02 7a f6 ad 01 51   5d+14:51:21.805  READ DMA
  c8 00 02 78 f6 ad 01 51   5d+14:51:21.800  READ DMA
  c8 00 02 76 f6 ad 01 51   5d+14:51:21.800  READ DMA
  c8 00 02 74 f6 ad 01 51   5d+14:51:21.800  READ DMA

Error 15965 occurred at disk power-on lifetime: 2732 hours (113 days + 20 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 01 7b f6 ad f1  Error: UNC 1 sectors at LBA = 0x01adf67b = 28178043

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 02 7a f6 ad 01 51   5d+14:51:21.805  READ DMA
  c8 00 02 78 f6 ad 01 51   5d+14:51:21.800  READ DMA
  c8 00 02 76 f6 ad 01 51   5d+14:51:21.800  READ DMA
  c8 00 02 74 f6 ad 01 51   5d+14:51:21.800  READ DMA
  c8 00 02 72 f6 ad 01 51   5d+14:51:21.800  READ DMA

SMART Extended Self-test Log (GP Log 0x07) not supported

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%     38045         -
# 2  Short offline       Completed without error       00%     37877         -
# 3  Short offline       Completed without error       00%     37780         -
# 4  Short offline       Completed without error       00%     37612         -
# 5  Short offline       Completed without error       00%     37444         -
# 6  Short offline       Completed without error       00%     37277         -
# 7  Short offline       Completed without error       00%     37109         -
# 8  Short offline       Completed without error       00%     36941         -
# 9  Short offline       Completed without error       00%     36773         -
#10  Short offline       Completed without error       00%     36606         -
#11  Short offline       Completed without error       00%     36438         -
#12  Short offline       Completed without error       00%     36270         -
#13  Short offline       Completed without error       00%     36102         -
#14  Short offline       Completed without error       00%     35935         -
#15  Short offline       Completed without error       00%     35767         -
#16  Short offline       Completed without error       00%     35599         -
#17  Short offline       Completed without error       00%     35432         -
#18  Short offline       Completed without error       00%     35264         -
#19  Short offline       Completed without error       00%     35096         -
#20  Short offline       Completed without error       00%     34928         -
#21  Short offline       Completed without error       00%     34761         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Commands not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11) not supported



