smartctl 7.3 2022-02-28 r5338 [FreeBSD 13.0-RELEASE-p12 amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Barracuda 7200.14 (AF)
Device Model:     ST2000DM001-9YN164
Serial Number:    --
LU WWN Device Id: 5 000c50 ...
Firmware Version: CC4H
User Capacity:    2,000,398,934,016 bytes [2.00 TB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Rotation Rate:    7200 rpm
Device is:        In smartctl database 7.2/5254
ATA Version is:   ATA8-ACS T13/1699-D revision 4
SATA Version is:  SATA 3.0, 6.0 Gb/s (current: 1.5 Gb/s)
Local Time is:    Sun Aug 14 12:34:21 2022 MSK
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     254 (maximum performance)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  575) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 ( 223) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x3085)	SCT Status supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   118   099   006    -    187295952
  3 Spin_Up_Time            PO----   095   094   000    -    0
  4 Start_Stop_Count        -O--CK   100   100   020    -    104
  5 Reallocated_Sector_Ct   PO--CK   100   100   036    -    0
  7 Seek_Error_Rate         POSR--   079   060   030    -    13128501680
  9 Power_On_Hours          -O--CK   065   065   000    -    31348
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   100   100   020    -    101
183 Runtime_Bad_Block       -O--CK   001   001   000    -    4005
184 End-to-End_Error        -O--CK   100   100   099    -    0
187 Reported_Uncorrect      -O--CK   001   001   000    -    109
188 Command_Timeout         -O--CK   100   097   000    -    119 119 132
189 High_Fly_Writes         -O-RCK   099   099   000    -    1
190 Airflow_Temperature_Cel -O---K   058   051   045    -    42 (Min/Max 27/48)
191 G-Sense_Error_Rate      -O--CK   100   100   000    -    0
192 Power-Off_Retract_Count -O--CK   100   100   000    -    70
193 Load_Cycle_Count        -O--CK   050   050   000    -    100029
194 Temperature_Celsius     -O---K   042   049   000    -    42 (0 19 0 0 0)
197 Current_Pending_Sector  -O--C-   100   100   000    -    0
198 Offline_Uncorrectable   ----C-   100   100   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   131   000    -    71982
240 Head_Flying_Hours       ------   100   253   000    -    24686h+10m+01.953s
241 Total_LBAs_Written      ------   100   253   000    -    64996686611340
242 Total_LBAs_Read         ------   100   253   000    -    194221905140606
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      5  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x21       GPL     R/O      1  Write stream error log
0x22       GPL     R/O      1  Read stream error log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS      20  Device vendor specific log
0xa2       GPL     VS    4496  Device vendor specific log
0xa8       GPL,SL  VS      20  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xab       GPL     VS       1  Device vendor specific log
0xb0       GPL     VS    5067  Device vendor specific log
0xbd       GPL     VS     512  Device vendor specific log
0xbe-0xbf  GPL     VS   65535  Device vendor specific log
0xc0       GPL,SL  VS       1  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 109 (device log contains only the most recent 20 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 109 [8] occurred at disk power-on lifetime: 25540 hours (1064 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 9f 17 20 18 00 00  Error: UNC at LBA = 0x9f172018 = 2669092888

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 00 69 e1 af c8 40 00 15d+12:26:16.034  READ FPDMA QUEUED
  60 00 00 00 08 00 00 69 e1 af b8 40 00 15d+12:26:16.034  READ FPDMA QUEUED
  60 00 00 06 80 00 00 2a 44 4f f0 40 00 15d+12:26:16.034  READ FPDMA QUEUED
  60 00 00 02 b0 00 00 9f 17 1e b8 40 00 15d+12:26:16.034  READ FPDMA QUEUED
  2f 00 00 00 01 00 00 00 00 00 10 00 00 15d+12:26:15.986  READ LOG EXT

Error 108 [7] occurred at disk power-on lifetime: 25540 hours (1064 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 9f 17 20 18 00 00  Error: UNC at LBA = 0x9f172018 = 2669092888

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 00 69 e1 af c8 40 00 15d+12:26:13.086  READ FPDMA QUEUED
  60 00 00 00 08 00 00 69 e1 af b8 40 00 15d+12:26:13.086  READ FPDMA QUEUED
  60 00 00 06 80 00 00 2a 44 4f f0 40 00 15d+12:26:13.086  READ FPDMA QUEUED
  60 00 00 02 b0 00 00 9f 17 1e b8 40 00 15d+12:26:13.086  READ FPDMA QUEUED
  2f 00 00 00 01 00 00 00 00 00 10 00 00 15d+12:26:13.086  READ LOG EXT

Error 107 [6] occurred at disk power-on lifetime: 25540 hours (1064 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 9f 17 20 18 00 00  Error: UNC at LBA = 0x9f172018 = 2669092888

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 02 b0 00 00 28 65 c2 88 40 00 15d+12:26:10.331  READ FPDMA QUEUED
  60 00 00 02 b0 00 00 28 65 bf d8 40 00 15d+12:26:10.331  READ FPDMA QUEUED
  60 00 00 02 b0 00 00 28 65 ba f8 40 00 15d+12:26:10.330  READ FPDMA QUEUED
  60 00 00 02 b0 00 00 9f 17 1e b8 40 00 15d+12:26:10.322  READ FPDMA QUEUED
  61 00 00 00 10 00 00 00 00 02 10 40 00 15d+12:26:10.315  WRITE FPDMA QUEUED

Error 106 [5] occurred at disk power-on lifetime: 25540 hours (1064 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 9f 17 20 18 00 00  Error: UNC at LBA = 0x9f172018 = 2669092888

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 08 00 00 00 0a 29 87 58 40 00 15d+12:26:07.414  READ FPDMA QUEUED
  60 00 00 00 08 00 00 2a 42 c1 38 40 00 15d+12:26:07.414  READ FPDMA QUEUED
  60 00 00 00 08 00 00 69 e1 b0 80 40 00 15d+12:26:07.414  READ FPDMA QUEUED
  60 00 00 02 b0 00 00 9f 17 21 68 40 00 15d+12:26:07.414  READ FPDMA QUEUED
  60 00 00 02 b0 00 00 9f 17 1e b8 40 00 15d+12:26:07.414  READ FPDMA QUEUED

Error 105 [4] occurred at disk power-on lifetime: 25540 hours (1064 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 9f 17 20 18 00 00  Error: UNC at LBA = 0x9f172018 = 2669092888

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 02 b0 00 00 9f 17 21 68 40 00 15d+12:26:04.597  READ FPDMA QUEUED
  60 00 00 02 b0 00 00 9f 17 1e b8 40 00 15d+12:26:04.597  READ FPDMA QUEUED
  2f 00 00 00 01 00 00 00 00 00 10 00 00 15d+12:26:04.511  READ LOG EXT
  60 00 00 02 b0 00 00 9f 17 1c 08 40 00 15d+12:26:01.701  READ FPDMA QUEUED
  60 00 00 02 b0 00 00 9f 17 13 f8 40 00 15d+12:26:01.675  READ FPDMA QUEUED

Error 104 [3] occurred at disk power-on lifetime: 25540 hours (1064 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 9f 17 20 18 00 00  Error: UNC at LBA = 0x9f172018 = 2669092888

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 02 b0 00 00 9f 17 1c 08 40 00 15d+12:26:01.701  READ FPDMA QUEUED
  60 00 00 02 b0 00 00 9f 17 13 f8 40 00 15d+12:26:01.675  READ FPDMA QUEUED
  60 00 00 02 b0 00 00 9f 17 19 58 40 00 15d+12:26:01.670  READ FPDMA QUEUED
  60 00 00 02 b0 00 00 9f 17 16 a8 40 00 15d+12:26:01.662  READ FPDMA QUEUED
  60 00 00 02 b0 00 00 9f 17 0e 98 40 00 15d+12:25:59.589  READ FPDMA QUEUED

Error 103 [2] occurred at disk power-on lifetime: 24379 hours (1015 days + 19 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 7b c4 47 a8 00 00  Error: UNC at LBA = 0x7bc447a8 = 2076460968

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 d0 ff 00 80 00 00 7b ba 3f 00 40 00     01:39:52.841  READ DMA EXT
  25 d0 ff 00 80 00 00 7b ba 3e 80 40 00     01:39:52.832  READ DMA EXT
  25 d0 ff 00 80 00 00 7b aa 4d 00 40 00     01:39:50.025  READ DMA EXT
  25 d0 ff 00 80 00 00 7b aa 4c 80 40 00     01:39:50.013  READ DMA EXT
  25 d0 ff 00 80 00 00 7b aa 4c 00 40 00     01:39:50.012  READ DMA EXT

Error 102 [1] occurred at disk power-on lifetime: 24369 hours (1015 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 7b c4 47 a8 00 00  Error: UNC at LBA = 0x7bc447a8 = 2076460968

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 d8 00 00 80 00 00 7b c4 47 80 40 00     01:59:04.504  READ DMA EXT
  25 d8 00 00 80 00 00 7b c4 47 00 40 00     01:59:04.504  READ DMA EXT
  25 d8 00 00 80 00 00 7b c4 46 80 40 00     01:59:04.503  READ DMA EXT
  25 d8 00 00 80 00 00 7b c4 46 00 40 00     01:59:04.503  READ DMA EXT
  25 d8 00 00 80 00 00 7b c4 45 80 40 00     01:59:04.502  READ DMA EXT

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%     20066         -
# 2  Short offline       Completed without error       00%     20066         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       522 (0x020a)
Device State:                        Active (0)
Current Temperature:                    42 Celsius
Power Cycle Min/Max Temperature:     27/48 Celsius
Lifetime    Min/Max Temperature:     19/49 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Data Table command not supported

SCT Error Recovery Control command not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2         4523  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS



