smartctl 7.4 2023-08-01 r5530 [FreeBSD 14.1-RELEASE-p5 amd64] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     SAMSUNG SpinPoint P80
Device Model:     SAMSUNG SP0812C
Serial Number:    --
Firmware Version: SU100-34
User Capacity:    80,060,424,192 bytes [80.0 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database 7.3/5528
ATA Version is:   ATA/ATAPI-7 T13/1532D revision 0
Local Time is:    Sun Nov 17 16:46:19 2024 -03
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Disabled
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		( 3000) seconds.
Offline data collection
capabilities: 			 (0x1b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					No Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					No General Purpose Logging support.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (  50) minutes.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   100   100   051    -    0
  3 Spin_Up_Time            POS---   100   100   025    -    4160
  4 Start_Stop_Count        -O--CK   089   089   000    -    11741
  5 Reallocated_Sector_Ct   PO--CK   100   100   011    -    0
  7 Seek_Error_Rate         POSR--   100   100   051    -    0
  8 Seek_Time_Performance   P-S--K   100   100   015    -    0
  9 Power_On_Half_Minutes   -O--CK   096   096   000    -    21160h+47m
 10 Spin_Retry_Count        PO--CK   100   100   051    -    0
 11 Calibration_Retry_Count -O--C-   100   100   000    -    0
 12 Power_Cycle_Count       -O--CK   093   093   000    -    7100
194 Temperature_Celsius     -O---K   145   082   000    -    31
195 Hardware_ECC_Recovered  -O-RC-   100   100   000    -    88563
196 Reallocated_Event_Count -O--CK   095   095   000    -    12
197 Current_Pending_Sector  -O--C-   100   100   000    -    0
198 Total_Offl_Uncorrectabl ----CK   100   100   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    0
200 Multi_Zone_Error_Rate   -O-R--   100   100   051    -    0
201 Soft_Read_Error_Rate    -O-R--   100   100   051    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory not supported

SMART Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00           SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      2  Comprehensive SMART error log
0x06           SL  R/O      2  SMART self-test log
0x80-0x9f      SL  R/W     16  Host vendor specific log

SMART Extended Comprehensive Error Log (GP Log 0x03) not supported

SMART Error Log Version: 1
ATA Error Count: 2253 (device log contains only the most recent five errors)
	CR = Command Register [HEX]
	FR = Features Register [HEX]
	SC = Sector Count Register [HEX]
	SN = Sector Number Register [HEX]
	CL = Cylinder Low Register [HEX]
	CH = Cylinder High Register [HEX]
	DH = Device/Head Register [HEX]
	DC = Device Command Register [HEX]
	ER = Error register [HEX]
	ST = Status register [HEX]
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 2253 occurred at disk power-on lifetime: 20847 hours (868 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 80 40 31 2d e2  Error: UNC 128 sectors at LBA = 0x022d3140 = 36516160

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 80 40 31 2d e2 00      00:10:07.750  READ DMA
  ca 00 10 70 43 68 e0 00      00:10:07.750  WRITE DMA
  ca 00 00 70 42 68 e0 00      00:10:07.750  WRITE DMA
  ca 00 00 70 41 68 e0 00      00:10:07.750  WRITE DMA
  ca 00 00 70 40 68 e0 00      00:10:07.688  WRITE DMA

Error 2252 occurred at disk power-on lifetime: 20815 hours (867 days + 7 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 00 18 0e 18 e2  Error: UNC at LBA = 0x02180e18 = 35130904

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 00 18 0e 18 e2 00      00:39:20.313  READ DMA
  c8 00 40 dc b5 79 e0 00      00:39:20.313  READ DMA
  c8 00 08 98 ff 54 e2 00      00:39:20.313  READ DMA
  ca 00 90 38 04 d8 e2 00      00:39:20.313  WRITE DMA
  ca 00 00 38 03 d8 e2 00      00:39:20.313  WRITE DMA

Error 2251 occurred at disk power-on lifetime: 20812 hours (867 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 00 18 0e 18 e2  Error: UNC at LBA = 0x02180e18 = 35130904

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 00 18 0e 18 e2 00      00:11:47.875  READ DMA
  ca 00 20 c0 ea a3 e1 00      00:11:47.875  WRITE DMA
  c8 00 40 1a a5 43 e2 00      00:11:47.875  READ DMA
  ca 00 20 20 20 a4 e1 00      00:11:47.875  WRITE DMA
  ca 00 20 c0 1e a4 e1 00      00:11:47.875  WRITE DMA

Error 2250 occurred at disk power-on lifetime: 20782 hours (865 days + 22 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 00 00 12 29 e2  Error: UNC at LBA = 0x02291200 = 36246016

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 00 00 12 29 e2 00      00:02:57.688  READ DMA
  c8 00 02 12 12 29 e2 00      00:02:57.625  READ DMA

Error 2249 occurred at disk power-on lifetime: 20782 hours (865 days + 22 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 00 00 12 29 e2  Error: UNC at LBA = 0x02291200 = 36246016

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 00 00 12 29 e2 00      00:02:56.625  READ DMA
  c8 00 00 00 33 9b e0 00      00:02:56.563  READ DMA
  c8 00 02 02 12 29 e2 00      00:02:56.563  READ DMA

SMART Extended Self-test Log (GP Log 0x07) not supported

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%     20843         -
# 2  Short offline       Interrupted (host reset)      80%     15491         -
# 3  Short offline       Completed without error       00%     13535         -
# 4  Short offline       Interrupted (host reset)      80%     12021         -
# 5  Short offline       Completed without error       00%     12019         -
# 6  Short offline       Completed without error       00%     11432         -
# 7  Short offline       Completed without error       00%      7737         -
# 8  Short offline       Interrupted (host reset)      20%      5867         -
# 9  Short offline       Interrupted (host reset)      40%      5549         -
#10  Short offline       Completed without error       00%      5546         -
#11  Short offline       Completed without error       00%      5534         -
#12  Short offline       Interrupted (host reset)      80%      5528         -
#13  Short offline       Completed without error       00%      5525         -
#14  Short offline       Completed without error       00%      5421         -

Selective Self-tests/Logging not supported

SCT Commands not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11) not supported

