smartctl 7.4 2023-08-01 r5530 [FreeBSD 14.0-RELEASE-p5 amd64] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     WDC WD10JPCX-24UE4T0
Serial Number:    --
LU WWN Device Id: 5 0014ee ...
Firmware Version: 01.01A01
User Capacity:    1,000,204,886,016 bytes [1.00 TB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Rotation Rate:    5400 rpm
Device is:        Not in smartctl database 7.3/5528
ATA Version is:   ACS-2 (minor revision not indicated)
SATA Version is:  SATA 3.0, 6.0 Gb/s (current: 3.0 Gb/s)
Local Time is:    Fri Mar  8 22:38:59 2024 -05
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     96 (intermediate level with standby)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(17640) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 ( 198) minutes.
Conveyance self-test routine
recommended polling time: 	 (   5) minutes.
SCT capabilities: 	       (0x7035)	SCT Status supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR-K   200   200   051    -    11122
  3 Spin_Up_Time            POS--K   186   176   021    -    1658
  4 Start_Stop_Count        -O--CK   046   046   000    -    54368
  5 Reallocated_Sector_Ct   PO--CK   200   200   140    -    5
  7 Seek_Error_Rate         POSR-K   200   200   051    -    0
  9 Power_On_Hours          -O--CK   093   093   000    -    5366
 10 Spin_Retry_Count        -O--CK   100   100   000    -    0
 11 Calibration_Retry_Count -O--CK   100   100   000    -    0
 12 Power_Cycle_Count       -O--CK   097   097   000    -    3264
192 Power-Off_Retract_Count -O--CK   200   200   000    -    241
193 Load_Cycle_Count        -O--CK   167   167   000    -    99514
194 Temperature_Celsius     -O---K   106   093   000    -    41
196 Reallocated_Event_Count -O--CK   199   199   000    -    1
197 Current_Pending_Sector  -O--CK   200   200   000    -    0
198 Offline_Uncorrectable   ----CK   100   253   000    -    0
199 UDMA_CRC_Error_Count    -O--CK   200   200   000    -    2
200 Multi_Zone_Error_Rate   ---R--   100   253   000    -    0
240 Head_Flying_Hours       -O--CK   094   094   000    -    5057
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      6  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa0-0xa7  GPL,SL  VS      16  Device vendor specific log
0xa8-0xb6  GPL,SL  VS       1  Device vendor specific log
0xb7       GPL,SL  VS      38  Device vendor specific log
0xbd       GPL,SL  VS       1  Device vendor specific log
0xc0       GPL,SL  VS       1  Device vendor specific log
0xc1       GPL     VS      93  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (6 sectors)
Device Error Count: 6726 (device log contains only the most recent 24 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 6726 [5] occurred at disk power-on lifetime: 5277 hours (219 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 01 00 00 03 f1 3d c8 40 00  Error: UNC at LBA = 0x03f13dc8 = 66141640

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 20 00 20 00 00 02 1b b1 ed 40 00     01:08:26.990  READ FPDMA QUEUED
  60 00 40 00 18 00 00 03 f1 3d c8 40 00     01:08:26.985  READ FPDMA QUEUED
  60 00 40 00 10 00 00 03 f1 3d 88 40 00     01:08:26.985  READ FPDMA QUEUED
  60 00 40 00 08 00 00 03 f1 3d 48 40 00     01:08:26.984  READ FPDMA QUEUED
  60 00 40 00 f8 00 00 03 f1 3d 08 40 00     01:08:26.983  READ FPDMA QUEUED

Error 6725 [4] occurred at disk power-on lifetime: 5168 hours (215 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 7f 00 00 03 ca 6e c8 e0 00  Error: UNC 127 sectors at LBA = 0x03ca6ec8 = 63598280

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 60 60 00 7f 00 00 03 ca 6e 61 e0 08     00:49:40.098  READ DMA EXT
  25 60 60 00 7f 00 00 03 ca 6d e2 e0 08     00:49:40.097  READ DMA EXT
  25 60 60 00 7f 00 00 03 ca 6d 63 e0 08     00:49:40.097  READ DMA EXT
  25 60 60 00 7f 00 00 03 ca 6c e4 e0 08     00:49:40.096  READ DMA EXT
  25 60 60 00 7f 00 00 03 ca 6c 65 e0 08     00:49:40.096  READ DMA EXT

Error 6724 [3] occurred at disk power-on lifetime: 4657 hours (194 days + 1 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 03 a5 d1 10 40 00  Error: UNC at LBA = 0x03a5d110 = 61198608

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 60 00 50 00 00 03 a5 d2 60 40 00     01:36:38.624  READ FPDMA QUEUED
  60 01 00 00 48 00 00 03 a5 d1 60 40 00     01:36:38.624  READ FPDMA QUEUED
  60 01 00 00 40 00 00 03 a5 d0 60 40 00     01:36:38.623  READ FPDMA QUEUED
  60 01 00 00 38 00 00 03 a5 cf 60 40 00     01:36:38.622  READ FPDMA QUEUED
  60 01 00 00 30 00 00 03 a5 ce 60 40 00     01:36:38.622  READ FPDMA QUEUED

Error 6723 [2] occurred at disk power-on lifetime: 4094 hours (170 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 01 00 00 03 df 64 5f e0 00  Error: UNC at LBA = 0x03df645f = 64971871

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  29 00 00 00 01 00 00 03 df 64 5f e0 00     06:34:30.583  READ MULTIPLE EXT
  39 00 00 00 01 00 00 03 df 64 5e e0 00     06:34:30.417  WRITE MULTIPLE EXT
  29 00 00 00 01 00 00 03 df 64 5e e0 00     06:34:30.417  READ MULTIPLE EXT
  25 00 00 00 01 00 00 03 df 64 5f e0 00     06:34:30.396  READ DMA EXT
  29 00 00 00 01 00 00 03 df 64 5e e0 00     06:34:30.396  READ MULTIPLE EXT

Error 6722 [1] occurred at disk power-on lifetime: 4094 hours (170 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 01 00 00 03 df 64 5f e0 00  Error: UNC 1 sectors at LBA = 0x03df645f = 64971871

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 01 00 00 03 df 64 5f e0 00     06:34:30.396  READ DMA EXT
  29 00 00 00 01 00 00 03 df 64 5e e0 00     06:34:30.396  READ MULTIPLE EXT
  39 00 00 00 01 00 00 03 df 64 5e e0 00     06:34:30.395  WRITE MULTIPLE EXT
  39 00 00 00 01 00 00 03 df 64 5d e0 00     06:34:30.395  WRITE MULTIPLE EXT
  39 00 00 00 01 00 00 03 df 64 5e e0 00     06:34:30.395  WRITE MULTIPLE EXT

Error 6721 [0] occurred at disk power-on lifetime: 4094 hours (170 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 01 00 00 03 df 64 5e e0 00  Error: UNC at LBA = 0x03df645e = 64971870

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  29 00 00 00 01 00 00 03 df 64 5e e0 00     06:34:30.201  READ MULTIPLE EXT
  39 00 00 00 01 00 00 03 df 64 5d e0 00     06:34:30.036  WRITE MULTIPLE EXT
  29 00 00 00 01 00 00 03 df 64 5d e0 00     06:34:30.035  READ MULTIPLE EXT
  25 00 00 00 01 00 00 03 df 64 5e e0 00     06:34:30.014  READ DMA EXT
  29 00 00 00 01 00 00 03 df 64 5d e0 00     06:34:30.014  READ MULTIPLE EXT

Error 6720 [23] occurred at disk power-on lifetime: 4094 hours (170 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 01 00 00 03 df 64 5e e0 00  Error: UNC 1 sectors at LBA = 0x03df645e = 64971870

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 01 00 00 03 df 64 5e e0 00     06:34:30.014  READ DMA EXT
  29 00 00 00 01 00 00 03 df 64 5d e0 00     06:34:30.014  READ MULTIPLE EXT
  39 00 00 00 01 00 00 03 df 64 5d e0 00     06:34:30.014  WRITE MULTIPLE EXT
  39 00 00 00 01 00 00 03 df 64 5c e0 00     06:34:30.013  WRITE MULTIPLE EXT
  39 00 00 00 01 00 00 03 df 64 5d e0 00     06:34:30.013  WRITE MULTIPLE EXT

Error 6719 [22] occurred at disk power-on lifetime: 4094 hours (170 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 01 00 00 03 df 64 5d e0 00  Error: UNC at LBA = 0x03df645d = 64971869

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  29 00 00 00 01 00 00 03 df 64 5d e0 00     06:34:29.819  READ MULTIPLE EXT
  39 00 00 00 01 00 00 03 df 64 5c e0 00     06:34:29.653  WRITE MULTIPLE EXT
  29 00 00 00 01 00 00 03 df 64 5c e0 00     06:34:29.653  READ MULTIPLE EXT
  25 00 00 00 01 00 00 03 df 64 5d e0 00     06:34:29.632  READ DMA EXT
  29 00 00 00 01 00 00 03 df 64 5c e0 00     06:34:29.632  READ MULTIPLE EXT

SMART Extended Self-test Log Version: 1 (1 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       258 (0x0102)
Device State:                        Active (0)
Current Temperature:                    41 Celsius
Power Cycle Min/Max Temperature:     31/45 Celsius
Lifetime    Min/Max Temperature:     22/54 Celsius
Specified Max Operating Temperature:    30 Celsius
Under/Over Temperature Limit Count:   0/0
Vendor specific:
01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      0/60 Celsius
Min/Max Temperature Limit:           -41/85 Celsius
Temperature History Size (Index):    128 (90)

SCT Error Recovery Control command not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x0002  2            0  R_ERR response for data FIS
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0005  2            0  R_ERR response for non-data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x0008  2            0  Device-to-host non-data FIS retries
0x0009  2        14081  Transition from drive PhyRdy to drive PhyNRdy
0x000a  2           11  Device-to-host register FISes sent due to a COMRESET
0x000b  2            0  CRC errors within host-to-device FIS
0x000f  2            0  R_ERR response for host-to-device data FIS, CRC
0x0012  2            0  R_ERR response for host-to-device non-data FIS, CRC
0x8000  4         9174  Vendor specific

