smartctl 7.4 2023-08-01 r5530 [OpenBSD 7.4 macppc] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Fujitsu MHS AT
Device Model:     FUJITSU MHS2060AT
Serial Number:    --
Firmware Version: 8105
User Capacity:    60,011,642,880 bytes [60.0 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database 7.3/5528
ATA Version is:   ATA/ATAPI-6 T13/1410D revision 3a
Local Time is:    Wed Dec 20 02:57:24 2023 EST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  621) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					No General Purpose Logging support.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  83) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  1 Raw_Read_Error_Rate     0x000f   100   100   046    Pre-fail  Always       -       225439
  2 Throughput_Performance  0x0005   100   100   030    Pre-fail  Offline      -       0
  3 Spin_Up_Time            0x0003   093   093   025    Pre-fail  Always       -       23809
  4 Start_Stop_Count        0x0032   098   098   000    Old_age   Always       -       1252
  5 Reallocated_Sector_Ct   0x0033   100   100   024    Pre-fail  Always       -       0
  7 Seek_Error_Rate         0x000f   100   100   047    Pre-fail  Always       -       4005
  8 Seek_Time_Performance   0x0005   100   100   019    Pre-fail  Offline      -       0
  9 Power_On_Seconds        0x0032   098   098   000    Old_age   Always       -       429h+27m+45s
 10 Spin_Retry_Count        0x0013   100   100   020    Pre-fail  Always       -       0
 12 Power_Cycle_Count       0x0032   095   095   000    Old_age   Always       -       773
192 Emerg_Retract_Cycle_Ct  0x0032   099   099   000    Old_age   Always       -       27
193 Load_Cycle_Count        0x0032   096   096   000    Old_age   Always       -       14325
194 Temperature_Celsius     0x0022   100   100   000    Old_age   Always       -       39 (Min/Max 9/54)
195 Hardware_ECC_Recovered  0x001a   100   100   000    Old_age   Always       -       14788
196 Reallocated_Event_Count 0x0032   100   100   000    Old_age   Always       -       0
197 Current_Pending_Sector  0x0012   100   100   000    Old_age   Always       -       0
198 Offline_Scan_UNC_SectCt 0x0010   100   100   000    Old_age   Offline      -       0
199 UDMA_CRC_Error_Count    0x003e   200   200   000    Old_age   Always       -       0
200 Write_Error_Count       0x000f   100   100   060    Pre-fail  Always       -       17657
203 Run_Out_Cancel          0x0002   100   100   000    Old_age   Always       -       429500858987

SMART Error Log Version: 1
No Errors Logged

SMART Self-test log structure revision number 1
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

The above only provides legacy SMART information - try 'smartctl -x' for more

