smartctl 7.2 2020-12-30 r5155 [FreeBSD 13.0-STABLE amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Western Digital Red
Device Model:     WDC WD40EFRX-68N32N0
Serial Number:    --
LU WWN Device Id: 5 0014ee ...
Firmware Version: 82.00A82
User Capacity:    4,000,787,030,016 bytes [4.00 TB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Rotation Rate:    5400 rpm
Form Factor:      3.5 inches
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ACS-3 T13/2161-D revision 5
SATA Version is:  SATA 3.1, 6.0 Gb/s (current: 3.0 Gb/s)
Local Time is:    Fri Sep  3 13:28:05 2021 ACST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(44640) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 ( 473) minutes.
Conveyance self-test routine
recommended polling time: 	 (   5) minutes.
SCT capabilities: 	       (0x303d)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR-K   200   200   051    -    0
  3 Spin_Up_Time            POS--K   214   177   021    -    4283
  4 Start_Stop_Count        -O--CK   100   100   000    -    31
  5 Reallocated_Sector_Ct   PO--CK   200   200   140    -    0
  7 Seek_Error_Rate         -OSR-K   200   200   000    -    0
  9 Power_On_Hours          -O--CK   065   065   000    -    25922
 10 Spin_Retry_Count        -O--CK   100   253   000    -    0
 11 Calibration_Retry_Count -O--CK   100   253   000    -    0
 12 Power_Cycle_Count       -O--CK   100   100   000    -    30
192 Power-Off_Retract_Count -O--CK   200   200   000    -    16
193 Load_Cycle_Count        -O--CK   200   200   000    -    77
194 Temperature_Celsius     -O---K   122   101   000    -    28
196 Reallocated_Event_Count -O--CK   200   200   000    -    0
197 Current_Pending_Sector  -O--CK   200   200   000    -    0
198 Offline_Uncorrectable   ----CK   100   253   000    -    0
199 UDMA_CRC_Error_Count    -O--CK   200   200   000    -    0
200 Multi_Zone_Error_Rate   ---R--   100   253   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      6  Ext. Comprehensive SMART error log
0x04       GPL,SL  R/O      8  Device Statistics log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x30       GPL,SL  R/O      9  IDENTIFY DEVICE data log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa0-0xa7  GPL,SL  VS      16  Device vendor specific log
0xa8-0xb6  GPL,SL  VS       1  Device vendor specific log
0xb7       GPL,SL  VS      56  Device vendor specific log
0xbd       GPL,SL  VS       1  Device vendor specific log
0xc0       GPL,SL  VS       1  Device vendor specific log
0xc1       GPL     VS      93  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (6 sectors)
Device Error Count: 14
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 14 [13] occurred at disk power-on lifetime: 3 hours (0 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 00 00 00 89 87 7f 40 40 00  Error: IDNF at LBA = 0x89877f40 = 2307358528

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 50 00 f0 00 00 89 87 7f 40 40 08     03:12:51.338  WRITE FPDMA QUEUED
  61 00 80 00 e8 00 00 b6 9e db 68 40 08     03:12:48.857  WRITE FPDMA QUEUED
  61 00 80 00 e0 00 00 b6 9e da e8 40 08     03:12:48.857  WRITE FPDMA QUEUED
  61 00 80 00 d8 00 00 89 87 7e c0 40 08     03:12:48.857  WRITE FPDMA QUEUED
  61 00 80 00 d0 00 00 89 87 7e 40 40 08     03:12:48.856  WRITE FPDMA QUEUED

Error 13 [12] occurred at disk power-on lifetime: 3 hours (0 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 01 00 00 02 00 09 d8 40 00  Error: IDNF at LBA = 0x020009d8 = 33556952

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 08 00 80 00 00 02 00 09 d8 40 08     03:08:33.957  WRITE FPDMA QUEUED
  ea 00 00 00 00 00 00 00 00 00 00 40 08     03:08:33.695  FLUSH CACHE EXT
  61 00 08 00 70 00 00 06 43 af 88 40 08     03:08:33.692  WRITE FPDMA QUEUED
  61 00 08 00 68 00 00 ce 7f de a0 40 08     03:08:33.692  WRITE FPDMA QUEUED
  61 00 10 00 60 00 00 ce 7f de 88 40 08     03:08:33.692  WRITE FPDMA QUEUED

Error 12 [11] occurred at disk power-on lifetime: 3 hours (0 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 00 00 00 25 3d cf f8 40 00  Error: IDNF at LBA = 0x253dcff8 = 624807928

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 80 00 a8 00 00 25 3d cf f8 40 08     03:07:48.651  WRITE FPDMA QUEUED
  61 00 68 00 a0 00 00 25 3d cf 88 40 08     03:07:48.650  WRITE FPDMA QUEUED
  ec 00 00 00 01 00 00 00 00 00 00 40 08     03:07:45.399  IDENTIFY DEVICE
  61 00 68 00 90 00 00 25 3d ce 40 40 08     03:07:40.770  WRITE FPDMA QUEUED
  61 00 80 00 88 00 00 9a 37 52 98 40 08     03:07:38.307  WRITE FPDMA QUEUED

Error 11 [10] occurred at disk power-on lifetime: 3 hours (0 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 00 00 00 e0 d6 ea 50 40 00  Error: IDNF at LBA = 0xe0d6ea50 = 3772181072

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 08 00 20 00 00 e0 d6 ea 50 40 08     03:02:08.702  WRITE FPDMA QUEUED
  61 00 08 00 18 00 00 21 1d 98 c0 40 08     03:02:08.677  WRITE FPDMA QUEUED
  61 00 80 00 10 00 00 be f0 79 b8 40 08     03:02:08.669  WRITE FPDMA QUEUED
  61 00 80 00 08 00 00 e1 c4 67 78 40 08     03:02:08.665  WRITE FPDMA QUEUED
  61 00 20 00 00 00 00 21 fd ab e8 40 08     03:02:08.659  WRITE FPDMA QUEUED

Error 10 [9] occurred at disk power-on lifetime: 3 hours (0 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 00 00 00 5c 1c 4d c8 40 00  Error: IDNF at LBA = 0x5c1c4dc8 = 1545358792

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 80 00 30 00 00 5c 1c 4d c8 40 08     03:01:40.508  WRITE FPDMA QUEUED
  61 00 08 00 28 00 00 79 38 24 d8 40 08     03:01:40.498  WRITE FPDMA QUEUED
  61 00 48 00 20 00 00 aa 62 1c 28 40 08     03:01:40.492  WRITE FPDMA QUEUED
  61 00 48 00 18 00 00 5c 1c 3d 88 40 08     03:01:40.491  WRITE FPDMA QUEUED
  61 00 08 00 10 00 00 20 bb ae 98 40 08     03:01:40.485  WRITE FPDMA QUEUED

Error 9 [8] occurred at disk power-on lifetime: 3 hours (0 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 00 00 00 09 57 79 18 40 00  Error: IDNF at LBA = 0x09577918 = 156727576

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 08 00 08 00 00 09 57 79 18 40 08     03:01:11.067  WRITE FPDMA QUEUED
  61 00 80 00 00 00 00 09 0b 71 78 40 08     03:01:08.164  WRITE FPDMA QUEUED
  61 00 80 00 f8 00 00 09 0b 70 d8 40 08     03:01:08.160  WRITE FPDMA QUEUED
  61 00 80 00 f0 00 00 09 0b 6e b0 40 08     03:01:08.159  WRITE FPDMA QUEUED
  61 00 80 00 e8 00 00 09 0b 6d b0 40 08     03:01:08.159  WRITE FPDMA QUEUED

Error 8 [7] occurred at disk power-on lifetime: 3 hours (0 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 00 00 00 09 08 d6 88 40 00  Error: IDNF at LBA = 0x0908d688 = 151574152

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 80 00 f8 00 00 09 08 d6 88 40 08     03:00:30.639  WRITE FPDMA QUEUED
  61 00 58 00 f0 00 00 08 d4 53 88 40 08     03:00:30.047  WRITE FPDMA QUEUED
  61 00 08 00 e8 00 00 de 42 ee 80 40 08     03:00:30.045  WRITE FPDMA QUEUED
  61 00 08 00 e0 00 00 de 42 ee 48 40 08     03:00:30.043  WRITE FPDMA QUEUED
  61 00 08 00 d8 00 00 c2 7b 0c d0 40 08     03:00:30.039  WRITE FPDMA QUEUED

Error 7 [6] occurred at disk power-on lifetime: 3 hours (0 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 00 00 00 ce 5f 77 90 40 00  Error: IDNF at LBA = 0xce5f7790 = 3462363024

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 20 00 90 00 00 ce 5f 77 90 40 08     02:59:48.503  WRITE FPDMA QUEUED
  61 00 08 00 88 00 00 ce 5f 77 78 40 08     02:59:45.603  WRITE FPDMA QUEUED
  61 00 08 00 80 00 00 ce 5f 77 60 40 08     02:59:45.602  WRITE FPDMA QUEUED
  61 00 70 00 78 00 00 2a 1c e4 38 40 08     02:59:45.600  WRITE FPDMA QUEUED
  61 00 08 00 70 00 00 2a 1c e3 b0 40 08     02:59:45.599  WRITE FPDMA QUEUED

SMART Extended Self-test Log Version: 1 (1 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       258 (0x0102)
Device State:                        Active (0)
Current Temperature:                    28 Celsius
Power Cycle Min/Max Temperature:     21/34 Celsius
Lifetime    Min/Max Temperature:     18/49 Celsius
Under/Over Temperature Limit Count:   0/0
Vendor specific:
01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      0/65 Celsius
Min/Max Temperature Limit:           -41/85 Celsius
Temperature History Size (Index):    478 (265)

SCT Error Recovery Control:
           Read:     70 (7.0 seconds)
          Write:     70 (7.0 seconds)

Device Statistics (GP Log 0x04)
Page  Offset Size        Value Flags Description
0x01  =====  =               =  ===  == General Statistics (rev 1) ==
0x01  0x008  4              30  ---  Lifetime Power-On Resets
0x01  0x010  4           25922  ---  Power-on Hours
0x01  0x018  6    160630113423  ---  Logical Sectors Written
0x01  0x020  6      3561756237  ---  Number of Write Commands
0x01  0x028  6     34342024975  ---  Logical Sectors Read
0x01  0x030  6       978680311  ---  Number of Read Commands
0x01  0x038  6      3124886784  ---  Date and Time TimeStamp
0x03  =====  =               =  ===  == Rotating Media Statistics (rev 1) ==
0x03  0x008  4           25744  ---  Spindle Motor Power-on Hours
0x03  0x010  4           25744  ---  Head Flying Hours
0x03  0x018  4              94  ---  Head Load Events
0x03  0x020  4               0  ---  Number of Reallocated Logical Sectors
0x03  0x028  4              60  ---  Read Recovery Attempts
0x03  0x030  4               0  ---  Number of Mechanical Start Failures
0x03  0x038  4              88  ---  Number of Realloc. Candidate Logical Sectors
0x03  0x040  4              16  ---  Number of High Priority Unload Events
0x04  =====  =               =  ===  == General Errors Statistics (rev 1) ==
0x04  0x008  4              14  ---  Number of Reported Uncorrectable Errors
0x04  0x010  4               3  ---  Resets Between Cmd Acceptance and Completion
0x05  =====  =               =  ===  == Temperature Statistics (rev 1) ==
0x05  0x008  1              28  ---  Current Temperature
0x05  0x010  1              30  ---  Average Short Term Temperature
0x05  0x018  1              25  ---  Average Long Term Temperature
0x05  0x020  1              49  ---  Highest Temperature
0x05  0x028  1              20  ---  Lowest Temperature
0x05  0x030  1              46  ---  Highest Average Short Term Temperature
0x05  0x038  1              21  ---  Lowest Average Short Term Temperature
0x05  0x040  1              38  ---  Highest Average Long Term Temperature
0x05  0x048  1              24  ---  Lowest Average Long Term Temperature
0x05  0x050  4               0  ---  Time in Over-Temperature
0x05  0x058  1              65  ---  Specified Maximum Operating Temperature
0x05  0x060  4               0  ---  Time in Under-Temperature
0x05  0x068  1               0  ---  Specified Minimum Operating Temperature
0x06  =====  =               =  ===  == Transport Statistics (rev 1) ==
0x06  0x008  4             194  ---  Number of Hardware Resets
0x06  0x010  4              42  ---  Number of ASR Events
0x06  0x018  4               0  ---  Number of Interface CRC Errors
                                |||_ C monitored condition met
                                ||__ D supports DSN
                                |___ N normalized value

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x0002  2            0  R_ERR response for data FIS
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0005  2            0  R_ERR response for non-data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x0008  2            0  Device-to-host non-data FIS retries
0x0009  2            3  Transition from drive PhyRdy to drive PhyNRdy
0x000a  2            4  Device-to-host register FISes sent due to a COMRESET
0x000b  2            0  CRC errors within host-to-device FIS
0x000d  2            0  Non-CRC errors within host-to-device FIS
0x000f  2            0  R_ERR response for host-to-device data FIS, CRC
0x0012  2            0  R_ERR response for host-to-device non-data FIS, CRC
0x8000  4      8433104  Vendor specific



