smartctl 7.3 2022-02-28 r5338 [OpenBSD 7.1 amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Apacer AS340 SSDs
Device Model:     Apacer AS340 240GB
Serial Number:    --
LU WWN Device Id: 5 02b2a2 ...
Add. Product Id:  mavlsata
Firmware Version: V4.7
User Capacity:    240,057,409,536 bytes [240 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
TRIM Command:     Available
Device is:        In smartctl database 7.3/5319
ATA Version is:   ACS-3 T13/2161-D revision 4
SATA Version is:  SATA 3.2, 6.0 Gb/s (current: 3.0 Gb/s)
Local Time is:    Wed Jul 20 08:51:45 2022 PST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART Status not supported: Incomplete response, ATA output registers missing
SMART overall-health self-assessment test result: PASSED
Warning: This result is based on an Attribute check.

General SMART Values:
Offline data collection status:  (0x02)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(    0) seconds.
Offline data collection
capabilities: 			 (0x35) SMART execute Offline immediate.
					No Auto Offline data collection support.
					Abort Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					No Selective Self-test supported.
SMART capabilities:            (0x0002)	Does not save SMART data before
					entering power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x00)	Error logging NOT supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (   1) minutes.
Conveyance self-test routine
recommended polling time: 	 (   1) minutes.

SMART Attributes Data Structure revision number: 5
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  5 Reallocated_Sector_Ct   0x0033   100   100   010    Pre-fail  Always       -       0
  9 Power_On_Hours          0x0033   100   100   010    Pre-fail  Always       -       12597
 12 Power_Cycle_Count       0x0033   100   100   010    Pre-fail  Always       -       443
161 Unknown_Attribute       0x0033   100   100   010    Pre-fail  Always       -       0
164 Average_Erase_Count     0x0033   100   100   010    Pre-fail  Always       -       28949
165 Unknown_Attribute       0x0033   100   100   010    Pre-fail  Always       -       103
166 Later_Bad_Block_Count   0x0033   100   100   010    Pre-fail  Always       -       0
167 SSD_Protect_Mode        0x0033   100   100   010    Pre-fail  Always       -       67
169 Unknown_Attribute       0x0033   100   100   010    Pre-fail  Always       -       0
176 Erase_Fail_Count_Chip   0x0033   100   100   010    Pre-fail  Always       -       0
177 Wear_Leveling_Count     0x0033   100   100   010    Pre-fail  Always       -       0
178 Used_Rsvd_Blk_Cnt_Chip  0x0033   100   100   010    Pre-fail  Always       -       0
192 Unexpect_Power_Loss_Ct  0x0033   100   100   010    Pre-fail  Always       -       0
194 Temperature_Celsius     0x0033   100   100   010    Pre-fail  Always       -       47
195 Hardware_ECC_Recovered  0x0033   100   100   010    Pre-fail  Always       -       0
199 UDMA_CRC_Error_Count    0x0033   100   100   010    Pre-fail  Always       -       0
241 Total_LBAs_Written      0x0033   100   100   010    Pre-fail  Always       -       11173
242 Total_LBAs_Read         0x0033   100   100   010    Pre-fail  Always       -       9830
243 Unknown_Attribute       0x0033   100   100   010    Pre-fail  Always       -       0
244 Unknown_Attribute       0x0033   100   100   010    Pre-fail  Always       -       0
245 Unknown_Attribute       0x0033   100   100   010    Pre-fail  Always       -       0
246 Unknown_Attribute       0x0033   100   100   010    Pre-fail  Always       -       0
248 Unknown_Attribute       0x0033   100   100   010    Pre-fail  Always       -       0
250 Read_Error_Retry_Rate   0x0033   100   100   010    Pre-fail  Always       -       0
251 Unknown_Attribute       0x0033   100   100   010    Pre-fail  Always       -       0
252 Unknown_Attribute       0x0033   100   100   010    Pre-fail  Always       -       0
253 Unknown_Attribute       0x0033   100   100   010    Pre-fail  Always       -       0
254 Unknown_SSD_Attribute   0x0033   100   100   010    Pre-fail  Always       -       0

SMART Error Log not supported

SMART Self-test Log not supported

Selective Self-tests/Logging not supported



