smartctl 7.4 2023-08-01 r5530 [FreeBSD 14.0-BETA5 amd64] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     JMicron/Maxiotek based SSDs
Device Model:     KINGSTON SSDNOW 30GB
Serial Number:    --
Firmware Version: AJXA0202
User Capacity:    30,016,659,456 bytes [30.0 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
Form Factor:      2.5 inches
TRIM Command:     Available
Device is:        In smartctl database 7.3/5528
ATA Version is:   ATA8-ACS (minor revision not indicated)
SATA Version is:  SATA 2.6, 3.0 Gb/s
Local Time is:    Tue Mar 19 23:29:36 2024 +10
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Disabled
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (  16)	The self-test routine was aborted by
					the host.
Total time to complete Offline 
data collection: 		(  184) seconds.
Offline data collection
capabilities: 			 (0x1b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					No Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (   4) minutes.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     -O-R--   100   100   000    -    0
  2 Throughput_Performance  P-S---   100   100   050    -    0
  3 Unknown_JMF_Attribute   POS---   100   100   050    -    0
  5 Reallocated_Sector_Ct   PO--C-   100   100   050    -    0
  7 Unknown_JMF_Attribute   PO-R--   100   100   050    -    0
  8 Unknown_JMF_Attribute   P-S---   100   100   050    -    0
  9 Power_On_Hours          -O--C-   100   100   000    -    66518
 10 Unknown_JMF_Attribute   PO--C-   100   100   050    -    0
 12 Power_Cycle_Count       -O--C-   100   100   000    -    619
167 Unknown_JMF_Attribute   -O---K   100   100   000    -    0
168 SATA_Phy_Error_Count    -O--C-   100   100   000    -    0
169 Unknown_JMF_Attribute   PO--C-   100   100   010    -    94522966250
170 Bad_Block_Count         PO--C-   100   100   010    -    10 234 98
173 Erase_Count             -O--C-   100   100   000    -    9 507 166
175 Bad_Cluster_Table_Count PO--C-   100   100   010    -    0
192 Unexpect_Power_Loss_Ct  -O--C-   100   100   000    -    579
194 Temperature_Celsius     PO---K   069   060   030    -    31 (Min/Max 16/40)
240 Unknown_JMF_Attribute   PO--C-   100   100   050    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O     51  Comprehensive SMART error log
0x03       GPL     R/O     64  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log

SMART Extended Comprehensive Error Log Version: 1 (64 sectors)
Device Error Count: 305 (device log contains only the most recent 256 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 305 [48] occurred at disk power-on lifetime: 64083 hours (2670 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 10 00 00 00 00 04 28 40 00  Error: ICRC, ABRT 16 sectors at LBA = 0x00000428 = 1064

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 02 00 00 10 00 00 00 00 04 28 40 00     00:05:05.116  READ DMA
  ef 00 02 00 00 00 00 00 00 00 00 40 00     00:05:05.116  SET FEATURES [Enable write cache]
  ef 00 aa 00 00 00 00 00 00 00 00 40 00     00:05:05.116  SET FEATURES [Enable read look-ahead]
  c6 00 00 00 10 00 00 00 00 00 00 40 00     00:05:05.116  SET MULTIPLE MODE
  ef 00 03 00 45 00 00 00 00 00 00 40 00     00:05:05.116  SET FEATURES [Set transfer mode]

Error 304 [47] occurred at disk power-on lifetime: 64083 hours (2670 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 10 00 00 00 00 04 28 40 00  Error: ICRC, ABRT 16 sectors at LBA = 0x00000428 = 1064

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 02 00 00 10 00 00 00 00 04 28 40 00     00:05:05.008  READ DMA
  ef 00 02 00 00 00 00 00 00 00 00 40 00     00:05:05.008  SET FEATURES [Enable write cache]
  ef 00 aa 00 00 00 00 00 00 00 00 40 00     00:05:05.008  SET FEATURES [Enable read look-ahead]
  c8 00 00 00 10 00 00 00 00 00 28 40 00     00:05:05.007  READ DMA
  c8 00 00 00 10 00 00 00 00 02 28 40 00     00:05:05.007  READ DMA

Error 303 [46] occurred at disk power-on lifetime: 64083 hours (2670 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 10 00 00 00 00 02 28 40 00  Error: ICRC, ABRT 16 sectors at LBA = 0x00000228 = 552

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 02 00 00 10 00 00 00 00 02 28 40 00     00:05:04.898  READ DMA
  ef 00 02 00 00 00 00 00 00 00 00 40 00     00:05:04.898  SET FEATURES [Enable write cache]
  ef 00 aa 00 00 00 00 00 00 00 00 40 00     00:05:04.898  SET FEATURES [Enable read look-ahead]
  c8 00 00 00 10 00 00 00 00 00 38 40 00     00:05:04.898  READ DMA
  c8 00 00 00 10 00 00 00 00 02 38 40 00     00:05:04.897  READ DMA

Error 302 [45] occurred at disk power-on lifetime: 64083 hours (2670 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 10 10 00 00 00 00 02 38 40 00  Error: ICRC, ABRT 4112 sectors at LBA = 0x00000238 = 568

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 10 10 00 00 00 00 02 38 40 00     00:05:04.790  READ DMA
  c6 00 00 00 10 00 00 00 00 00 00 40 00     00:05:04.790  SET MULTIPLE MODE
  ef 00 03 00 45 00 00 00 00 00 00 40 00     00:05:04.790  SET FEATURES [Set transfer mode]
  ec 00 00 00 00 00 00 00 00 00 00 40 00     00:05:04.790  IDENTIFY DEVICE
  ff ff ff ff ff ff ff ff ff ff ff ff ff     00:05:04.687  [VENDOR SPECIFIC]

Error 301 [44] occurred at disk power-on lifetime: 64083 hours (2670 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 10 10 00 00 00 00 02 38 40 00  Error: ICRC, ABRT 4112 sectors at LBA = 0x00000238 = 568

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 10 10 00 00 00 00 02 38 40 00     00:05:04.686  READ DMA
  c6 00 00 00 10 00 00 00 00 00 00 40 00     00:05:04.686  SET MULTIPLE MODE
  ef 00 03 00 45 00 00 00 00 00 00 40 00     00:05:04.686  SET FEATURES [Set transfer mode]
  ec 00 00 00 00 00 00 00 00 00 00 40 00     00:05:04.686  IDENTIFY DEVICE
  ff ff ff ff ff ff ff ff ff ff ff ff ff     00:05:04.578  [VENDOR SPECIFIC]

Error 300 [43] occurred at disk power-on lifetime: 64083 hours (2670 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 10 00 00 00 00 02 38 40 00  Error: ICRC, ABRT 16 sectors at LBA = 0x00000238 = 568

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 02 00 00 10 00 00 00 00 02 38 40 00     00:05:04.577  READ DMA
  c8 00 00 00 10 00 00 00 00 02 38 40 00     00:05:04.577  READ DMA
  ef 00 02 00 00 00 00 00 00 00 00 40 00     00:05:04.577  SET FEATURES [Enable write cache]
  ef 00 aa 00 00 00 00 00 00 00 00 40 00     00:05:04.577  SET FEATURES [Enable read look-ahead]
  c8 00 00 00 10 00 00 00 00 00 a8 40 00     00:05:04.577  READ DMA

Error 299 [42] occurred at disk power-on lifetime: 64083 hours (2670 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 10 10 00 00 00 00 02 a8 40 00  Error: ICRC, ABRT 4112 sectors at LBA = 0x000002a8 = 680

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 10 10 00 00 00 00 02 a8 40 00     00:05:04.474  READ DMA
  c6 00 00 00 10 00 00 00 00 00 00 40 00     00:05:04.474  SET MULTIPLE MODE
  ef 00 03 00 45 00 00 00 00 00 00 40 00     00:05:04.474  SET FEATURES [Set transfer mode]
  ec 00 00 00 00 00 00 00 00 00 00 40 00     00:05:04.474  IDENTIFY DEVICE
  ff ff ff ff ff ff ff ff ff ff ff ff ff     00:05:04.366  [VENDOR SPECIFIC]

Error 298 [41] occurred at disk power-on lifetime: 64083 hours (2670 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 10 00 00 00 00 02 a8 40 00  Error: ICRC, ABRT 16 sectors at LBA = 0x000002a8 = 680

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 02 00 00 10 00 00 00 00 02 a8 40 00     00:05:04.365  READ DMA
  ef 00 02 00 00 00 00 00 00 00 00 40 00     00:05:04.365  SET FEATURES [Enable write cache]
  ef 00 aa 00 00 00 00 00 00 00 00 40 00     00:05:04.365  SET FEATURES [Enable read look-ahead]
  c6 00 00 00 10 00 00 00 00 00 00 40 00     00:05:04.365  SET MULTIPLE MODE
  ef 00 03 00 45 00 00 00 00 00 00 40 00     00:05:04.365  SET FEATURES [Set transfer mode]

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Aborted by host               00%       868         -

Selective Self-tests/Logging not supported

SCT Commands not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x0008  2            0  Device-to-host non-data FIS retries
0x0009  4           13  Transition from drive PhyRdy to drive PhyNRdy
0x000a  4           13  Device-to-host register FISes sent due to a COMRESET
0x000f  2            0  R_ERR response for host-to-device data FIS, CRC
0x0010  2            0  R_ERR response for host-to-device data FIS, non-CRC
0x0012  2            0  R_ERR response for host-to-device non-data FIS, CRC
0x0013  2            0  R_ERR response for host-to-device non-data FIS, non-CRC



