smartctl 7.4 2023-08-01 r5530 [FreeBSD 14.0-RELEASE-p5 amd64] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     SAMSUNG SpinPoint M6
Device Model:     SAMSUNG HM500LI
Serial Number:    --
LU WWN Device Id: 5 0f0000 ...
Firmware Version: 2TF00_00
User Capacity:    500,107,862,016 bytes [500 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database 7.2/5319
ATA Version is:   ATA8-ACS, ATA/ATAPI-7 T13/1532D revision 0
SATA Version is:  SATA 2.5, 3.0 Gb/s
Local Time is:    Fri Mar 22 10:21:27 2024 CET
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM level is:     0 (vendor specific), recommended: 254
APM level is:     1 (minimum power consumption with standby)
Rd look-ahead is: Enabled
Write cache is:   Disabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  165) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 ( 165) minutes.
SCT capabilities: 	       (0x003f)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   100   100   051    -    0
  3 Spin_Up_Time            POS---   252   252   025    -    3500
  4 Start_Stop_Count        -O--CK   072   072   000    -    28369
  5 Reallocated_Sector_Ct   PO--CK   080   080   010    -    189
  7 Seek_Error_Rate         -OSR--   252   252   051    -    0
  8 Seek_Time_Performance   --S--K   252   252   015    -    0
  9 Power_On_Hours          -O--CK   067   067   000    -    17377
 10 Spin_Retry_Count        -O--CK   100   100   051    -    4
 12 Power_Cycle_Count       -O--CK   100   100   000    -    384
191 G-Sense_Error_Rate      -O--CK   100   100   000    -    166
192 Power-Off_Retract_Count -O--CK   252   252   000    -    0
194 Temperature_Celsius     -O---K   163   070   000    -    25 (Min/Max 13/56)
195 Hardware_ECC_Recovered  -O-RC-   100   100   000    -    0
196 Reallocated_Event_Count -O--CK   252   252   000    -    0
197 Current_Pending_Sector  -O--C-   252   252   000    -    0
198 Offline_Uncorrectable   ----CK   252   252   000    -    0
199 UDMA_CRC_Error_Count    -OS-CK   200   200   000    -    0
200 Multi_Zone_Error_Rate   -O-R--   100   100   000    -    0
201 Soft_Read_Error_Rate    -O--CK   252   252   000    -    0
223 Load_Retry_Count        -O--CK   100   100   000    -    3
225 Load_Cycle_Count        -O--CK   065   065   000    -    360792
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      2  Comprehensive SMART error log
0x03       GPL     R/O      2  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x08           SL  R/O      1  Power Conditions log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x80       GPL,SL  R/W     16  Host vendor specific log
0x81-0x9f      SL  R/W     16  Host vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (2 sectors)
Device Error Count: 4
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 4 [3] occurred at disk power-on lifetime: 16561 hours (690 days + 1 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 02 00 00 00 08 38 17 d8 40 00  Error: ABRT at LBA = 0x083817d8 = 137893848

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 08 00 02 00 00 00 08 38 17 d8 40 00     01:07:46.000  READ FPDMA QUEUED
  60 08 00 01 10 00 00 08 38 0f d8 40 00     01:07:46.000  READ FPDMA QUEUED
  60 08 00 02 08 00 00 08 38 07 d8 40 00     01:07:45.937  READ FPDMA QUEUED
  60 08 00 00 10 00 00 08 37 ff d8 40 00     01:07:45.937  READ FPDMA QUEUED
  60 08 00 01 00 00 00 08 37 f7 d8 40 00     01:07:45.937  READ FPDMA QUEUED

Error 3 [2] occurred at disk power-on lifetime: 6955 hours (289 days + 19 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 00 08 00 00 2c 75 0b b2 40 00  Error: ABRT at LBA = 0x2c750bb2 = 745868210

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 80 00 08 00 00 2c 75 0b b2 40 00     08:26:45.187  WRITE FPDMA QUEUED
  60 00 03 00 00 00 00 2c 2e 86 22 40 00     08:26:45.187  READ FPDMA QUEUED
  61 00 04 00 00 00 00 2c 58 3a 5d 40 00     08:26:45.187  WRITE FPDMA QUEUED
  61 00 04 00 00 00 00 22 20 49 18 40 00     08:26:45.187  WRITE FPDMA QUEUED
  61 00 0e 00 00 00 00 2c 75 0c da 40 00     08:26:45.187  WRITE FPDMA QUEUED

Error 2 [1] occurred at disk power-on lifetime: 6955 hours (289 days + 19 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 01 08 00 00 2c 57 e2 c7 40 00  Error: ABRT at LBA = 0x2c57e2c7 = 743957191

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 02 01 08 00 00 2c 57 e2 c7 40 00     08:26:06.437  WRITE FPDMA QUEUED
  61 00 02 01 08 00 00 2c 57 e2 c4 40 00     08:26:06.375  WRITE FPDMA QUEUED
  61 00 02 01 08 00 00 22 1f b4 ee 40 00     08:26:06.375  WRITE FPDMA QUEUED
  61 00 02 01 08 00 00 22 1f 49 ab 40 00     08:26:06.375  WRITE FPDMA QUEUED
  61 00 05 01 08 00 00 19 ff 1d be 40 00     08:26:06.375  WRITE FPDMA QUEUED

Error 1 [0] occurred at disk power-on lifetime: 6955 hours (289 days + 19 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 03 20 00 00 2c 0d af 51 40 00  Error: ABRT at LBA = 0x2c0daf51 = 739094353

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 02 03 20 00 00 2c 0d af 51 40 00     08:25:00.875  READ FPDMA QUEUED
  61 00 51 02 18 00 00 2c 72 65 43 40 00     08:25:00.875  WRITE FPDMA QUEUED
  61 01 00 01 10 00 00 2c 72 64 43 40 00     08:25:00.875  WRITE FPDMA QUEUED
  61 00 39 00 08 00 00 2c 56 fc 04 40 00     08:25:00.812  WRITE FPDMA QUEUED
  60 00 02 00 00 00 00 15 08 36 15 40 00     08:25:00.812  READ FPDMA QUEUED

SMART Extended Self-test Log (GP Log 0x07) not supported

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%     17365         -
# 2  Short offline       Completed without error       00%     17335         -
# 3  Short offline       Completed without error       00%     17313         -
# 4  Short offline       Completed without error       00%     17277         -
# 5  Short offline       Completed without error       00%     17197         -
# 6  Short offline       Completed without error       00%     17175         -
# 7  Short offline       Completed without error       00%     17147         -
# 8  Short offline       Completed without error       00%     17076         -
# 9  Short offline       Completed without error       00%     17062         -
#10  Short offline       Completed without error       00%     17046         -
#11  Short offline       Completed without error       00%     17031         -
#12  Short offline       Completed without error       00%     16923         -
#13  Short offline       Completed without error       00%     16760         -
#14  Short offline       Completed without error       00%     16740         -
#15  Short offline       Completed without error       00%     16722         -
#16  Short offline       Completed without error       00%     16297         -
#17  Extended offline    Completed without error       00%     16235         -
#18  Short offline       Completed without error       00%     15609         -
#19  Short offline       Completed without error       00%     15592         -
#20  Short offline       Completed without error       00%     15551         -
#21  Short offline       Completed without error       00%     15538         -

SMART Selective self-test log data structure revision number 0
Note: revision number not 1 implies that no selective self-test has ever been run
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Completed [00% left] (0-65535)
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  2
SCT Version (vendor specific):       256 (0x0100)
Device State:                        Active (0)
Current Temperature:                    24 Celsius
Power Cycle Min/Max Temperature:     21/25 Celsius
Lifetime    Min/Max Temperature:     14/56 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:     15/55 Celsius
Min/Max Temperature Limit:           10/60 Celsius
Temperature History Size (Index):    128 (113)

SCT Error Recovery Control:
           Read:      1 (0.1 seconds)
          Write:      1 (0.1 seconds)

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x000a  2            1  Device-to-host register FISes sent due to a COMRESET
0x0008  2            0  Device-to-host non-data FIS retries
0x0009  2            1  Transition from drive PhyRdy to drive PhyNRdy
0x000b  2            0  CRC errors within host-to-device FIS
0x000d  2            0  Non-CRC errors within host-to-device FIS
0x8001  2            0  Vendor specific

