smartctl 7.3 2022-02-28 r5338 [FreeBSD 13.2-RELEASE amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Momentus 5400.6
Device Model:     ST9320325AS
Serial Number:    --
LU WWN Device Id: 5 000c50 ...
Firmware Version: 0003SDM1
User Capacity:    320,072,933,376 bytes [320 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    5400 rpm
Device is:        In smartctl database 7.3/5319
ATA Version is:   ATA8-ACS T13/1699-D revision 4
SATA Version is:  SATA 2.6, 3.0 Gb/s
Local Time is:    Wed Jun  7 14:18:06 2023    
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     128 (minimum power consumption without standby)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unknown

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(    0) seconds.
Offline data collection
capabilities: 			 (0x73) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (  95) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x103b)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   117   086   006    -    128094528
  3 Spin_Up_Time            PO----   099   098   000    -    0
  4 Start_Stop_Count        -O--CK   091   091   020    -    9808
  5 Reallocated_Sector_Ct   PO--CK   096   096   036    -    92
  7 Seek_Error_Rate         POSR--   085   060   030    -    4669498421
  9 Power_On_Hours          -O--CK   071   071   000    -    25836
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   091   091   020    -    9563
184 End-to-End_Error        -O--CK   100   100   099    -    0
187 Reported_Uncorrect      -O--CK   001   001   000    -    2215
188 Command_Timeout         -O--CK   100   097   000    -    179
189 High_Fly_Writes         -O-RCK   100   100   000    -    0
190 Airflow_Temperature_Cel -O---K   061   047   045    -    39 (Min/Max 38/41)
191 G-Sense_Error_Rate      -O--CK   100   100   000    -    852
192 Power-Off_Retract_Count -O--CK   100   100   000    -    1595
193 Load_Cycle_Count        -O--CK   001   001   000    -    229868
194 Temperature_Celsius     -O---K   039   053   000    -    39 (0 8 0 0 0)
195 Hardware_ECC_Recovered  -O-RC-   066   052   000    -    128094528
197 Current_Pending_Sector  -O--C-   100   100   000    -    0
198 Offline_Uncorrectable   ----C-   100   100   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    0
254 Free_Fall_Sensor        -O--CK   100   100   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01       GPL,SL  R/O      1  Summary SMART error log
0x02       GPL,SL  R/O      5  Comprehensive SMART error log
0x03       GPL,SL  R/O      5  Ext. Comprehensive SMART error log
0x06       GPL,SL  R/O      1  SMART self-test log
0x07       GPL,SL  R/O      1  Extended self-test log
0x09       GPL,SL  R/W      1  Selective self-test log
0x10       GPL,SL  R/O      1  NCQ Command Error log
0x11       GPL,SL  R/O      1  SATA Phy Event Counters log
0x21       GPL,SL  R/O      1  Write stream error log
0x22       GPL,SL  R/O      1  Read stream error log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS      20  Device vendor specific log
0xa2       GPL     VS    2248  Device vendor specific log
0xa8       GPL,SL  VS      65  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xb0       GPL     VS    2864  Device vendor specific log
0xbe-0xbf  GPL     VS   65535  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 2412 (device log contains only the most recent 20 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 2412 [11] occurred at disk power-on lifetime: 23455 hours (977 days + 7 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 b5 00 52 11 be 00 00  Error: UNC at LBA = 0xb5005211be = 777394459070

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 b5 00 52 11 b8 40 00     00:06:19.742  READ FPDMA QUEUED
  61 00 00 00 08 00 91 00 4f 12 f8 40 00     00:06:19.742  WRITE FPDMA QUEUED
  ea 00 00 00 00 00 00 00 00 00 00 a0 00     00:06:19.742  FLUSH CACHE EXT
  27 00 00 00 00 00 00 00 00 00 00 e0 00     00:06:19.741  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 00 00 00 00 00 00 00 00 00 00 a0 00     00:06:19.740  IDENTIFY DEVICE

Error 2411 [10] occurred at disk power-on lifetime: 23455 hours (977 days + 7 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 b5 00 52 11 be 00 00  Error: UNC at LBA = 0xb5005211be = 777394459070

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 b5 00 52 11 b8 40 00     00:06:17.319  READ FPDMA QUEUED
  61 00 00 00 c8 00 91 00 4f 12 30 40 00     00:06:17.319  WRITE FPDMA QUEUED
  27 00 00 00 00 00 00 00 00 00 00 e0 00     00:06:17.318  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 00 00 00 00 00 00 00 00 00 00 a0 00     00:06:17.316  IDENTIFY DEVICE
  ef 00 03 00 46 00 00 00 00 00 00 a0 00     00:06:17.284  SET FEATURES [Set transfer mode]

Error 2410 [9] occurred at disk power-on lifetime: 23455 hours (977 days + 7 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 b5 00 52 11 be 00 00  Error: UNC at LBA = 0xb5005211be = 777394459070

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 b5 00 52 11 b8 40 00     00:06:14.737  READ FPDMA QUEUED
  60 00 00 00 08 00 b5 00 52 11 b0 40 00     00:06:14.737  READ FPDMA QUEUED
  60 00 00 00 08 00 b5 00 52 11 a8 40 00     00:06:14.737  READ FPDMA QUEUED
  60 00 00 00 08 00 b5 00 52 11 a0 40 00     00:06:14.736  READ FPDMA QUEUED
  60 00 00 00 08 00 b5 00 52 11 98 40 00     00:06:14.736  READ FPDMA QUEUED

Error 2409 [8] occurred at disk power-on lifetime: 23455 hours (977 days + 7 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 b5 00 52 11 be 00 00  Error: UNC at LBA = 0xb5005211be = 777394459070

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 01 00 00 b5 00 53 11 68 40 00     00:06:12.132  READ FPDMA QUEUED
  60 00 00 01 00 00 b5 00 52 11 68 40 00     00:06:12.130  READ FPDMA QUEUED
  60 00 00 01 00 00 b5 00 51 11 68 40 00     00:06:12.129  READ FPDMA QUEUED
  60 00 00 01 00 00 b5 00 50 11 68 40 00     00:06:12.128  READ FPDMA QUEUED
  60 00 00 01 00 00 b5 00 4f 11 68 40 00     00:06:12.128  READ FPDMA QUEUED

Error 2408 [7] occurred at disk power-on lifetime: 23454 hours (977 days + 6 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 ba 00 fd 11 a8 00 00  Error: UNC at LBA = 0xba00fd11a8 = 798880502184

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 ba 00 fd 11 a8 40 00     01:11:53.509  READ FPDMA QUEUED
  61 00 00 00 08 00 90 00 72 12 18 40 00     01:11:53.509  WRITE FPDMA QUEUED
  ea 00 00 00 00 00 00 00 00 00 00 a0 00     01:11:53.509  FLUSH CACHE EXT
  27 00 00 00 00 00 00 00 00 00 00 e0 00     01:11:53.508  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 00 00 00 00 00 00 00 00 00 00 a0 00     01:11:53.506  IDENTIFY DEVICE

Error 2407 [6] occurred at disk power-on lifetime: 23454 hours (977 days + 6 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 ba 00 fd 11 a8 00 00  Error: UNC at LBA = 0xba00fd11a8 = 798880502184

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 ba 00 fd 11 a8 40 00     01:11:51.088  READ FPDMA QUEUED
  61 00 00 00 f8 00 90 00 71 12 20 40 00     01:11:51.088  WRITE FPDMA QUEUED
  27 00 00 00 00 00 00 00 00 00 00 e0 00     01:11:51.087  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 00 00 00 00 00 00 00 00 00 00 a0 00     01:11:51.086  IDENTIFY DEVICE
  ef 00 03 00 46 00 00 00 00 00 00 a0 00     01:11:51.085  SET FEATURES [Set transfer mode]

Error 2406 [5] occurred at disk power-on lifetime: 23454 hours (977 days + 6 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 ba 00 fd 11 a8 00 00  Error: UNC at LBA = 0xba00fd11a8 = 798880502184

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 ba 00 fd 11 a8 40 00     01:11:48.599  READ FPDMA QUEUED
  60 00 00 00 08 00 01 00 1b 01 b8 40 00     01:11:46.940  READ FPDMA QUEUED
  61 00 00 00 20 00 10 00 17 22 08 40 00     01:11:46.924  WRITE FPDMA QUEUED
  60 00 00 00 40 00 6b 00 02 00 10 40 00     01:11:46.922  READ FPDMA QUEUED
  60 00 00 00 18 00 6b 00 01 00 f0 40 00     01:11:46.922  READ FPDMA QUEUED

Error 2405 [4] occurred at disk power-on lifetime: 23454 hours (977 days + 6 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 ba 00 fd 11 a8 00 00  Error: UNC at LBA = 0xba00fd11a8 = 798880502184

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 ba 00 fd 11 a8 40 00     01:10:36.059  READ FPDMA QUEUED
  60 00 00 01 00 00 c1 00 15 03 e0 40 00     01:10:36.053  READ FPDMA QUEUED
  ea 00 00 00 00 00 00 00 00 00 00 a0 00     01:10:36.030  FLUSH CACHE EXT
  60 00 00 00 58 00 c1 00 15 03 88 40 00     01:10:36.009  READ FPDMA QUEUED
  61 00 00 00 08 00 90 00 67 12 c0 40 00     01:10:36.009  WRITE FPDMA QUEUED

SMART Extended Self-test Log Version: 1 (1 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       522 (0x020a)
Device State:                        Active (0)
Current Temperature:                    39 Celsius
Power Cycle Min/Max Temperature:     38/41 Celsius
Lifetime    Min/Max Temperature:      8/54 Celsius
Under/Over Temperature Limit Count:   0/94

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      0/ 0 Celsius
Min/Max Temperature Limit:            0/ 0 Celsius
Temperature History Size (Index):    128 (119)

SCT Error Recovery Control:
           Read: Disabled
          Write: Disabled

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2           16  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS

