HPE Hard Drives
===============

This is a list of all tested HPE hard drive models and their MTBFs. See more
info on reliability test in the [README](https://github.com/bsdhw/SMART).

Contents
--------

1. [ HDD by Model  ](#hdd-by-model)
2. [ HDD by Family ](#hdd-by-family)

HDD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| HPE       | MB4000GCWLV        | 4 TB   | 9       | 1662  | 0     | 4.55   |
| HPE       | MB4000GVYZK        | 4 TB   | 8       | 1005  | 0     | 2.76   |
| HPE       | MB0500GCEHE        | 500 GB | 6       | 659   | 2     | 1.70   |
| HPE       | MM2000GEFRA        | 2 TB   | 6       | 239   | 0     | 0.66   |

HDD by Family
-------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Family                 | Models | Samples | Days  | Err   | MTBF |
|-----------|------------------------|--------|---------|-------|-------|------|
| HPE       | Proliant HardDrive     | 3      | 23      | 1062  | 0     | 2.91   |
| HPE       | WDC Enterprise         | 1      | 6       | 659   | 2     | 1.70   |
