smartctl 7.3 2022-02-28 r5338 [FreeBSD 13.1-RELEASE amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     SAMSUNG SpinPoint MP5
Device Model:     SAMSUNG HM500JJ
Serial Number:    --
LU WWN Device Id: 5 0024e9 ...
Firmware Version: 2AK10002
User Capacity:    500,107,862,016 bytes [500 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    7200 rpm
Form Factor:      2.5 inches
Device is:        In smartctl database 7.3/5319
ATA Version is:   ATA8-ACS T13/1699-D revision 6
SATA Version is:  SATA 2.6, 3.0 Gb/s
Local Time is:    Sun May 14 13:04:32 2023 UTC
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Disabled
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Write SCT (Get) Feature Control Command failed: Read of ATA output registers not implemented [JMicron]
Wt Cache Reorder: Unknown (SCT Feature Control command failed)

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: FAILED!
Drive failure expected in less than 24 hours. SAVE ALL DATA.
See vendor-specific Attribute list for failed Attributes.

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		( 6240) seconds.
Offline data collection
capabilities: 			 (0x51) SMART execute Offline immediate.
					No Auto Offline data collection support.
					Suspend Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 ( 104) minutes.
SCT capabilities: 	       (0x003d)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR-K   001   001   051    NOW  109933
  2 Throughput_Performance  POS--K   252   252   000    -    0
  3 Spin_Up_Time            PO---K   090   088   025    -    3219
  4 Start_Stop_Count        -O--CK   097   097   000    -    3864
  5 Reallocated_Sector_Ct   PO--CK   252   252   010    -    0
  7 Seek_Error_Rate         POSR-K   252   252   051    -    0
  8 Seek_Time_Performance   P-S--K   252   252   015    -    0
  9 Power_On_Hours          -O--CK   100   100   000    -    3337
 10 Spin_Retry_Count        PO--CK   252   252   051    -    0
 11 Calibration_Retry_Count -O--CK   100   100   000    -    306
 12 Power_Cycle_Count       -O--CK   097   097   000    -    3706
183 Runtime_Bad_Block       -O--CK   100   100   010    -    2
184 End-to-End_Error        PO--CK   252   252   048    -    0
186 Unknown_Attribute       -O--CK   252   252   000    -    0
187 Reported_Uncorrect      -O--CK   100   100   000    -    44529
188 Command_Timeout         -O--CK   100   100   000    -    62
190 Airflow_Temperature_Cel -O----   069   048   040    -    31 (Min/Max 16/54)
191 G-Sense_Error_Rate      -O---K   099   099   000    -    19523
192 Power-Off_Retract_Count -O---K   252   252   000    -    0
193 Load_Cycle_Count        -O--CK   097   097   000    -    31280
194 Temperature_Celsius     -O----   064   048   000    -    31 (Min/Max 16/54)
195 Hardware_ECC_Recovered  -O-RCK   100   100   000    -    0
196 Reallocated_Event_Count -O--CK   252   252   000    -    0
197 Current_Pending_Sector  -O--CK   094   078   000    -    551
198 Offline_Uncorrectable   ----CK   252   252   000    -    0
199 UDMA_CRC_Error_Count    -OS-CK   100   100   000    -    1
200 Multi_Zone_Error_Rate   -O-R-K   100   100   000    -    5247
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

ATA_READ_LOG_EXT (addr=0x00:0x00, page=0, n=1) failed: 48-bit ATA commands not implemented [JMicron]
Read GP Log Directory failed

SMART Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00           SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      2  Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x09           SL  R/W      1  Selective self-test log
0x80-0x9f      SL  R/W     16  Host vendor specific log
0xe0           SL  R/W      1  SCT Command/Status
0xe1           SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log (GP Log 0x03) not supported

SMART Error Log Version: 1
ATA Error Count: 751 (device log contains only the most recent five errors)
	CR = Command Register [HEX]
	FR = Features Register [HEX]
	SC = Sector Count Register [HEX]
	SN = Sector Number Register [HEX]
	CL = Cylinder Low Register [HEX]
	CH = Cylinder High Register [HEX]
	DH = Device/Head Register [HEX]
	DC = Device Command Register [HEX]
	ER = Error register [HEX]
	ST = Status register [HEX]
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 751 occurred at disk power-on lifetime: 3326 hours (138 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 08 00 08 b5 e3  Error: UNC 8 sectors at LBA = 0x03b50800 = 62195712

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 08 00 08 b5 e3 08      00:00:02.325  READ DMA
  35 00 00 00 08 71 e0 08      00:00:02.325  WRITE DMA EXT
  ec 00 00 00 00 00 a0 08      00:00:02.325  IDENTIFY DEVICE
  ef 03 46 00 00 00 a0 08      00:00:02.325  SET FEATURES [Set transfer mode]
  ec 00 00 00 00 00 a0 08      00:00:02.324  IDENTIFY DEVICE

Error 750 occurred at disk power-on lifetime: 3326 hours (138 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 08 00 08 b5 e3  Error: UNC 8 sectors at LBA = 0x03b50800 = 62195712

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 08 00 08 b5 e3 08      00:00:02.322  READ DMA
  c8 00 08 00 08 35 e3 08      00:00:02.322  READ DMA
  c8 00 08 00 08 dd e2 08      00:00:02.322  READ DMA
  c8 00 08 00 08 d5 e2 08      00:00:02.322  READ DMA
  c8 00 08 00 08 95 e2 08      00:00:02.322  READ DMA

Error 749 occurred at disk power-on lifetime: 3326 hours (138 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 05 03 08 75 e3  Error: UNC 5 sectors at LBA = 0x03750803 = 58001411

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 08 00 08 75 e3 08      00:00:02.318  READ DMA
  c8 00 08 f8 07 e2 e4 08      00:00:02.318  READ DMA
  c8 00 08 f0 07 e2 e4 08      00:00:02.318  READ DMA
  ec 00 00 00 00 00 a0 08      00:00:02.318  IDENTIFY DEVICE
  ef 03 46 00 00 00 a0 08      00:00:02.318  SET FEATURES [Set transfer mode]

Error 748 occurred at disk power-on lifetime: 3326 hours (138 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 05 03 08 75 e3  Error: UNC 5 sectors at LBA = 0x03750803 = 58001411

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 08 00 08 75 e3 08      00:00:02.316  READ DMA
  c8 00 08 80 07 e2 e4 08      00:00:02.316  READ DMA
  ec 00 00 00 00 00 a0 08      00:00:02.316  IDENTIFY DEVICE
  ef 03 46 00 00 00 a0 08      00:00:02.316  SET FEATURES [Set transfer mode]
  ec 00 00 00 00 00 a0 08      00:00:02.316  IDENTIFY DEVICE

Error 747 occurred at disk power-on lifetime: 3326 hours (138 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 05 03 08 75 e3  Error: UNC 5 sectors at LBA = 0x03750803 = 58001411

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 08 00 08 75 e3 08      00:00:02.314  READ DMA
  c8 00 08 08 29 71 e2 08      00:00:02.314  READ DMA
  c8 00 40 20 08 71 e2 08      00:00:02.314  READ DMA
  c8 00 20 00 08 71 e2 08      00:00:02.314  READ DMA
  ea 00 00 ff 5f 38 e0 08      00:00:02.314  FLUSH CACHE EXT

SMART Extended Self-test Log (GP Log 0x07) not supported

SMART Self-test log structure revision number 1
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 0
Note: revision number not 1 implies that no selective self-test has ever been run
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Completed [00% left] (0-65535)
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  2
SCT Version (vendor specific):       256 (0x0100)
Device State:                        Active (0)
Current Temperature:                    30 Celsius
Power Cycle Min/Max Temperature:     30/30 Celsius
Lifetime    Min/Max Temperature:     20/65 Celsius
Specified Max Operating Temperature:    80 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Temperature History Version:     2
Temperature Sampling Period:         5 minutes
Temperature Logging Interval:        5 minutes
Min/Max recommended Temperature:     -5/80 Celsius
Min/Max Temperature Limit:           -10/85 Celsius
Temperature History Size (Index):    128 (56)

Write SCT (Get) Error Recovery Control Command failed: Read of ATA output registers not implemented [JMicron]
SCT (Get) Error Recovery Control command failed

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

ATA_READ_LOG_EXT (addr=0x11:0x00, page=0, n=1) failed: 48-bit ATA commands not implemented [JMicron]
Read SATA Phy Event Counters failed

