smartctl 7.3 2022-02-28 r5338 [FreeBSD 13.1-RELEASE amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Number:                       BIWIN SSD
Serial Number:                      --
Firmware Version:                   52AAT8KA
PCI Vendor/Subsystem ID:            0x1dee
IEEE OUI Identifier:                0x000000
Controller ID:                      1
NVMe Version:                       1.3
Number of Namespaces:               1
Namespace 1 Size/Capacity:          1,024,209,543,168 [1.02 TB]
Namespace 1 Utilization:            167,568,240,640 [167 GB]
Namespace 1 Formatted LBA Size:     512
Local Time is:                      Fri Mar 24 02:57:49 2023 UTC
Firmware Updates (0x14):            2 Slots, no Reset required
Optional Admin Commands (0x0017):   Security Format Frmw_DL Self_Test
Optional NVM Commands (0x005f):     Comp Wr_Unc DS_Mngmt Wr_Zero Sav/Sel_Feat Timestmp
Log Page Attributes (0x0b):         S/H_per_NS Cmd_Eff_Lg Telmtry_Lg
Maximum Data Transfer Size:         32 Pages
Warning  Comp. Temp. Threshold:     75 Celsius
Critical Comp. Temp. Threshold:     80 Celsius

Supported Power States
St Op     Max   Active     Idle   RL RT WL WT  Ent_Lat  Ex_Lat
 0 +     9.00W       -        -    0  0  0  0        0       0
 1 +     4.60W       -        -    1  1  1  1        0       0
 2 +     3.80W       -        -    2  2  2  2        0       0
 3 -   0.0450W       -        -    3  3  3  3     2000    2000
 4 -   0.0040W       -        -    4  4  4  4    15000   15000

Supported LBA Sizes (NSID 0x1)
Id Fmt  Data  Metadt  Rel_Perf
 0 +     512       0         0

=== START OF SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

SMART/Health Information (NVMe Log 0x02)
Critical Warning:                   0x00
Temperature:                        45 Celsius
Available Spare:                    100%
Available Spare Threshold:          10%
Percentage Used:                    3%
Data Units Read:                    39,520,633 [20.2 TB]
Data Units Written:                 44,885,887 [22.9 TB]
Host Read Commands:                 433,139,904
Host Write Commands:                375,739,237
Controller Busy Time:               9,300
Power Cycles:                       2,326
Power On Hours:                     4,387
Unsafe Shutdowns:                   370
Media and Data Integrity Errors:    0
Error Information Log Entries:      0
Warning  Comp. Temperature Time:    115
Critical Comp. Temperature Time:    27
Temperature Sensor 2:               45 Celsius
Temperature Sensor 3:               55 Celsius
Temperature Sensor 4:               45 Celsius
Temperature Sensor 5:               45 Celsius
Temperature Sensor 6:               39 Celsius
Thermal Temp. 1 Transition Count:   77
Thermal Temp. 1 Total Time:         1242

Error Information (NVMe Log 0x01, 16 of 256 entries)
No Errors Logged

