smartctl 7.1 2019-12-30 r5022 [x86_64-unknown-openbsd6.8] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Phison Driven SSDs
Device Model:     KINGSTON SUV300S37A240G
Serial Number:    --
Firmware Version: SAFM11.K
User Capacity:    240,057,409,536 bytes [240 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
Form Factor:      2.5 inches
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ACS-2 (minor revision not indicated)
SATA Version is:  SATA 3.1, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Sat Oct 31 00:10:57 2020 MSK
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART Status not supported: Incomplete response, ATA output registers missing
SMART overall-health self-assessment test result: PASSED
Warning: This result is based on an Attribute check.
See vendor-specific Attribute list for marginal Attributes.

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(   30) seconds.
Offline data collection
capabilities: 			 (0x79) SMART execute Offline immediate.
					No Auto Offline data collection support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (   2) minutes.
Conveyance self-test routine
recommended polling time: 	 (   3) minutes.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  1 Raw_Read_Error_Rate     0x000b   100   100   050    Pre-fail  Always       -       0
  2 Not_In_Use              0x0005   100   100   050    Pre-fail  Offline      -       0
  3 Not_In_Use              0x0007   100   100   050    Pre-fail  Always       -       0
  5 Retired_Block_Count     0x0013   100   100   050    Pre-fail  Always       -       0
  7 Not_In_Use              0x000b   100   100   050    Pre-fail  Always       -       0
  8 Not_In_Use              0x0005   100   100   050    Pre-fail  Offline      -       0
  9 Power_On_Hours          0x0012   100   100   000    Old_age   Always       -       19384
 12 Power_Cycle_Count       0x0012   100   100   000    Old_age   Always       -       41
168 SATA_Phy_Error_Count    0x0012   100   100   000    Old_age   Always       -       0
170 Bad_Blk_Ct_Erl/Lat      0x0003   100   100   010    Pre-fail  Always       -       0/265
173 MaxAvgErase_Ct          0x0012   100   100   000    Old_age   Always       -       73 (Average 31)
175 Not_In_Use              0x0013   100   100   050    Pre-fail  Always       -       0
183 Unknown_Phison_Attr     0x0012   100   100   100    Old_age   Always   FAILING_NOW 4784159
187 Reported_Uncorrect      0x0012   100   100   000    Old_age   Always       -       0
192 Unsafe_Shutdown_Count   0x0012   100   100   000    Old_age   Always       -       24
194 Temperature_Celsius     0x0023   069   055   030    Pre-fail  Always       -       31 (Min/Max 21/45)
196 Reallocated_Event_Count 0x0002   100   100   010    Old_age   Always       -       0
197 Not_In_Use              0x0032   100   100   000    Old_age   Always       -       0
199 SATA_CRC_Error_Count    0x000b   100   100   050    Pre-fail  Always       -       0
218 CRC_Error_Count         0x000b   100   100   050    Pre-fail  Always       -       0
231 SSD_Life_Left           0x0013   100   100   000    Pre-fail  Always       -       97
233 Flash_Writes_GiB        0x000b   100   100   000    Pre-fail  Always       -       7491
240 Not_In_Use              0x0013   100   100   000    Pre-fail  Always       -       0
241 Lifetime_Writes_GiB     0x0012   100   100   000    Old_age   Always       -       29976
242 Lifetime_Reads_GiB      0x0012   100   100   000    Old_age   Always       -       3402
244 Average_Erase_Count     0x0002   100   100   000    Old_age   Always       -       31
245 Max_Erase_Count         0x0002   100   100   000    Old_age   Always       -       73
246 Total_Erase_Count       0x0012   100   100   000    Old_age   Always       -       2103808

SMART Error Log Version: 1
No Errors Logged

SMART Self-test log structure revision number 1
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.



