smartctl 7.3 2022-02-28 r5338 [FreeBSD 13.1-STABLE amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Samsung SpinPoint M8 (AF)
Device Model:     ST1000LM024 HN-M101MBB
Serial Number:    --
LU WWN Device Id: 5 0004cf ...
Firmware Version: 2AR10002
User Capacity:    1,000,204,886,016 bytes [1.00 TB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Rotation Rate:    5400 rpm
Form Factor:      2.5 inches
Device is:        In smartctl database 7.3/5319
ATA Version is:   ATA8-ACS T13/1699-D revision 6
SATA Version is:  SATA 3.0, 3.0 Gb/s (current: 3.0 Gb/s)
Local Time is:    Sat Jul 30 23:42:15 2022 +03
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Disabled
APM feature is:   Disabled
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Read SCT Status failed: scsi error medium or hardware error (serious)
Wt Cache Reorder: Unknown (SCT Feature Control command failed)

=== START OF READ SMART DATA SECTION ===
SMART Status not supported: Incomplete response, ATA output registers missing
SMART overall-health self-assessment test result: PASSED
Warning: This result is based on an Attribute check.

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(13620) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 ( 227) minutes.
SCT capabilities: 	       (0x003f)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR-K   100   100   051    -    55
  2 Throughput_Performance  -OS--K   252   252   000    -    0
  3 Spin_Up_Time            PO---K   086   078   025    -    4454
  4 Start_Stop_Count        -O--CK   066   066   000    -    34644
  5 Reallocated_Sector_Ct   PO--CK   252   252   010    -    0
  7 Seek_Error_Rate         -OSR-K   252   252   051    -    0
  8 Seek_Time_Performance   --S--K   252   252   015    -    0
  9 Power_On_Hours          -O--CK   100   100   000    -    5790
 10 Spin_Retry_Count        -O--CK   252   252   051    -    0
 11 Calibration_Retry_Count -O--CK   100   100   000    -    58
 12 Power_Cycle_Count       -O--CK   097   097   000    -    3317
191 G-Sense_Error_Rate      -O---K   100   100   000    -    25
192 Power-Off_Retract_Count -O---K   252   252   000    -    0
194 Temperature_Celsius     -O----   064   052   000    -    30 (Min/Max 21/54)
195 Hardware_ECC_Recovered  -O-RCK   100   100   000    -    0
196 Reallocated_Event_Count -O--CK   252   252   000    -    0
197 Current_Pending_Sector  -O--CK   252   100   000    -    0
198 Offline_Uncorrectable   ----CK   252   252   000    -    0
199 UDMA_CRC_Error_Count    -OS-CK   100   100   000    -    2
200 Multi_Zone_Error_Rate   -O-R-K   100   100   000    -    115
223 Load_Retry_Count        -O--CK   100   100   000    -    58
225 Load_Cycle_Count        -O--CK   080   080   000    -    207403
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

ATA_READ_LOG_EXT (addr=0x00:0x00, page=0, n=1) failed: 48-bit ATA commands require SAT ATA PASS-THROUGH (16)
Read GP Log Directory failed

SMART Log Directory Version 16
Address    Access  R/W   Size  Description
0x00           SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x07           SL  R/O      2  Extended self-test log
0x0d           SL  R/O      3  LPS Mis-alignment log
0x13           SL  R/O      4  SATA NCQ Send and Receive log
0x19           SL  R/O      5  LBA Status log
0x1f           SL  -        7  Reserved
0x25           SL  R/O      8  Saved Device Internal Status Data log
0x2b           SL  -        9  Reserved
0x31           SL  -       10  Reserved
0x37           SL  -       11  Reserved
0x3d           SL  -       12  Reserved
0x43           SL  -      191  Reserved
0x49           SL  -      192  Reserved
0x4f           SL  -      194  Reserved
0x55           SL  -      195  Reserved
0x5b           SL  -      196  Reserved
0x61           SL  -      197  Reserved
0x67           SL  -      198  Reserved
0x6d           SL  -      199  Reserved
0x73           SL  -      200  Reserved
0x79           SL  -      223  Reserved
0x7f           SL  -      225  Reserved

SMART Extended Comprehensive Error Log (GP Log 0x03) not supported

SMART Error Log Version: 16
No Errors Logged

SMART Extended Self-test Log (GP Log 0x07) not supported

SMART Self-test Log not supported

SMART Selective self-test log data structure revision number 16
Note: revision number not 1 implies that no selective self-test has ever been run
 SPAN      MIN_LBA         MAX_LBA  CURRENT_TEST_STATUS
    1        13057      8589934592  Not_testing
    2            0            6403  Not_testing
    3  17179869184               0  Not_testing
    4         2565  56105157787648  Not_testing
    5            0            3848  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

Unknown SCT Status format version 16, should be 2 or 3.

Unknown SCT Status format version 16, should be 2 or 3.
SCT (Get) Error Recovery Control command failed

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

ATA_READ_LOG_EXT (addr=0x11:0x00, page=0, n=1) failed: 48-bit ATA commands require SAT ATA PASS-THROUGH (16)
Read SATA Phy Event Counters failed

