smartctl 7.3 2022-02-28 r5338 [FreeBSD 13.0-RELEASE amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Number:                       PM991 NVMe Samsung 512GB
Serial Number:                      --
Firmware Version:                   25305039
PCI Vendor/Subsystem ID:            0x144d
IEEE OUI Identifier:                0x002538
Total NVM Capacity:                 512,110,190,592 [512 GB]
Unallocated NVM Capacity:           0
Controller ID:                      5
NVMe Version:                       1.3
Number of Namespaces:               1
Namespace 1 Size/Capacity:          512,110,190,592 [512 GB]
Namespace 1 Utilization:            110,390,747,136 [110 GB]
Namespace 1 Formatted LBA Size:     512
Local Time is:                      Wed May  4 10:38:10 2022 BST
Firmware Updates (0x16):            3 Slots, no Reset required
Optional Admin Commands (0x0017):   Security Format Frmw_DL Self_Test
Optional NVM Commands (0x005f):     Comp Wr_Unc DS_Mngmt Wr_Zero Sav/Sel_Feat Timestmp
Log Page Attributes (0x0e):         Cmd_Eff_Lg Ext_Get_Lg Telmtry_Lg
Maximum Data Transfer Size:         512 Pages
Warning  Comp. Temp. Threshold:     81 Celsius
Critical Comp. Temp. Threshold:     85 Celsius

Supported Power States
St Op     Max   Active     Idle   RL RT WL WT  Ent_Lat  Ex_Lat
 0 +     4.83W       -        -    0  0  0  0        0       0
 1 +     3.54W       -        -    1  1  1  1        0       0
 2 +     3.04W       -        -    2  2  2  2        0     500
 3 -   0.0500W       -        -    3  3  3  3      210    1200
 4 -   0.0050W       -        -    4  4  4  4     1000    9000

Supported LBA Sizes (NSID 0x1)
Id Fmt  Data  Metadt  Rel_Perf
 0 +     512       0         0

=== START OF SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

SMART/Health Information (NVMe Log 0x02)
Critical Warning:                   0x00
Temperature:                        15 Celsius
Available Spare:                    100%
Available Spare Threshold:          50%
Percentage Used:                    3%
Data Units Read:                    32,384,102 [16.5 TB]
Data Units Written:                 30,046,528 [15.3 TB]
Host Read Commands:                 1,040,688,683
Host Write Commands:                1,645,485,161
Controller Busy Time:               2,871
Power Cycles:                       534
Power On Hours:                     6,372
Unsafe Shutdowns:                   209
Media and Data Integrity Errors:    0
Error Information Log Entries:      302
Warning  Comp. Temperature Time:    13
Critical Comp. Temperature Time:    9
Temperature Sensor 1:               15 Celsius
Thermal Temp. 1 Transition Count:   1420
Thermal Temp. 2 Transition Count:   32
Thermal Temp. 1 Total Time:         3210
Thermal Temp. 2 Total Time:         822

Error Information (NVMe Log 0x01, 16 of 64 entries)
No Errors Logged

