smartctl 7.4 2023-08-01 r5530 [FreeBSD 13.2-RELEASE-p4 amd64] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     Crucial_FCCT256M550SSD1
Serial Number:    --
LU WWN Device Id: 5 00a075 ...
Firmware Version: MU02
User Capacity:    256,060,514,304 bytes [256 GB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Rotation Rate:    Solid State Device
Form Factor:      2.5 inches
TRIM Command:     Available, deterministic, zeroed
Device is:        Not in smartctl database 7.3/5528
ATA Version is:   ACS-2, ATA8-ACS T13/1699-D revision 6
SATA Version is:  SATA 3.1, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Fri Nov  3 08:16:40 2023 -05
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     254 (maximum performance)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x80)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		( 1190) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (   3) minutes.
Conveyance self-test routine
recommended polling time: 	 (   3) minutes.
SCT capabilities: 	       (0x0035)	SCT Status supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR-K   100   100   000    -    25074422
  5 Reallocated_Sector_Ct   PO--CK   086   086   000    -    325
  9 Power_On_Hours          -O--CK   100   100   000    -    44470
 12 Power_Cycle_Count       -O--CK   100   100   000    -    93617
171 Unknown_Attribute       -O--CK   100   100   000    -    0
172 Unknown_Attribute       -O--CK   100   100   000    -    0
173 Unknown_Attribute       -O--CK   154   154   000    -    6076
174 Unknown_Attribute       -O--CK   100   100   000    -    80
180 Unused_Rsvd_Blk_Cnt_Tot PO--CK   000   000   000    -    1834
183 Runtime_Bad_Block       -O--CK   100   100   000    -    0
184 End-to-End_Error        -O--CK   100   100   000    -    0
187 Reported_Uncorrect      -O--CK   100   100   000    -    29
194 Temperature_Celsius     -O---K   065   052   000    -    35 (Min/Max 19/48)
196 Reallocated_Event_Count -O--CK   100   100   000    -    325
197 Current_Pending_Sector  -O--CK   100   100   000    -    0
198 Offline_Uncorrectable   ----CK   100   100   000    -    0
199 UDMA_CRC_Error_Count    -O--CK   100   100   000    -    0
202 Unknown_SSD_Attribute   P---CK   154   154   000    -    202
206 Unknown_SSD_Attribute   -OSR--   100   100   000    -    0
210 Unknown_Attribute       -O--CK   100   100   000    -    58
246 Unknown_Attribute       -O--CK   100   100   000    -    158015213858
247 Unknown_Attribute       -O--CK   100   100   000    -    4973367253
248 Unknown_Attribute       -O--CK   100   100   000    -    1472163843
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O     51  Comprehensive SMART error log
0x03       GPL     R/O  16383  Ext. Comprehensive SMART error log
0x04       GPL,SL  R/O    255  Device Statistics log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x13       GPL     R/O      1  SATA NCQ Send and Receive log
0x24       GPL     R/O    429  Current Device Internal Status Data log
0x25       GPL     R/O    145  Saved Device Internal Status Data log
0x30       GPL,SL  R/O      9  IDENTIFY DEVICE data log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa0       GPL     VS    2000  Device vendor specific log
0xa0       SL      VS     208  Device vendor specific log
0xa1-0xbf  GPL,SL  VS       1  Device vendor specific log
0xc0       GPL,SL  VS      80  Device vendor specific log
0xc1-0xdf  GPL,SL  VS       1  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (16383 sectors)
Device Error Count: 29
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 29 [28] occurred at disk power-on lifetime: 12556 hours (523 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 50 00 00 0b 4b d3 68 40 08  Error: UNC at LBA = 0x0b4bd368 = 189518696

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 50 00 00 0b 4b d6 50 40 08 26d+01:36:07.040  READ FPDMA QUEUED
  60 00 00 00 40 00 00 0b 4b d3 68 40 08 26d+01:36:07.040  READ FPDMA QUEUED
  60 00 00 00 40 00 00 0b 4b c7 10 40 08 26d+01:36:07.040  READ FPDMA QUEUED
  60 00 00 00 08 00 00 0b 4b c4 e0 40 08 26d+01:36:07.040  READ FPDMA QUEUED
  60 00 00 00 08 00 00 0b 4b c4 d8 40 08 26d+01:36:07.040  READ FPDMA QUEUED

Error 28 [27] occurred at disk power-on lifetime: 4563 hours (190 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 08 00 00 17 72 86 50 40 08  Error: UNC at LBA = 0x17728650 = 393381456

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 00 1d 92 00 10 40 08 41d+00:21:38.112  READ FPDMA QUEUED
  60 00 00 00 08 00 00 1d 91 dc c0 40 08 41d+00:21:38.112  READ FPDMA QUEUED
  60 00 00 00 18 00 00 17 72 86 50 40 08 41d+00:21:38.112  READ FPDMA QUEUED
  60 00 00 00 08 00 00 17 72 54 b0 40 08 41d+00:21:38.112  READ FPDMA QUEUED
  60 00 00 00 08 00 00 17 72 53 30 40 08 41d+00:21:38.112  READ FPDMA QUEUED

Error 27 [26] occurred at disk power-on lifetime: 3213 hours (133 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 30 00 00 01 42 f5 38 40 08  Error: UNC at LBA = 0x0142f538 = 21165368

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 30 00 00 01 44 cd 50 40 08 34d+11:07:25.408  READ FPDMA QUEUED
  60 00 00 00 68 00 00 01 42 f5 38 40 08 34d+11:07:25.408  READ FPDMA QUEUED
  60 00 00 00 18 00 00 01 04 ce e8 40 08 34d+11:07:25.408  READ FPDMA QUEUED
  60 00 00 00 38 00 00 01 44 cd 10 40 08 34d+11:07:25.408  READ FPDMA QUEUED
  60 00 00 00 08 00 00 01 44 cd 48 40 08 34d+11:07:25.408  READ FPDMA QUEUED

Error 26 [25] occurred at disk power-on lifetime: 2585 hours (107 days + 17 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 08 00 00 1b d4 cf 90 40 08  Error: UNC at LBA = 0x1bd4cf90 = 466931600

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 00 1c 01 a8 50 40 08  8d+07:34:25.408  READ FPDMA QUEUED
  60 00 00 00 08 00 00 1c 00 78 e0 40 08  8d+07:34:25.408  READ FPDMA QUEUED
  60 00 00 00 08 00 00 1b de 47 78 40 08  8d+07:34:25.408  READ FPDMA QUEUED
  60 00 00 00 08 00 00 1b db f3 80 40 08  8d+07:34:25.408  READ FPDMA QUEUED
  60 00 00 00 08 00 00 1b db 58 f0 40 08  8d+07:34:25.408  READ FPDMA QUEUED

Error 25 [24] occurred at disk power-on lifetime: 2585 hours (107 days + 17 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 08 00 00 1b d4 cf 90 40 08  Error: UNC at LBA = 0x1bd4cf90 = 466931600

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 00 1c 01 a8 50 40 08  8d+07:34:25.408  READ FPDMA QUEUED
  60 00 00 00 08 00 00 1c 00 78 e0 40 08  8d+07:34:25.408  READ FPDMA QUEUED
  60 00 00 00 08 00 00 1b de 47 78 40 08  8d+07:34:25.408  READ FPDMA QUEUED
  60 00 00 00 08 00 00 1b db f3 80 40 08  8d+07:34:25.408  READ FPDMA QUEUED
  60 00 00 00 08 00 00 1b db 58 f0 40 08  8d+07:34:25.408  READ FPDMA QUEUED

Error 24 [23] occurred at disk power-on lifetime: 2585 hours (107 days + 17 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 08 00 00 1b d4 cf 90 40 08  Error: WP at LBA = 0x1bd4cf90 = 466931600

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 08 00 00 1c 00 89 58 40 08  8d+07:34:25.408  WRITE FPDMA QUEUED
  61 00 00 00 18 00 00 1c 00 38 88 40 08  8d+07:34:25.408  WRITE FPDMA QUEUED
  60 00 00 00 08 00 00 1c 01 a8 50 40 08  8d+07:34:25.408  READ FPDMA QUEUED
  60 00 00 00 08 00 00 1c 00 78 e0 40 08  8d+07:34:25.408  READ FPDMA QUEUED
  60 00 00 00 08 00 00 1b de 47 78 40 08  8d+07:34:25.408  READ FPDMA QUEUED

Error 23 [22] occurred at disk power-on lifetime: 2585 hours (107 days + 17 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 08 00 00 1b d4 cf 90 40 08  Error: UNC at LBA = 0x1bd4cf90 = 466931600

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 00 1b de 47 78 40 08  8d+07:34:25.408  READ FPDMA QUEUED
  60 00 00 00 08 00 00 1b db f3 80 40 08  8d+07:34:25.408  READ FPDMA QUEUED
  60 00 00 00 08 00 00 1b db 58 f0 40 08  8d+07:34:25.408  READ FPDMA QUEUED
  60 00 00 00 08 00 00 1b d8 7c c0 40 08  8d+07:34:25.408  READ FPDMA QUEUED
  60 00 00 00 08 00 00 1b d5 48 68 40 08  8d+07:34:25.408  READ FPDMA QUEUED

Error 22 [21] occurred at disk power-on lifetime: 2554 hours (106 days + 10 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 88 00 00 09 c9 fe e8 40 08  Error: UNC at LBA = 0x09c9fee8 = 164232936

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 03 00 88 00 00 09 c9 fe e8 40 08  7d+00:10:25.408  READ FPDMA QUEUED
  2f 00 00 00 01 00 00 00 00 00 10 e0 08  7d+00:10:25.408  READ LOG EXT
  61 00 00 00 08 00 00 1b 80 5e b0 40 08  7d+00:10:25.408  WRITE FPDMA QUEUED
  60 00 03 00 88 00 00 09 c9 fe e8 40 08  7d+00:10:25.408  READ FPDMA QUEUED
  2f 00 00 00 01 00 00 00 00 00 10 e0 08  7d+00:10:25.408  READ LOG EXT

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Vendor (0xff)       Completed without error       00%     44356         -
# 2  Short offline       Completed without error       00%     44328         -
# 3  Vendor (0xff)       Completed without error       00%     44239         -
# 4  Vendor (0xff)       Completed without error       00%     44224         -
# 5  Short offline       Completed without error       00%     44209         -
# 6  Short offline       Completed without error       00%     44209         -
# 7  Vendor (0xff)       Completed without error       00%     42017         -
# 8  Vendor (0xff)       Completed without error       00%     41177         -
# 9  Vendor (0xff)       Completed without error       00%     36112         -
#10  Vendor (0xff)       Completed without error       00%     32538         -
#11  Vendor (0xff)       Completed without error       00%     25490         -
#12  Vendor (0xff)       Completed without error       00%     25324         -
#13  Vendor (0xff)       Completed without error       00%     25055         -
#14  Vendor (0xff)       Completed without error       00%     24878         -
#15  Vendor (0xff)       Completed without error       00%     24628         -
#16  Vendor (0xff)       Completed without error       00%     23547         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       1 (0x0001)
Device State:                        Active (0)
Current Temperature:                    35 Celsius
Power Cycle Min/Max Temperature:     26/36 Celsius
Lifetime    Min/Max Temperature:     19/48 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      0/70 Celsius
Min/Max Temperature Limit:           -5/75 Celsius
Temperature History Size (Index):    478 (210)

SCT Error Recovery Control command not supported

Device Statistics (GP Log 0x04)
Page  Offset Size        Value Flags Description
0x01  =====  =               =  ===  == General Statistics (rev 2) ==
0x01  0x008  4           93617  ---  Lifetime Power-On Resets
0x01  0x010  4           44470  ---  Power-on Hours
0x01  0x018  6    158015213858  ---  Logical Sectors Written
0x01  0x020  6      6550681855  ---  Number of Write Commands
0x01  0x028  6     47751574245  ---  Logical Sectors Read
0x01  0x030  6      1199598779  ---  Number of Read Commands
0x04  =====  =               =  ===  == General Errors Statistics (rev 1) ==
0x04  0x008  4              29  ---  Number of Reported Uncorrectable Errors
0x04  0x010  4           93573  ---  Resets Between Cmd Acceptance and Completion
0x05  =====  =               =  ===  == Temperature Statistics (rev 1) ==
0x05  0x008  1              35  ---  Current Temperature
0x05  0x010  1              34  ---  Average Short Term Temperature
0x05  0x018  1              34  ---  Average Long Term Temperature
0x05  0x020  1              48  ---  Highest Temperature
0x05  0x028  1              19  ---  Lowest Temperature
0x05  0x030  1              43  ---  Highest Average Short Term Temperature
0x05  0x038  1              22  ---  Lowest Average Short Term Temperature
0x05  0x040  1              41  ---  Highest Average Long Term Temperature
0x05  0x048  1              25  ---  Lowest Average Long Term Temperature
0x05  0x050  4               -  ---  Time in Over-Temperature
0x05  0x058  1              70  ---  Specified Maximum Operating Temperature
0x05  0x060  4               -  ---  Time in Under-Temperature
0x05  0x068  1               0  ---  Specified Minimum Operating Temperature
0x06  =====  =               =  ===  == Transport Statistics (rev 1) ==
0x06  0x008  4             100  ---  Number of Hardware Resets
0x06  0x010  4               0  ---  Number of ASR Events
0x06  0x018  4               0  ---  Number of Interface CRC Errors
0x07  =====  =               =  ===  == Solid State Device Statistics (rev 1) ==
0x07  0x008  1              59  N--  Percentage Used Endurance Indicator
                                |||_ C monitored condition met
                                ||__ D supports DSN
                                |___ N normalized value

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  4            0  Command failed due to ICRC error
0x000a  4            5  Device-to-host register FISes sent due to a COMRESET



