smartctl 7.4 2023-08-01 r5530 [OpenBSD 7.4 amd64] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Phison Driven SSDs
Device Model:     KINGSTON SA400S37240G
Serial Number:    --
LU WWN Device Id: 0 000000 ...
Firmware Version: FW200326
User Capacity:    120,034,123,776 bytes [120 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
Form Factor:      2.5 inches
TRIM Command:     Available
Device is:        In smartctl database 7.3/5528
ATA Version is:   ACS-2 T13/2015-D revision 3
SATA Version is:  SATA 3.2, 6.0 Gb/s (current: 3.0 Gb/s)
Local Time is:    Fri Jan 19 16:48:23 2024 -03
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART Status not supported: Incomplete response, ATA output registers missing
SMART overall-health self-assessment test result: PASSED
Warning: This result is based on an Attribute check.

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  120) seconds.
Offline data collection
capabilities: 			 (0x5d) SMART execute Offline immediate.
					No Auto Offline data collection support.
					Abort Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0002)	Does not save SMART data before
					entering power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (   4) minutes.

SMART Attributes Data Structure revision number: 1
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  1 Raw_Read_Error_Rate     0x0032   100   100   050    Old_age   Always       -       0
  5 Retired_Block_Count     0x0032   100   100   050    Old_age   Always       -       0
  9 Power_On_Hours          0x0032   100   100   050    Old_age   Always       -       42
 12 Power_Cycle_Count       0x0032   100   100   050    Old_age   Always       -       19
160 Unknown_Attribute       0x0032   100   100   050    Old_age   Always       -       0
161 Unknown_Attribute       0x0032   100   100   050    Old_age   Always       -       0
163 Unknown_Attribute       0x0032   100   100   050    Old_age   Always       -       282
164 Unknown_Attribute       0x0032   100   100   050    Old_age   Always       -       0
165 Unknown_Attribute       0x0032   100   100   050    Old_age   Always       -       0
166 Unknown_Attribute       0x0032   100   100   050    Old_age   Always       -       0
167 Write_Protect_Mode      0x0032   100   100   050    Old_age   Always       -       0
168 SATA_Phy_Error_Count    0x0032   100   100   050    Old_age   Always       -       0
169 Bad_Block_Rate          0x0032   100   100   050    Old_age   Always       -       0
175 Not_In_Use              0x0032   100   100   050    Old_age   Always       -       0
176 Erase_Fail_Count_Chip   0x0032   100   100   050    Old_age   Always       -       0
177 Wear_Leveling_Count     0x0032   100   100   050    Old_age   Always       -       0
178 Used_Rsvd_Blk_Cnt_Chip  0x0032   100   100   050    Old_age   Always       -       0
181 Program_Fail_Count      0x0032   100   100   050    Old_age   Always       -       0
182 Erase_Fail_Count        0x0032   100   100   050    Old_age   Always       -       0
192 Unsafe_Shutdown_Count   0x0032   100   100   050    Old_age   Always       -       16
194 Temperature_Celsius     0x0032   100   100   050    Old_age   Always       -       40
195 Power_Fail_Health       0x0032   100   100   050    Old_age   Always       -       0
196 Reallocated_Event_Count 0x0032   100   100   050    Old_age   Always       -       0
197 Not_In_Use              0x0032   100   100   050    Old_age   Always       -       0
198 Offline_Uncorrectable   0x0032   100   100   050    Old_age   Always       -       0
199 SATA_CRC_Error_Count    0x0032   100   100   050    Old_age   Always       -       0
232 Read_Fail_Count         0x0032   100   100   050    Old_age   Always       -       0
241 Lifetime_Writes_GiB     0x0032   100   100   050    Old_age   Always       -       606
242 Lifetime_Reads_GiB      0x0032   100   100   050    Old_age   Always       -       70
249 Unknown_Attribute       0x0032   100   100   050    Old_age   Always       -       619

SMART Error Log Version: 0
No Errors Logged

SMART Self-test log structure revision number 0
Warning: ATA Specification requires self-test log structure revision number = 1
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 0
Note: revision number not 1 implies that no selective self-test has ever been run
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

The above only provides legacy SMART information - try 'smartctl -x' for more



