smartctl 7.1 2019-12-30 r5022 [x86_64-unknown-openbsd6.8] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     ADATA SU630
Serial Number:    --
LU WWN Device Id: 0 000000 ...
Firmware Version: V8X01c87
User Capacity:    240,057,409,536 bytes [240 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
Form Factor:      2.5 inches
Device is:        Not in smartctl database [for details use: -P showall]
ATA Version is:   ACS-3, ATA8-ACS T13/1699-D revision 6
SATA Version is:  SATA 3.1, 6.0 Gb/s (current: 3.0 Gb/s)
Local Time is:    Sun Mar  7 10:26:26 2021 GMT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART Status not supported: Incomplete response, ATA output registers missing
SMART overall-health self-assessment test result: PASSED
Warning: This result is based on an Attribute check.

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(    1) seconds.
Offline data collection
capabilities: 			 (0x59) SMART execute Offline immediate.
					No Auto Offline data collection support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0002)	Does not save SMART data before
					entering power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   7) minutes.
Extended self-test routine
recommended polling time: 	 (  23) minutes.
SCT capabilities: 	       (0x0039)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  1 Raw_Read_Error_Rate     0x002f   100   100   050    Pre-fail  Always       -       0
  5 Reallocated_Sector_Ct   0x0033   100   100   010    Pre-fail  Always       -       0
  9 Power_On_Hours          0x0032   100   100   000    Old_age   Always       -       6093
 12 Power_Cycle_Count       0x0032   100   100   000    Old_age   Always       -       99
161 Unknown_Attribute       0x0032   100   100   000    Old_age   Always       -       0
162 Unknown_Attribute       0x0032   100   100   000    Old_age   Always       -       5987
163 Unknown_Attribute       0x0032   100   100   000    Old_age   Always       -       100
164 Unknown_Attribute       0x0032   100   100   000    Old_age   Always       -       3
166 Unknown_Attribute       0x0032   100   100   000    Old_age   Always       -       46
167 Unknown_Attribute       0x0032   100   100   050    Old_age   Always       -       0
168 Unknown_Attribute       0x0032   100   100   000    Old_age   Always       -       0
169 Unknown_Attribute       0x0032   100   100   000    Old_age   Always       -       100
171 Unknown_Attribute       0x0032   100   100   000    Old_age   Always       -       0
172 Unknown_Attribute       0x0032   100   100   000    Old_age   Always       -       0
174 Unknown_Attribute       0x0032   100   100   000    Old_age   Always       -       87
175 Program_Fail_Count_Chip 0x0032   100   100   000    Old_age   Always       -       0
181 Program_Fail_Cnt_Total  0x0022   100   100   000    Old_age   Always       -       252804
187 Reported_Uncorrect      0x0032   100   100   000    Old_age   Always       -       0
194 Temperature_Celsius     0x0022   100   100   030    Old_age   Always       -       47
195 Hardware_ECC_Recovered  0x003a   100   100   000    Old_age   Always       -       0
196 Reallocated_Event_Count 0x0032   100   100   000    Old_age   Always       -       0
199 UDMA_CRC_Error_Count    0x0032   100   100   000    Old_age   Always       -       0
206 Unknown_SSD_Attribute   0x0032   100   100   000    Old_age   Always       -       0
207 Unknown_SSD_Attribute   0x0032   100   100   000    Old_age   Always       -       39
232 Available_Reservd_Space 0x0032   100   100   000    Old_age   Always       -       100
233 Media_Wearout_Indicator 0x0032   100   100   000    Old_age   Always       -       1710
241 Total_LBAs_Written      0x0032   100   100   000    Old_age   Always       -       276
242 Total_LBAs_Read         0x0032   100   100   000    Old_age   Always       -       186
249 Unknown_Attribute       0x0032   100   100   000    Old_age   Always       -       25
250 Read_Error_Retry_Rate   0x0032   100   100   000    Old_age   Always       -       474

SMART Error Log Version: 1
No Errors Logged

SMART Self-test log structure revision number 1
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 0
Note: revision number not 1 implies that no selective self-test has ever been run
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.



