smartctl 7.4 2023-08-01 r5530 [FreeBSD 13.2-RELEASE-p11 amd64] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Momentus 7200.4
Device Model:     ST9500420AS
Serial Number:    --
LU WWN Device Id: 5 000c50 ...
Firmware Version: 0006HPM1
User Capacity:    500,106,780,160 bytes [500 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    7200 rpm
Form Factor:      2.5 inches
Device is:        In smartctl database 7.3/5528
ATA Version is:   ATA8-ACS T13/1699-D revision 4
SATA Version is:  SATA 2.6, 3.0 Gb/s
Local Time is:    Sun May 19 04:25:28 2024 UTC
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     128 (minimum power consumption without standby)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Unknown

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED
See vendor-specific Attribute list for marginal Attributes.

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(    0) seconds.
Offline data collection
capabilities: 			 (0x53) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 ( 106) minutes.
SCT capabilities: 	       (0x103f)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   113   066   006    -    50422774
  3 Spin_Up_Time            PO----   100   097   085    -    0
  4 Start_Stop_Count        -O--CK   097   097   020    -    3332
  5 Reallocated_Sector_Ct   PO--CK   092   092   036    -    171
  7 Seek_Error_Rate         POSR--   056   051   030    -    700153459624
  9 Power_On_Hours          -O--CK   096   096   000    -    4332
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   097   037   020    -    3242
183 Runtime_Bad_Block       ------   100   253   000    -    96
184 End-to-End_Error        -O--CK   100   100   099    -    0
187 Reported_Uncorrect      -O--CK   001   001   000    -    65535
188 Command_Timeout         -O--CK   100   099   000    -    4295032842
189 High_Fly_Writes         -O-RCK   100   100   000    -    0
190 Airflow_Temperature_Cel -O---K   070   037   045    Past 30 (0 50 31 29 0)
191 G-Sense_Error_Rate      -O--CK   100   100   000    -    53
192 Power-Off_Retract_Count -O--CK   100   100   000    -    54
193 Load_Cycle_Count        -O--CK   082   082   000    -    36358
194 Temperature_Celsius     -O---K   030   063   000    -    30 (0 9 0 0 0)
195 Hardware_ECC_Recovered  -O-RC-   043   038   000    -    50422774
196 Reallocated_Event_Count ------   092   092   000    -    171
197 Current_Pending_Sector  -O--C-   100   100   000    -    18
198 Offline_Uncorrectable   ----C-   100   100   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    0
254 Free_Fall_Sensor        -O--CK   100   100   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01       GPL,SL  R/O      1  Summary SMART error log
0x02       GPL,SL  R/O      5  Comprehensive SMART error log
0x03       GPL,SL  R/O      5  Ext. Comprehensive SMART error log
0x06       GPL,SL  R/O      1  SMART self-test log
0x07       GPL,SL  R/O      1  Extended self-test log
0x09       GPL,SL  R/W      1  Selective self-test log
0x10       GPL,SL  R/O      1  NCQ Command Error log
0x11       GPL,SL  R/O      1  SATA Phy Event Counters log
0x21       GPL,SL  R/O      1  Write stream error log
0x22       GPL,SL  R/O      1  Read stream error log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS      20  Device vendor specific log
0xa2       GPL     VS    2248  Device vendor specific log
0xa8       GPL,SL  VS      65  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xb0       GPL     VS    2864  Device vendor specific log
0xbe-0xbf  GPL     VS   65535  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 55020 (device log contains only the most recent 20 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 55020 [19] occurred at disk power-on lifetime: 3837 hours (159 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 07 a5 c5 39 00 00  Error: UNC at LBA = 0x07a5c539 = 128304441

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 04 00 00 00 07 a5 c1 b8 e0 00  3d+06:21:35.729  READ DMA EXT
  00 00 00 00 00 00 00 00 00 00 00 00 ff  3d+06:21:34.739  NOP [Abort queued commands]
  00 00 00 00 00 00 00 00 00 00 00 00 ff  3d+06:21:34.729  NOP [Abort queued commands]
  25 00 00 04 00 00 00 07 a5 c1 b8 e0 00  3d+06:21:14.727  READ DMA EXT
  00 00 00 00 00 00 00 00 00 00 00 00 ff  3d+06:21:13.738  NOP [Abort queued commands]

Error 55019 [18] occurred at disk power-on lifetime: 3837 hours (159 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 07 a5 c5 39 00 00  Error: UNC at LBA = 0x07a5c539 = 128304441

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 04 00 00 00 07 a5 c1 b8 e0 00  3d+06:21:14.727  READ DMA EXT
  00 00 00 00 00 00 00 00 00 00 00 00 ff  3d+06:21:13.738  NOP [Abort queued commands]
  00 00 00 00 00 00 00 00 00 00 00 00 ff  3d+06:21:13.727  NOP [Abort queued commands]
  25 00 00 04 00 00 00 07 a5 c1 b8 e0 00  3d+06:20:53.727  READ DMA EXT
  35 00 00 00 08 00 00 00 5e b3 88 e0 00  3d+06:20:53.010  WRITE DMA EXT

Error 55018 [17] occurred at disk power-on lifetime: 3837 hours (159 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 07 a5 c5 39 00 00  Error: UNC at LBA = 0x07a5c539 = 128304441

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 04 00 00 00 07 a5 c1 b8 e0 00  3d+06:20:53.727  READ DMA EXT
  35 00 00 00 08 00 00 00 5e b3 88 e0 00  3d+06:20:53.010  WRITE DMA EXT
  35 00 00 00 08 00 00 00 5e b3 98 e0 00  3d+06:20:52.779  WRITE DMA EXT
  35 00 00 00 10 00 00 00 60 7f 80 e0 00  3d+06:20:52.778  WRITE DMA EXT
  00 00 00 00 00 00 00 00 00 00 00 00 ff  3d+06:20:52.736  NOP [Abort queued commands]

Error 55017 [16] occurred at disk power-on lifetime: 3837 hours (159 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 07 a5 c5 39 00 00  Error: UNC at LBA = 0x07a5c539 = 128304441

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 04 00 00 00 07 a5 c1 b8 e0 00  3d+06:20:32.726  READ DMA EXT
  35 00 00 00 08 00 00 00 67 0f d0 e0 00  3d+06:20:32.080  WRITE DMA EXT
  35 00 00 00 08 00 00 00 62 bb f8 e0 00  3d+06:20:32.078  WRITE DMA EXT
  35 00 00 00 08 00 00 00 5e b3 80 e0 00  3d+06:20:32.054  WRITE DMA EXT
  35 00 00 00 08 00 00 00 5e b3 90 e0 00  3d+06:20:32.054  WRITE DMA EXT

Error 55016 [15] occurred at disk power-on lifetime: 3837 hours (159 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 07 a5 c5 39 00 00  Error: UNC at LBA = 0x07a5c539 = 128304441

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 04 00 00 00 07 a5 c1 b8 e0 00  3d+06:20:11.724  READ DMA EXT
  35 00 00 04 00 00 00 04 40 38 f8 e0 00  3d+06:20:11.719  WRITE DMA EXT
  35 00 00 04 00 00 00 04 40 34 f8 e0 00  3d+06:20:11.714  WRITE DMA EXT
  25 00 00 04 00 00 00 04 41 80 78 e0 00  3d+06:20:11.710  READ DMA EXT
  25 00 00 04 00 00 00 04 41 7c 78 e0 00  3d+06:20:11.705  READ DMA EXT

Error 55015 [14] occurred at disk power-on lifetime: 3837 hours (159 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 07 a6 50 e6 00 00  Error: UNC at LBA = 0x07a650e6 = 128340198

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 03 00 00 00 07 a6 50 38 e0 00  3d+06:19:51.222  READ DMA EXT
  00 00 00 00 00 00 00 00 00 00 00 00 ff  3d+06:19:50.232  NOP [Abort queued commands]
  00 00 00 00 00 00 00 00 00 00 00 00 ff  3d+06:19:50.222  NOP [Abort queued commands]
  25 00 00 03 00 00 00 07 a6 50 38 e0 00  3d+06:19:30.222  READ DMA EXT
  35 00 00 00 08 00 00 00 5e b3 88 e0 00  3d+06:19:29.733  WRITE DMA EXT

Error 55014 [13] occurred at disk power-on lifetime: 3837 hours (159 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 07 a6 50 e6 00 00  Error: UNC at LBA = 0x07a650e6 = 128340198

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 03 00 00 00 07 a6 50 38 e0 00  3d+06:19:30.222  READ DMA EXT
  35 00 00 00 08 00 00 00 5e b3 88 e0 00  3d+06:19:29.733  WRITE DMA EXT
  35 00 00 00 08 00 00 00 5e b3 90 e0 00  3d+06:19:29.733  WRITE DMA EXT
  35 00 00 00 10 00 00 00 60 7f 60 e0 00  3d+06:19:29.732  WRITE DMA EXT
  35 00 00 00 08 00 00 00 64 38 88 e0 00  3d+06:19:29.274  WRITE DMA EXT

Error 55013 [12] occurred at disk power-on lifetime: 3837 hours (159 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 07 a6 50 e6 00 00  Error: UNC at LBA = 0x07a650e6 = 128340198

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 03 00 00 00 07 a6 50 38 e0 00  3d+06:19:09.221  READ DMA EXT
  35 00 00 00 08 00 00 00 5e b3 80 e0 00  3d+06:19:09.150  WRITE DMA EXT
  35 00 00 00 08 00 00 00 5e b3 98 e0 00  3d+06:19:09.148  WRITE DMA EXT
  35 00 00 00 60 00 00 00 60 7f 00 e0 00  3d+06:19:09.146  WRITE DMA EXT
  35 00 00 00 08 00 00 00 62 bb 50 e0 00  3d+06:19:09.143  WRITE DMA EXT

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%      1945         -
# 2  Short offline       Completed without error       00%      1945         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       522 (0x020a)
Device State:                        Active (0)
Current Temperature:                    30 Celsius
Power Cycle Min/Max Temperature:     29/31 Celsius
Lifetime    Min/Max Temperature:      9/64 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:     14/55 Celsius
Min/Max Temperature Limit:           10/60 Celsius
Temperature History Size (Index):    128 (100)

SCT Error Recovery Control:
           Read: Disabled
          Write: Disabled

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2           15  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS

