smartctl 7.3 2022-02-28 r5338 [FreeBSD 12.4-RELEASE amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Momentus 5400.6
Device Model:     ST9500325ASG
Serial Number:    --
LU WWN Device Id: 5 000c50 ...
Firmware Version: 0009APM1
User Capacity:    500,107,862,016 bytes [500 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    5400 rpm
Device is:        In smartctl database 7.3/5319
ATA Version is:   ATA8-ACS T13/1699-D revision 4
SATA Version is:  SATA 2.6, 3.0 Gb/s
Local Time is:    Sat Jul 29 18:10:48 2023 CST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     128 (minimum power consumption without standby)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unknown

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(    0) seconds.
Offline data collection
capabilities: 			 (0x73) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 ( 140) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x103f)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     -OSR--   112   073   006    -    42255197
  3 Spin_Up_Time            PO----   100   099   000    -    0
  4 Start_Stop_Count        -O--CK   093   093   020    -    7264
  5 Reallocated_Sector_Ct   PO--CK   047   047   036    -    1101
  7 Seek_Error_Rate         POSR--   084   060   030    -    246520682
  9 Power_On_Hours          -O--CK   089   089   000    -    9877
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   093   093   020    -    7168
184 End-to-End_Error        -O--CK   100   100   099    -    0
187 Reported_Uncorrect      -O--CK   001   001   000    -    65535
188 Command_Timeout         -O--CK   100   001   000    -    73015625332
189 High_Fly_Writes         -O-RCK   100   100   000    -    0
190 Airflow_Temperature_Cel -O---K   064   046   045    -    36 (Min/Max 33/36)
191 G-Sense_Error_Rate      -O--CK   100   100   000    -    393
192 Power-Off_Retract_Count -O--CK   096   095   000    -    9832
193 Load_Cycle_Count        -O--CK   001   001   000    -    405478
194 Temperature_Celsius     -O---K   036   054   000    -    36 (243 52 0 0 0)
195 Hardware_ECC_Recovered  -O-RC-   042   036   000    -    42255197
197 Current_Pending_Sector  -O--C-   100   100   000    -    0
198 Offline_Uncorrectable   ----C-   100   100   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    0
254 Free_Fall_Sensor        -O--CK   001   001   000    -    3001
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01       GPL,SL  R/O      1  Summary SMART error log
0x02       GPL,SL  R/O      5  Comprehensive SMART error log
0x03       GPL,SL  R/O      5  Ext. Comprehensive SMART error log
0x06       GPL,SL  R/O      1  SMART self-test log
0x07       GPL,SL  R/O      1  Extended self-test log
0x09       GPL,SL  R/W      1  Selective self-test log
0x10       GPL,SL  R/O      1  NCQ Command Error log
0x11       GPL,SL  R/O      1  SATA Phy Event Counters log
0x21       GPL,SL  R/O      1  Write stream error log
0x22       GPL,SL  R/O      1  Read stream error log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS     128  Device vendor specific log
0xa2       GPL     VS    2248  Device vendor specific log
0xa8       GPL,SL  VS      65  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xb0       GPL     VS    2972  Device vendor specific log
0xbe-0xbf  GPL     VS   65535  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 20219 (device log contains only the most recent 20 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 20219 [18] occurred at disk power-on lifetime: 9782 hours (407 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 2f 13 6b 00 00  Error: UNC at LBA = 0x002f136b = 3085163

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 08 00 00 00 00 2f 12 28 40 00     00:15:14.192  READ DMA EXT
  25 00 00 08 00 00 00 00 2f 12 28 40 00     00:15:11.570  READ DMA EXT
  ef 00 02 00 00 00 00 00 00 00 00 00 00     00:15:11.519  SET FEATURES [Enable write cache]
  ef 00 aa 00 00 00 00 00 00 00 00 00 00     00:15:11.519  SET FEATURES [Enable read look-ahead]
  ef 00 03 00 46 00 00 00 00 00 00 00 00     00:15:11.519  SET FEATURES [Set transfer mode]

Error 20218 [17] occurred at disk power-on lifetime: 9782 hours (407 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 2f 13 6b 00 00  Error: UNC at LBA = 0x002f136b = 3085163

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 08 00 00 00 00 2f 12 28 40 00     00:15:11.570  READ DMA EXT
  ef 00 02 00 00 00 00 00 00 00 00 00 00     00:15:11.519  SET FEATURES [Enable write cache]
  ef 00 aa 00 00 00 00 00 00 00 00 00 00     00:15:11.519  SET FEATURES [Enable read look-ahead]
  ef 00 03 00 46 00 00 00 00 00 00 00 00     00:15:11.519  SET FEATURES [Set transfer mode]
  00 00 00 00 00 00 00 00 00 00 00 00 ff     00:15:11.502  NOP [Abort queued commands]

Error 20217 [16] occurred at disk power-on lifetime: 9782 hours (407 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 2f 13 6b 00 00  Error: UNC at LBA = 0x002f136b = 3085163

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 08 00 00 00 00 2f 12 28 40 00     00:14:39.499  READ DMA EXT
  25 00 00 08 00 00 00 00 2f 12 28 40 00     00:14:37.079  READ DMA EXT
  2f 00 00 00 01 00 00 00 00 00 10 00 00     00:14:37.078  READ LOG EXT
  60 00 00 08 00 00 00 00 2f 12 28 40 00     00:14:34.739  READ FPDMA QUEUED
  60 00 00 08 00 00 00 00 2f 0a 28 40 00     00:14:34.650  READ FPDMA QUEUED

Error 20216 [15] occurred at disk power-on lifetime: 9782 hours (407 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 2f 13 6b 00 00  Error: UNC at LBA = 0x002f136b = 3085163

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 08 00 00 00 00 2f 12 28 40 00     00:14:37.079  READ DMA EXT
  2f 00 00 00 01 00 00 00 00 00 10 00 00     00:14:37.078  READ LOG EXT
  60 00 00 08 00 00 00 00 2f 12 28 40 00     00:14:34.739  READ FPDMA QUEUED
  60 00 00 08 00 00 00 00 2f 0a 28 40 00     00:14:34.650  READ FPDMA QUEUED
  60 00 00 08 00 00 00 00 2f 02 28 40 00     00:14:34.561  READ FPDMA QUEUED

Error 20215 [14] occurred at disk power-on lifetime: 9782 hours (407 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 2f 13 6b 00 00  Error: UNC at LBA = 0x002f136b = 3085163

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 08 00 00 00 00 2f 12 28 40 00     00:14:34.739  READ FPDMA QUEUED
  60 00 00 08 00 00 00 00 2f 0a 28 40 00     00:14:34.650  READ FPDMA QUEUED
  60 00 00 08 00 00 00 00 2f 02 28 40 00     00:14:34.561  READ FPDMA QUEUED
  60 00 00 08 00 00 00 00 2e fa 28 40 00     00:14:34.461  READ FPDMA QUEUED
  60 00 00 08 00 00 00 00 2e f2 28 40 00     00:14:34.372  READ FPDMA QUEUED

Error 20214 [13] occurred at disk power-on lifetime: 9766 hours (406 days + 22 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 2f 13 6b 00 00  Error: UNC at LBA = 0x002f136b = 3085163

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 03 03 01 00 00 00 00 2f 12 f0 40 00     00:12:10.983  READ DMA EXT
  25 03 03 00 10 00 00 1d 21 d2 58 4d 00     00:12:10.979  READ DMA EXT
  35 03 03 00 01 00 00 1d 29 f9 c0 4d 00     00:12:10.978  WRITE DMA EXT
  25 03 03 00 40 00 00 1d 37 c8 f8 4d 00     00:12:10.874  READ DMA EXT
  25 03 03 01 00 00 00 00 2f 12 f0 40 00     00:12:08.485  READ DMA EXT

Error 20213 [12] occurred at disk power-on lifetime: 9766 hours (406 days + 22 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 2f 13 6b 00 00  Error: UNC at LBA = 0x002f136b = 3085163

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 03 03 01 00 00 00 00 2f 12 f0 40 00     00:12:08.485  READ DMA EXT
  25 03 03 00 08 00 00 1e d9 fc 70 4e 00     00:12:08.475  READ DMA EXT
  25 03 03 00 10 00 00 1d 3a d9 a8 4d 00     00:12:08.395  READ DMA EXT
  35 03 03 00 08 00 00 1d c9 f9 20 4d 00     00:12:08.394  WRITE DMA EXT
  25 03 03 01 00 00 00 00 2f 12 f0 40 00     00:12:05.996  READ DMA EXT

Error 20212 [11] occurred at disk power-on lifetime: 9766 hours (406 days + 22 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 2f 13 6b 00 00  Error: UNC at LBA = 0x002f136b = 3085163

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 03 03 01 00 00 00 00 2f 12 f0 40 00     00:12:05.996  READ DMA EXT
  25 03 03 00 10 00 00 1d 39 2a 08 4d 00     00:12:05.974  READ DMA EXT
  35 03 03 00 08 00 00 1d c9 9d c0 4d 00     00:12:05.973  WRITE DMA EXT
  35 03 03 00 08 00 00 1e 2e 1f 88 4e 00     00:12:05.972  WRITE DMA EXT
  35 03 03 00 10 00 00 1d db 51 40 4d 00     00:12:05.971  WRITE DMA EXT

SMART Extended Self-test Log Version: 1 (1 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       522 (0x020a)
Device State:                        Active (0)
Current Temperature:                    36 Celsius
Power Cycle Min/Max Temperature:     33/36 Celsius
Lifetime    Min/Max Temperature:      0/54 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      3/62 Celsius
Min/Max Temperature Limit:            0/65 Celsius
Temperature History Size (Index):    128 (118)

SCT Error Recovery Control:
           Read: Disabled
          Write: Disabled

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2           14  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS

