smartctl 7.4 2023-08-01 r5530 [FreeBSD 14.2-RELEASE amd64] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Toshiba 2.5" HDD MK..52GSX
Device Model:     TOSHIBA MK3252GSX
Serial Number:    --
LU WWN Device Id: 5 000039 ...
Firmware Version: LV011C
User Capacity:    320,072,933,376 bytes [320 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database 7.3/5528
ATA Version is:   ATA8-ACS (minor revision not indicated)
SATA Version is:  SATA 2.6, 3.0 Gb/s
Local Time is:    Fri Dec 20 00:37:11 2024 CET
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     128 (minimum power consumption without standby)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Write SCT (Get) Feature Control Command failed: Input/output error
Wt Cache Reorder: Unknown (SCT Feature Control command failed)

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED
See vendor-specific Attribute list for marginal Attributes.

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  120) seconds.
Offline data collection
capabilities: 			 (0x51) SMART execute Offline immediate.
					No Auto Offline data collection support.
					Suspend Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 ( 115) minutes.
SCT capabilities: 	       (0x0033)	SCT Status supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   100   100   050    -    0
  2 Throughput_Performance  POS---   100   100   050    -    0
  3 Spin_Up_Time            PO----   100   100   002    -    1534
  4 Start_Stop_Count        -O--CK   100   100   000    -    5932
  5 Reallocated_Sector_Ct   PO--CK   100   100   010    -    0
  7 Seek_Error_Rate         POSR--   100   100   050    -    0
  8 Seek_Time_Performance   P-S---   100   100   050    -    0
  9 Power_On_Hours          -O--CK   053   053   000    -    18971
 10 Spin_Retry_Count        PO--C-   218   100   030    -    0
 12 Power_Cycle_Count       -O--CK   100   100   000    -    4307
184 End-to-End_Error        -O--CK   001   001   001    NOW  6191
187 Reported_Uncorrect      -O--CK   001   001   000    -    6191
188 Command_Timeout         -O--CK   100   099   000    -    2
189 High_Fly_Writes         -O-RCK   100   100   001    -    0
190 Airflow_Temperature_Cel -O---K   079   039   045    Past 21 (Min/Max 21/22)
191 G-Sense_Error_Rate      -O--CK   100   100   000    -    875
192 Power-Off_Retract_Count -O--CK   100   100   000    -    12255419
193 Load_Cycle_Count        -O--CK   097   097   000    -    34221
194 Temperature_Celsius     -O---K   100   100   000    -    21 (Min/Max 11/61)
196 Reallocated_Event_Count -O--CK   100   100   000    -    0
197 Current_Pending_Sector  -O--C-   100   100   000    -    8
198 Offline_Uncorrectable   ----C-   100   100   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    0
220 Disk_Shift              -O----   100   100   000    -    8334
222 Loaded_Hours            -O--CK   068   068   000    -    12915
223 Load_Retry_Count        -O--CK   100   100   000    -    0
224 Load_Friction           -O---K   100   100   000    -    0
226 Load-in_Time            -OS--K   100   100   000    -    339
240 Head_Flying_Hours       P-----   100   100   001    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O     51  Comprehensive SMART error log
0x03       GPL     R/O     64  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (64 sectors)
Device Error Count: 8384 (device log contains only the most recent 256 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 8384 [191] occurred at disk power-on lifetime: 16992 hours (708 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 41 00 0a 00 00 09 4d 6a ab 69 00  Error: WP at LBA = 0x094d6aab = 156068523

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 08 00 18 00 00 00 5e dd 70 40 00     00:02:45.294  WRITE FPDMA QUEUED
  61 00 08 00 18 00 00 00 5e dd 80 40 00     00:02:45.294  WRITE FPDMA QUEUED
  61 00 08 00 18 00 00 00 5e e7 f0 40 00     00:02:45.294  WRITE FPDMA QUEUED
  60 00 08 00 20 00 00 00 65 3b d8 40 00     00:02:42.689  READ FPDMA QUEUED
  60 00 02 00 10 00 00 00 0f 36 75 40 00     00:02:42.689  READ FPDMA QUEUED

Error 8383 [190] occurred at disk power-on lifetime: 16992 hours (708 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 41 00 12 00 00 09 4d 6a ab 69 00  Error: WP at LBA = 0x094d6aab = 156068523

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 08 00 20 00 00 00 64 25 18 40 00     00:02:40.084  WRITE FPDMA QUEUED
  60 00 02 00 18 00 00 00 0f 36 75 40 00     00:02:38.476  READ FPDMA QUEUED
  60 00 08 00 08 00 00 00 65 3b d8 40 00     00:02:38.463  READ FPDMA QUEUED
  60 00 08 00 38 00 00 00 0f 33 60 40 00     00:02:38.415  READ FPDMA QUEUED
  60 00 40 00 10 00 00 09 4d 6a a8 40 00     00:02:38.415  READ FPDMA QUEUED

Error 8382 [189] occurred at disk power-on lifetime: 16992 hours (708 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 41 00 5a 00 00 09 4d 6a ab 69 00  Error: WP at LBA = 0x094d6aab = 156068523

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 08 00 30 00 00 00 5e dd 78 40 00     00:02:35.046  WRITE FPDMA QUEUED
  61 00 08 00 28 00 00 00 5e dd 88 40 00     00:02:35.045  WRITE FPDMA QUEUED
  61 00 08 00 20 00 00 00 5e e7 e8 40 00     00:02:35.045  WRITE FPDMA QUEUED
  61 00 07 00 20 00 00 00 0c 2a 70 40 00     00:02:34.796  WRITE FPDMA QUEUED
  61 00 04 00 18 00 00 00 0c 0c b8 40 00     00:02:34.796  WRITE FPDMA QUEUED

Error 8381 [188] occurred at disk power-on lifetime: 16992 hours (708 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 41 00 32 00 00 09 4d 6a ab 69 00  Error: WP at LBA = 0x094d6aab = 156068523

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 08 00 50 00 00 00 03 2f 08 40 00     00:02:32.783  WRITE FPDMA QUEUED
  60 00 08 00 48 00 00 00 1d 16 58 40 00     00:02:30.029  READ FPDMA QUEUED
  60 00 08 00 48 00 00 00 65 34 08 40 00     00:02:30.023  READ FPDMA QUEUED
  60 00 08 00 38 00 00 00 65 32 08 40 00     00:02:30.023  READ FPDMA QUEUED
  60 00 08 00 38 00 00 00 65 31 30 40 00     00:02:30.022  READ FPDMA QUEUED

Error 8380 [187] occurred at disk power-on lifetime: 16992 hours (708 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 41 00 0a 00 00 09 4d 6a ab 69 00  Error: WP at LBA = 0x094d6aab = 156068523

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 08 00 38 00 00 00 03 38 80 40 00     00:02:28.790  WRITE FPDMA QUEUED
  61 00 08 00 30 00 00 01 cf dc c8 40 00     00:02:28.790  WRITE FPDMA QUEUED
  61 00 08 00 28 00 00 00 5e e7 e0 40 00     00:02:27.090  WRITE FPDMA QUEUED
  61 00 08 00 20 00 00 00 08 97 60 40 00     00:02:26.794  WRITE FPDMA QUEUED
  61 00 10 00 18 00 00 02 0d 17 e8 40 00     00:02:26.793  WRITE FPDMA QUEUED

Error 8379 [186] occurred at disk power-on lifetime: 16992 hours (708 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 41 00 72 00 00 09 4d 6a ab 69 00  Error: WP at LBA = 0x094d6aab = 156068523

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 08 00 50 00 00 00 62 f0 50 40 00     00:02:22.787  WRITE FPDMA QUEUED
  61 00 08 00 48 00 00 00 62 f0 38 40 00     00:02:22.786  WRITE FPDMA QUEUED
  61 00 08 00 40 00 00 00 62 f0 00 40 00     00:02:22.786  WRITE FPDMA QUEUED
  61 00 08 00 38 00 00 00 62 ee 18 40 00     00:02:22.786  WRITE FPDMA QUEUED
  61 00 08 00 30 00 00 00 62 e2 c8 40 00     00:02:22.786  WRITE FPDMA QUEUED

Error 8378 [185] occurred at disk power-on lifetime: 16992 hours (708 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 41 00 12 00 00 09 4d 6a ab 69 00  Error: WP at LBA = 0x094d6aab = 156068523

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 08 00 48 00 00 00 03 28 18 40 00     00:02:12.723  WRITE FPDMA QUEUED
  60 00 08 00 40 00 00 00 63 2b f8 40 00     00:02:12.723  READ FPDMA QUEUED
  61 00 08 00 38 00 00 00 63 28 38 40 00     00:02:12.723  WRITE FPDMA QUEUED
  61 00 18 00 30 00 00 00 5e e7 c0 40 00     00:02:12.723  WRITE FPDMA QUEUED
  61 00 02 00 28 00 00 00 15 d7 a0 40 00     00:02:12.723  WRITE FPDMA QUEUED

Error 8377 [184] occurred at disk power-on lifetime: 16992 hours (708 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 41 00 12 00 00 09 4d 6a ab 69 00  Error: WP at LBA = 0x094d6aab = 156068523

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 08 00 48 00 00 00 03 28 18 40 00     00:02:08.527  WRITE FPDMA QUEUED
  60 00 08 00 40 00 00 00 63 2b f8 40 00     00:02:08.527  READ FPDMA QUEUED
  61 00 08 00 38 00 00 00 63 28 38 40 00     00:02:08.527  WRITE FPDMA QUEUED
  61 00 18 00 30 00 00 00 5e e7 c0 40 00     00:02:08.527  WRITE FPDMA QUEUED
  61 00 02 00 28 00 00 00 15 d7 a0 40 00     00:02:08.527  WRITE FPDMA QUEUED

SMART Extended Self-test Log Version: 1 (1 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  2
SCT Version (vendor specific):       1 (0x0001)
Device State:                        Active (0)
Current Temperature:                    21 Celsius
Power Cycle Min/Max Temperature:     21/22 Celsius
Lifetime    Min/Max Temperature:     11/61 Celsius
Under/Over Temperature Limit Count:   0/96

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      5/55 Celsius
Min/Max Temperature Limit:            5/55 Celsius
Temperature History Size (Index):    478 (78)

SCT Error Recovery Control command not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  4            0  Command failed due to ICRC error
0x0002  4            0  R_ERR response for data FIS
0x0003  4            0  R_ERR response for device-to-host data FIS
0x0004  4            0  R_ERR response for host-to-device data FIS
0x0005  4            0  R_ERR response for non-data FIS
0x0006  4            0  R_ERR response for device-to-host non-data FIS
0x0007  4            0  R_ERR response for host-to-device non-data FIS
0x0008  4            0  Device-to-host non-data FIS retries
0x0009  4            4  Transition from drive PhyRdy to drive PhyNRdy
0x000a  4            5  Device-to-host register FISes sent due to a COMRESET
0x000b  4            0  CRC errors within host-to-device FIS
0x000d  4            0  Non-CRC errors within host-to-device FIS
0x000f  4            0  R_ERR response for host-to-device data FIS, CRC
0x0010  4            0  R_ERR response for host-to-device data FIS, non-CRC
0x0012  4            0  R_ERR response for host-to-device non-data FIS, CRC
0x0013  4            0  R_ERR response for host-to-device non-data FIS, non-CRC



