smartctl 7.4 2023-08-01 r5530 [FreeBSD 14.2-RELEASE i386] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Barracuda 7200.10
Device Model:     ST3250410AS
Serial Number:    --
Firmware Version: 3.AAC
User Capacity:    250,059,350,016 bytes [250 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database 7.3/5528
ATA Version is:   ATA/ATAPI-7 (minor revision not indicated)
Local Time is:    Mon Dec 16 22:34:55 2024 MSK
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  430) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (  64) minutes.
SCT capabilities: 	       (0x0001)	SCT Status supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   114   081   006    -    70647879
  3 Spin_Up_Time            PO----   097   097   000    -    0
  4 Start_Stop_Count        -O--CK   094   094   020    -    6595
  5 Reallocated_Sector_Ct   PO--CK   100   100   036    -    4
  7 Seek_Error_Rate         POSR--   083   060   030    -    219854262
  9 Power_On_Hours          -O--CK   093   093   000    -    6766
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   094   094   020    -    7004
187 Reported_Uncorrect      -O--CK   001   001   000    -    20048
189 High_Fly_Writes         -O-RCK   100   100   000    -    0
190 Airflow_Temperature_Cel -O---K   055   051   045    -    45 (Min/Max 23/45)
194 Temperature_Celsius     -O---K   045   049   000    -    45 (0 10 0 0 0)
195 Hardware_ECC_Recovered  -O-RC-   066   054   000    -    3679323
197 Current_Pending_Sector  -O--C-   100   073   000    -    1
198 Offline_Uncorrectable   ----C-   100   073   000    -    1
199 UDMA_CRC_Error_Count    -OSRCK   200   196   000    -    69
200 Multi_Zone_Error_Rate   ------   100   253   000    -    0
202 Data_Address_Mark_Errs  -O--CK   099   252   000    -    1
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

ATA_READ_LOG_EXT (addr=0x00:0x00, page=0, n=1) failed: 48-bit ATA commands not implemented [JMicron]
Read GP Log Directory failed

SMART Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00           SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03           SL  R/O      5  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07           SL  R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10           SL  R/O      1  NCQ Command Error log
0x11           SL  R/O      1  SATA Phy Event Counters log
0x20           SL  R/O      1  Streaming performance log
0x21           SL  R/O      1  Write stream error log
0x22           SL  R/O      1  Read stream error log
0x23           SL  R/O      1  Delayed sector log
0x80-0x9f      SL  R/W     16  Host vendor specific log
0xa0           SL  VS       1  Device vendor specific log
0xa1           SL  VS      20  Device vendor specific log
0xa2           SL  VS     101  Device vendor specific log
0xa8           SL  VS      20  Device vendor specific log
0xa9           SL  VS       1  Device vendor specific log
0xe0           SL  R/W      1  SCT Command/Status
0xe1           SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log (GP Log 0x03) not supported

SMART Error Log Version: 1
ATA Error Count: 20199 (device log contains only the most recent five errors)
	CR = Command Register [HEX]
	FR = Features Register [HEX]
	SC = Sector Count Register [HEX]
	SN = Sector Number Register [HEX]
	CL = Cylinder Low Register [HEX]
	CH = Cylinder High Register [HEX]
	DH = Device/Head Register [HEX]
	DC = Device Command Register [HEX]
	ER = Error register [HEX]
	ST = Status register [HEX]
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 20199 occurred at disk power-on lifetime: 6641 hours (276 days + 17 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 00 4d 42 99 e0  Error: UNC at LBA = 0x0099424d = 10043981

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 00 80 00 42 99 e0 00      00:28:19.088  READ DMA EXT
  25 00 40 80 c2 a4 e0 00      00:28:19.081  READ DMA EXT
  25 00 40 00 bf a4 e0 00      00:28:19.073  READ DMA EXT
  25 00 40 c0 98 a4 e0 00      00:28:19.064  READ DMA EXT
  25 00 40 00 8b a4 e0 00      00:28:19.170  READ DMA EXT

Error 20198 occurred at disk power-on lifetime: 6641 hours (276 days + 17 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 00 4d 42 99 e0  Error: UNC at LBA = 0x0099424d = 10043981

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 00 01 4d 42 99 e0 00      00:26:06.437  READ DMA EXT
  25 00 01 4c 42 99 e0 00      00:26:06.417  READ DMA EXT
  25 00 01 4b 42 99 e0 00      00:26:06.461  READ DMA EXT
  25 00 01 4a 42 99 e0 00      00:26:06.461  READ DMA EXT
  25 00 01 49 42 99 e0 00      00:26:06.460  READ DMA EXT

Error 20197 occurred at disk power-on lifetime: 6641 hours (276 days + 17 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 00 4d 42 99 e0  Error: UNC at LBA = 0x0099424d = 10043981

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 00 40 40 42 99 e0 00      00:26:02.269  READ DMA EXT
  25 00 40 00 42 99 e0 00      00:26:02.269  READ DMA EXT
  25 00 08 98 90 98 e0 00      00:26:02.262  READ DMA EXT
  25 00 08 70 90 98 e0 00      00:26:02.327  READ DMA EXT
  25 00 08 48 90 98 e0 00      00:26:02.318  READ DMA EXT

Error 20196 occurred at disk power-on lifetime: 6641 hours (276 days + 17 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 00 4d 42 99 e0  Error: UNC at LBA = 0x0099424d = 10043981

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 00 01 4d 42 99 e0 00      00:25:33.411  READ DMA EXT
  25 00 01 4c 42 99 e0 00      00:25:33.455  READ DMA EXT
  25 00 01 4b 42 99 e0 00      00:25:33.455  READ DMA EXT
  25 00 01 4a 42 99 e0 00      00:25:33.454  READ DMA EXT
  25 00 01 49 42 99 e0 00      00:25:33.454  READ DMA EXT

Error 20195 occurred at disk power-on lifetime: 6641 hours (276 days + 17 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 00 4d 42 99 e0  Error: UNC at LBA = 0x0099424d = 10043981

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 00 40 40 42 99 e0 00      00:25:29.248  READ DMA EXT
  25 00 08 00 e0 09 e0 00      00:25:29.248  READ DMA EXT
  25 00 40 80 01 00 e0 00      00:25:29.349  READ DMA EXT
  25 00 08 80 19 26 e0 00      00:25:29.312  READ DMA EXT
  25 00 40 c0 7c 25 e0 00      00:25:29.298  READ DMA EXT

SMART Extended Self-test Log (GP Log 0x07) not supported

SMART Self-test log structure revision number 1

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  2
SCT Version (vendor specific):       521 (0x0209)
Device State:                        Active (0)
Current Temperature:                    45 Celsius
Power Cycle Min/Max Temperature:     --/ 0 Celsius
Lifetime    Min/Max Temperature:     --/ 0 Celsius

SCT Data Table command not supported

SCT Error Recovery Control command not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

ATA_READ_LOG_EXT (addr=0x11:0x00, page=0, n=1) failed: 48-bit ATA commands not implemented [JMicron]
Read SATA Phy Event Counters failed

