smartctl 7.3 2022-02-28 r5338 [FreeBSD 13.1-RELEASE amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Laptop SSHD
Device Model:     ST500LM000-1EJ162-SSHD-8GB
Serial Number:    --
LU WWN Device Id: 5 000c50 ...
Firmware Version: LVD6
User Capacity:    500,107,862,016 bytes [500 GB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Rotation Rate:    5400 rpm
Form Factor:      2.5 inches
Device is:        In smartctl database 7.3/5319
ATA Version is:   ACS-2, ACS-3 T13/2161-D revision 3b
SATA Version is:  SATA 3.1, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Tue Sep  5 05:27:40 2023 CEST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Disabled
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED
See vendor-specific Attribute list for marginal Attributes.

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  150) seconds.
Offline data collection
capabilities: 			 (0x73) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (  99) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x1081)	SCT Status supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   117   099   006    -    121953400
  3 Spin_Up_Time            PO----   098   098   000    -    0
  4 Start_Stop_Count        -O--CK   079   079   020    -    22236
  5 Reallocated_Sector_Ct   PO--CK   100   100   010    -    0
  7 Seek_Error_Rate         POSR--   074   060   030    -    64844924853
  9 Power_On_Hours          -O--CK   074   074   000    -    23034
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   093   093   020    -    7525
184 End-to-End_Error        -O--CK   001   001   099    NOW  280
187 Reported_Uncorrect      -O--CK   098   098   000    -    2
188 Command_Timeout         -O--CK   099   098   000    -    393598
189 High_Fly_Writes         -O-RCK   100   100   000    -    0
190 Airflow_Temperature_Cel -O---K   058   040   045    Past 42 (Min/Max 33/42 #38)
191 G-Sense_Error_Rate      -O--CK   100   100   000    -    0
192 Power-Off_Retract_Count -O--CK   100   100   000    -    536
193 Load_Cycle_Count        -O--CK   070   070   000    -    61905
194 Temperature_Celsius     -O---K   042   060   000    -    42 (0 17 0 0 0)
197 Current_Pending_Sector  -O--C-   100   100   000    -    0
198 Offline_Uncorrectable   ----C-   100   100   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    0
254 Free_Fall_Sensor        -O--CK   100   100   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      5  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x21       GPL     R/O      1  Write stream error log
0x22       GPL     R/O      1  Read stream error log
0x24       GPL     R/O   1223  Current Device Internal Status Data log
0x25       GPL     R/O   1223  Saved Device Internal Status Data log
0x30       GPL,SL  R/O      9  IDENTIFY DEVICE data log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS      20  Device vendor specific log
0xa2       GPL     VS    3900  Device vendor specific log
0xa8       GPL,SL  VS     129  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xab       GPL     VS       1  Device vendor specific log
0xae       GPL     VS       1  Device vendor specific log
0xb0       GPL     VS    4580  Device vendor specific log
0xbe-0xbf  GPL     VS   65535  Device vendor specific log
0xc1       GPL,SL  VS      10  Device vendor specific log
0xc2       GPL,SL  VS      50  Device vendor specific log
0xc4       GPL,SL  VS       5  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 26 (device log contains only the most recent 20 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 26 [5] occurred at disk power-on lifetime: 22184 hours (924 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 1f 6e e8 18 00 00  Error: UNC at LBA = 0x1f6ee818 = 527362072

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 40 00 00 1f 6e e8 00 e0 00     00:00:54.132  READ DMA EXT
  25 00 00 00 01 00 00 1f 6e e8 08 e0 00     00:00:54.132  READ DMA EXT
  00 00 00 00 00 00 00 00 00 00 00 00 04     00:00:53.995  NOP [Abort queued commands]
  25 00 00 00 40 00 00 1f 6e e8 00 e0 00     00:00:53.966  READ DMA EXT
  25 00 00 00 01 00 00 1f 6e e8 08 e0 00     00:00:53.965  READ DMA EXT

Error 25 [4] occurred at disk power-on lifetime: 22184 hours (924 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 1f 6e e8 18 00 00  Error: UNC at LBA = 0x1f6ee818 = 527362072

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 40 00 00 1f 6e e8 00 e0 00     00:00:53.966  READ DMA EXT
  25 00 00 00 01 00 00 1f 6e e8 08 e0 00     00:00:53.965  READ DMA EXT
  00 00 00 00 00 00 00 00 00 00 00 00 04     00:00:53.819  NOP [Abort queued commands]
  25 00 00 00 40 00 00 1f 6e e8 00 e0 00     00:00:53.790  READ DMA EXT
  25 00 00 00 01 00 00 1f 6e e8 02 e0 00     00:00:53.652  READ DMA EXT

Error 24 [3] occurred at disk power-on lifetime: 22184 hours (924 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 1f 6e e8 18 00 00  Error: UNC at LBA = 0x1f6ee818 = 527362072

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 40 00 00 1f 6e e8 00 e0 00     00:00:53.790  READ DMA EXT
  25 00 00 00 01 00 00 1f 6e e8 02 e0 00     00:00:53.652  READ DMA EXT
  00 00 00 00 00 00 00 00 00 00 00 00 04     00:00:53.573  NOP [Abort queued commands]
  25 00 00 00 40 00 00 1f 6e e8 00 e0 00     00:00:53.543  READ DMA EXT
  25 00 00 00 40 00 00 00 00 00 00 e0 00     00:00:53.542  READ DMA EXT

Error 23 [2] occurred at disk power-on lifetime: 22184 hours (924 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 1f 6e e8 18 00 00  Error: UNC at LBA = 0x1f6ee818 = 527362072

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 40 00 00 1f 6e e8 00 e0 00     00:00:53.543  READ DMA EXT
  25 00 00 00 40 00 00 00 00 00 00 e0 00     00:00:53.542  READ DMA EXT
  25 00 00 00 40 00 00 29 3b 01 00 e0 00     00:00:53.512  READ DMA EXT
  25 00 00 00 40 00 00 29 3b 00 c0 e0 00     00:00:53.426  READ DMA EXT
  25 00 00 00 40 00 00 29 3b 00 80 e0 00     00:00:53.423  READ DMA EXT

Error 22 [1] occurred at disk power-on lifetime: 22184 hours (924 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 1f 6e e8 18 00 00  Error: UNC at LBA = 0x1f6ee818 = 527362072

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 40 00 00 1f 6e e8 00 e0 00     00:00:45.112  READ DMA EXT
  25 00 00 00 01 00 00 1f 6e e8 08 e0 00     00:00:45.112  READ DMA EXT
  00 00 00 00 00 00 00 00 00 00 00 00 04     00:00:44.954  NOP [Abort queued commands]
  25 00 00 00 40 00 00 1f 6e e8 00 e0 00     00:00:44.925  READ DMA EXT
  25 00 00 00 40 00 00 1f 70 09 c0 e0 00     00:00:44.924  READ DMA EXT

Error 21 [0] occurred at disk power-on lifetime: 22184 hours (924 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 1f 6e e8 18 00 00  Error: UNC at LBA = 0x1f6ee818 = 527362072

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 40 00 00 1f 6e e8 00 e0 00     00:00:44.925  READ DMA EXT
  25 00 00 00 40 00 00 1f 70 09 c0 e0 00     00:00:44.924  READ DMA EXT
  25 00 00 00 40 00 00 1f 6f 09 c0 e0 00     00:00:44.924  READ DMA EXT
  25 00 00 00 01 00 00 1f 6e e8 08 e0 00     00:00:44.924  READ DMA EXT
  00 00 00 00 00 00 00 00 00 00 00 00 04     00:00:44.775  NOP [Abort queued commands]

Error 20 [19] occurred at disk power-on lifetime: 22184 hours (924 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 1f 6e e8 18 00 00  Error: UNC at LBA = 0x1f6ee818 = 527362072

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 40 00 00 1f 6e e8 00 e0 00     00:00:44.756  READ DMA EXT
  25 00 00 00 01 00 00 1f 6e e8 02 e0 00     00:00:44.755  READ DMA EXT
  00 00 00 00 00 00 00 00 00 00 00 00 04     00:00:44.737  NOP [Abort queued commands]
  25 00 00 00 40 00 00 1f 6e e8 00 e0 00     00:00:44.708  READ DMA EXT
  25 00 00 00 40 00 00 29 3d 4d 40 e0 00     00:00:42.607  READ DMA EXT

Error 19 [18] occurred at disk power-on lifetime: 22184 hours (924 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 1f 6e e8 18 00 00  Error: UNC at LBA = 0x1f6ee818 = 527362072

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 40 00 00 1f 6e e8 00 e0 00     00:00:44.708  READ DMA EXT
  25 00 00 00 40 00 00 29 3d 4d 40 e0 00     00:00:42.607  READ DMA EXT
  25 00 00 00 01 00 00 1f 6e e8 08 e0 00     00:00:42.605  READ DMA EXT
  00 00 00 00 00 00 00 00 00 00 00 00 04     00:00:42.456  NOP [Abort queued commands]
  25 00 00 00 40 00 00 1f 6e e8 00 e0 00     00:00:42.428  READ DMA EXT

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%     18338         -
# 2  Short offline       Aborted by host               30%     17743         -
# 3  Short offline       Completed without error       00%     17722         -
# 4  Extended offline    Completed without error       00%     14961         -
# 5  Short offline       Completed without error       00%     14277         -
# 6  Short offline       Completed without error       00%     14186         -
# 7  Short offline       Interrupted (host reset)      00%     14141         -
# 8  Short offline       Completed without error       00%     14117         -
# 9  Short offline       Completed without error       00%     14099         -
#10  Short offline       Completed without error       00%     14091         -
#11  Short offline       Completed without error       00%     14084         -
#12  Short offline       Completed without error       00%     14021         -
#13  Short offline       Completed without error       00%     14008         -
#14  Short offline       Completed without error       00%     14007         -
#15  Short offline       Completed without error       00%     13960         -
#16  Short offline       Completed without error       00%     13950         -
#17  Short offline       Completed without error       00%     13945         -
#18  Short offline       Completed without error       00%     13918         -
#19  Short offline       Completed without error       00%     13503         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       522 (0x020a)
Device State:                        Active (0)
Current Temperature:                    41 Celsius
Power Cycle Min/Max Temperature:     25/41 Celsius
Lifetime    Min/Max Temperature:     17/59 Celsius
Under/Over Temperature Limit Count:   0/4

SCT Data Table command not supported

SCT Error Recovery Control command not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2           24  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS



