smartctl 7.4 2023-08-01 r5530 [FreeBSD 14.0-RELEASE amd64] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Momentus 5400.6
Device Model:     ST9500325AS
Serial Number:    --
LU WWN Device Id: 5 000c50 ...
Firmware Version: 0002SDM1
User Capacity:    500,107,862,016 bytes [500 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    5400 rpm
Device is:        In smartctl database 7.3/5528
ATA Version is:   ATA8-ACS T13/1699-D revision 4
SATA Version is:  SATA 2.6, 3.0 Gb/s
Local Time is:    Wed Jan 31 08:26:04 2024 EST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     128 (minimum power consumption without standby)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unknown

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(    0) seconds.
Offline data collection
capabilities: 			 (0x73) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 ( 139) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x103b)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   120   083   006    -    238538894
  3 Spin_Up_Time            PO----   099   099   000    -    0
  4 Start_Stop_Count        -O--CK+  098   098   020    -    2316
  5 Reallocated_Sector_Ct   PO--CK   092   092   036    -    178
  7 Seek_Error_Rate         POSR--   081   060   030    -    153353272
  9 Power_On_Hours          -O--CK   094   094   000    -    5587
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   099   037   020    -    1972
184 End-to-End_Error        -O--CK   100   100   099    -    0
187 Reported_Uncorrect      -O--CK   001   001   000    -    11998
188 Command_Timeout         -O--CK   100   091   000    -    42950328994
189 High_Fly_Writes         -O-RCK   100   100   000    -    0
190 Airflow_Temperature_Cel -O---K   066   053   045    -    34 (Min/Max 18/34)
191 G-Sense_Error_Rate      -O--CK   100   100   000    -    59
192 Power-Off_Retract_Count -O--CK   100   100   000    -    275
193 Load_Cycle_Count        -O--CK   045   045   000    -    111126
194 Temperature_Celsius     -O---K   034   047   000    -    34 (0 10 0 0 0)
195 Hardware_ECC_Recovered  -O-RC-   048   040   000    -    238538894
197 Current_Pending_Sector  -O--C-   100   100   000    -    0
198 Offline_Uncorrectable   ----C-   100   100   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    0
254 Free_Fall_Sensor        -O--CK   100   100   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01       GPL,SL  R/O      1  Summary SMART error log
0x02       GPL,SL  R/O      5  Comprehensive SMART error log
0x03       GPL,SL  R/O      5  Ext. Comprehensive SMART error log
0x06       GPL,SL  R/O      1  SMART self-test log
0x07       GPL,SL  R/O      1  Extended self-test log
0x09       GPL,SL  R/W      1  Selective self-test log
0x10       GPL,SL  R/O      1  NCQ Command Error log
0x11       GPL,SL  R/O      1  SATA Phy Event Counters log
0x21       GPL,SL  R/O      1  Write stream error log
0x22       GPL,SL  R/O      1  Read stream error log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS      20  Device vendor specific log
0xa2       GPL     VS    2248  Device vendor specific log
0xa8       GPL,SL  VS      65  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xb0       GPL     VS    2864  Device vendor specific log
0xbe-0xbf  GPL     VS   65535  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 11473 (device log contains only the most recent 20 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 11473 [12] occurred at disk power-on lifetime: 4214 hours (175 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 8f de 87 00 00  Error: UNC at LBA = 0x008fde87 = 9428615

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 00 00 8f de 80 40 00     00:29:34.204  READ FPDMA QUEUED
  60 00 00 00 40 00 00 00 40 e7 fa 40 00     00:29:32.033  READ FPDMA QUEUED
  61 00 00 00 38 00 00 00 5c c0 c0 40 00     00:29:32.033  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 00 5c 7e 18 40 00     00:29:32.033  WRITE FPDMA QUEUED
  60 00 00 00 1d 00 00 00 3a bc 80 40 00     00:29:32.032  READ FPDMA QUEUED

Error 11472 [11] occurred at disk power-on lifetime: 4214 hours (175 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 8f de 87 00 00  Error: UNC at LBA = 0x008fde87 = 9428615

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 20 00 00 00 13 c6 12 40 00     00:29:11.403  READ FPDMA QUEUED
  60 00 00 00 08 00 00 00 0b 13 30 40 00     00:29:11.403  READ FPDMA QUEUED
  60 00 00 00 08 00 00 00 62 96 50 40 00     00:29:11.401  READ FPDMA QUEUED
  60 00 00 00 40 00 00 00 13 be 3a 40 00     00:29:11.400  READ FPDMA QUEUED
  61 00 00 00 08 00 00 00 52 82 80 40 00     00:29:11.400  WRITE FPDMA QUEUED

Error 11471 [10] occurred at disk power-on lifetime: 4214 hours (175 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 52 83 fc 00 00  Error: UNC at LBA = 0x005283fc = 5407740

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 10 00 00 00 7e 90 2a 40 00     00:26:55.645  READ FPDMA QUEUED
  61 00 00 00 08 00 00 00 82 ec e0 40 00     00:26:55.645  WRITE FPDMA QUEUED
  60 00 00 00 80 00 00 00 52 83 88 40 00     00:26:55.644  READ FPDMA QUEUED
  61 00 00 00 38 00 00 00 34 aa 18 40 00     00:26:55.644  WRITE FPDMA QUEUED
  60 00 00 00 08 00 00 00 52 83 80 40 00     00:26:53.953  READ FPDMA QUEUED

Error 11470 [9] occurred at disk power-on lifetime: 3345 hours (139 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 15 8f 7a f7 00 00  Error: WP at LBA = 0x158f7af7 = 361724663

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 48 00 00 02 34 97 50 40 00     02:55:25.759  WRITE FPDMA QUEUED
  60 00 00 00 20 00 00 15 f8 f3 d7 40 00     02:55:25.758  READ FPDMA QUEUED
  61 00 00 00 48 00 00 02 32 56 e8 40 00     02:55:25.757  WRITE FPDMA QUEUED
  61 00 00 01 00 00 00 1d 05 a7 37 40 00     02:55:25.755  WRITE FPDMA QUEUED
  61 00 00 01 00 00 00 1d 05 a6 37 40 00     02:55:25.754  WRITE FPDMA QUEUED

Error 11469 [8] occurred at disk power-on lifetime: 3345 hours (139 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 15 8f 7a f7 00 00  Error: UNC at LBA = 0x158f7af7 = 361724663

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 20 00 00 01 e3 6f d8 40 00     02:55:23.355  READ FPDMA QUEUED
  61 00 00 01 00 00 00 1d 05 9f 37 40 00     02:55:23.355  WRITE FPDMA QUEUED
  61 00 00 01 00 00 00 1d 05 9e 37 40 00     02:55:23.354  WRITE FPDMA QUEUED
  61 00 00 01 00 00 00 1d 05 9d 37 40 00     02:55:23.354  WRITE FPDMA QUEUED
  61 00 00 01 00 00 00 1d 05 9c 37 40 00     02:55:23.353  WRITE FPDMA QUEUED

Error 11468 [7] occurred at disk power-on lifetime: 3345 hours (139 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 15 8f 7a f7 00 00  Error: WP at LBA = 0x158f7af7 = 361724663

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 01 00 00 00 1d 05 87 37 40 00     02:55:20.914  WRITE FPDMA QUEUED
  61 00 00 01 00 00 00 1d 05 86 37 40 00     02:55:20.914  WRITE FPDMA QUEUED
  61 00 00 01 00 00 00 1d 05 85 37 40 00     02:55:20.913  WRITE FPDMA QUEUED
  61 00 00 01 00 00 00 1d 05 84 37 40 00     02:55:20.913  WRITE FPDMA QUEUED
  61 00 00 01 00 00 00 1d 05 83 37 40 00     02:55:20.911  WRITE FPDMA QUEUED

Error 11467 [6] occurred at disk power-on lifetime: 3345 hours (139 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 15 8f 7a f7 00 00  Error: WP at LBA = 0x158f7af7 = 361724663

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 01 00 00 00 19 4c 62 b7 40 00     02:55:18.339  WRITE FPDMA QUEUED
  61 00 00 01 00 00 00 19 4c 61 b7 40 00     02:55:18.339  WRITE FPDMA QUEUED
  61 00 00 01 00 00 00 19 4c 60 b7 40 00     02:55:18.339  WRITE FPDMA QUEUED
  61 00 00 01 00 00 00 19 4c 5f b7 40 00     02:55:18.338  WRITE FPDMA QUEUED
  61 00 00 01 00 00 00 19 4c 5e b7 40 00     02:55:18.338  WRITE FPDMA QUEUED

Error 11466 [5] occurred at disk power-on lifetime: 3345 hours (139 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 15 8f 7a f7 00 00  Error: WP at LBA = 0x158f7af7 = 361724663

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 20 00 00 1c be 44 d7 40 00     02:55:15.399  WRITE FPDMA QUEUED
  61 00 00 01 00 00 00 19 4b 88 ef 40 00     02:55:15.397  WRITE FPDMA QUEUED
  61 00 00 01 00 00 00 19 4b 87 ef 40 00     02:55:15.395  WRITE FPDMA QUEUED
  61 00 00 01 00 00 00 19 4b 86 ef 40 00     02:55:15.394  WRITE FPDMA QUEUED
  61 00 00 01 00 00 00 19 4b 85 ef 40 00     02:55:15.394  WRITE FPDMA QUEUED

SMART Extended Self-test Log Version: 1 (1 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       522 (0x020a)
Device State:                        Active (0)
Current Temperature:                    34 Celsius
Power Cycle Min/Max Temperature:     18/34 Celsius
Lifetime    Min/Max Temperature:     10/47 Celsius
Under/Over Temperature Limit Count:   0/53

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      0/ 0 Celsius
Min/Max Temperature Limit:            0/ 0 Celsius
Temperature History Size (Index):    128 (25)

SCT Error Recovery Control:
           Read: Disabled
          Write: Disabled

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2            4  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS

