smartctl 7.3 2022-02-28 r5338 [OpenBSD 7.2 amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Intel 730 and DC S35x0/3610/3700 Series SSDs
Device Model:     INTEL SSDSC2BB120G4
Serial Number:    --
LU WWN Device Id: 5 5cd2e4 ...
Firmware Version: D2012370
User Capacity:    120,034,123,776 bytes [120 GB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Rotation Rate:    Solid State Device
Form Factor:      2.5 inches
TRIM Command:     Available, deterministic, zeroed
Device is:        In smartctl database 7.3/5319
ATA Version is:   ACS-2 T13/2015-D revision 3
SATA Version is:  SATA 2.6, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Fri Jan 20 11:35:10 2023 CET
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x02)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(    2) seconds.
Offline data collection
capabilities: 			 (0x79) SMART execute Offline immediate.
					No Auto Offline data collection support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (   2) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x003d)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 1
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  5 Reallocated_Sector_Ct   0x0032   100   100   000    Old_age   Always       -       0
  9 Power_On_Hours          0x0032   100   100   000    Old_age   Always       -       36845
 12 Power_Cycle_Count       0x0032   100   100   000    Old_age   Always       -       155
170 Available_Reservd_Space 0x0033   100   100   010    Pre-fail  Always       -       0
171 Program_Fail_Count      0x0032   100   100   000    Old_age   Always       -       0
172 Erase_Fail_Count        0x0032   100   100   000    Old_age   Always       -       0
174 Unsafe_Shutdown_Count   0x0032   100   100   000    Old_age   Always       -       121
175 Power_Loss_Cap_Test     0x0033   100   100   010    Pre-fail  Always       -       638 (200 62)
183 SATA_Downshift_Count    0x0032   100   100   000    Old_age   Always       -       0
184 End-to-End_Error        0x0033   100   100   090    Pre-fail  Always       -       0
187 Reported_Uncorrect      0x0032   100   100   000    Old_age   Always       -       0
190 Temperature_Case        0x0022   082   082   000    Old_age   Always       -       18 (Min/Max 11/18)
192 Unsafe_Shutdown_Count   0x0032   100   100   000    Old_age   Always       -       121
194 Temperature_Internal    0x0022   100   100   000    Old_age   Always       -       25
197 Current_Pending_Sector  0x0032   100   100   000    Old_age   Always       -       0
199 CRC_Error_Count         0x003e   100   100   000    Old_age   Always       -       0
225 Host_Writes_32MiB       0x0032   100   100   000    Old_age   Always       -       5153478
226 Workld_Media_Wear_Indic 0x0032   100   100   000    Old_age   Always       -       56627
227 Workld_Host_Reads_Perc  0x0032   100   100   000    Old_age   Always       -       5
228 Workload_Minutes        0x0032   100   100   000    Old_age   Always       -       2209947
232 Available_Reservd_Space 0x0033   100   100   010    Pre-fail  Always       -       0
233 Media_Wearout_Indicator 0x0032   045   045   000    Old_age   Always       -       0
234 Thermal_Throttle        0x0032   100   100   000    Old_age   Always       -       0/0
241 Host_Writes_32MiB       0x0032   100   100   000    Old_age   Always       -       5153478
242 Host_Reads_32MiB        0x0032   100   100   000    Old_age   Always       -       287124

SMART Error Log Version: 1
No Errors Logged

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%     36798         -
# 2  Short offline       Completed without error       00%     36630         -
# 3  Short offline       Completed without error       00%     36463         -
# 4  Short offline       Completed without error       00%     36296         -
# 5  Short offline       Completed without error       00%     36129         -
# 6  Short offline       Completed without error       00%     35962         -
# 7  Short offline       Completed without error       00%     35794         -
# 8  Short offline       Completed without error       00%     35627         -
# 9  Short offline       Completed without error       00%     35460         -
#10  Short offline       Completed without error       00%     35293         -
#11  Short offline       Completed without error       00%     35127         -
#12  Short offline       Completed without error       00%     34959         -
#13  Short offline       Completed without error       00%     34792         -
#14  Short offline       Completed without error       00%     34625         -
#15  Short offline       Completed without error       00%     34458         -
#16  Short offline       Completed without error       00%     34291         -
#17  Short offline       Completed without error       00%     34124         -
#18  Short offline       Completed without error       00%     33956         -
#19  Short offline       Completed without error       00%     33789         -
#20  Short offline       Completed without error       00%     33622         -
#21  Short offline       Completed without error       00%     33455         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

