smartctl 7.2 2020-12-30 r5155 [FreeBSD 12.1-RELEASE-p19-HBSD amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Silicon Motion based SSDs
Device Model:     ADATA SU650
Serial Number:    --
LU WWN Device Id: 0 000000 ...
Firmware Version: V8X01c87
User Capacity:    120,034,123,776 bytes [120 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
Form Factor:      2.5 inches
TRIM Command:     Available, deterministic, zeroed
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ACS-3, ATA8-ACS T13/1699-D revision 6
SATA Version is:  SATA 3.1, 6.0 Gb/s (current: 3.0 Gb/s)
Local Time is:    Mon Aug  2 14:51:47 2021 CST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(    1) seconds.
Offline data collection
capabilities: 			 (0x59) SMART execute Offline immediate.
					No Auto Offline data collection support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0002)	Does not save SMART data before
					entering power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   3) minutes.
Extended self-test routine
recommended polling time: 	 (  11) minutes.
SCT capabilities: 	       (0x0039)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR-K   100   100   050    -    0
  5 Reallocated_Sector_Ct   PO--CK   100   100   010    -    3184
  9 Power_On_Hours          -O--CK   100   100   000    -    14977
 12 Power_Cycle_Count       -O--CK   100   100   000    -    119
161 Valid_Spare_Block_Cnt   -O--CK   100   100   000    -    138
162 Unknown_Attribute       -O--CK   100   100   000    -    126247
163 Initial_Bad_Block_Count -O--CK   100   100   000    -    100
164 Total_Erase_Count       -O--CK   100   100   000    -    89
166 Min_Erase_Count         -O--CK   100   100   000    -    153
167 Average_Erase_Count     -O--CK   100   100   050    -    0
168 Max_Erase_Count_of_Spec -O--CK   100   100   000    -    0
169 Remaining_Lifetime_Perc -O--CK   100   100   000    -    100
171 Unknown_Attribute       -O--CK   100   100   000    -    0
172 Unknown_Attribute       -O--CK   100   100   000    -    0
174 Unknown_Attribute       -O--CK   100   100   000    -    89
175 Program_Fail_Count_Chip -O--CK   100   100   000    -    49
181 Program_Fail_Cnt_Total  -O---K   100   100   000    -    5282428
187 Reported_Uncorrect      -O--CK   100   100   000    -    49
194 Temperature_Celsius     -O---K   100   100   030    -    52
195 Hardware_ECC_Recovered  -O-RCK   100   100   000    -    4311
196 Reallocated_Event_Count -O--CK   100   100   000    -    49
199 UDMA_CRC_Error_Count    -O--CK   100   100   000    -    49
206 Unknown_SSD_Attribute   -O--CK   100   100   000    -    7
207 Unknown_SSD_Attribute   -O--CK   100   100   000    -    109
232 Available_Reservd_Space -O--CK   100   100   000    -    83
233 Media_Wearout_Indicator -O--CK   100   100   000    -    721
241 Host_Writes_32MiB       -O--CK   100   100   000    -    3577
242 Host_Reads_32MiB        -O--CK   100   100   000    -    813
249 Unkn_SiliconMotion_Attr -O--CK   100   100   000    -    220
250 Read_Error_Retry_Rate   -O--CK   100   100   000    -    4101
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      1  Comprehensive SMART error log
0x03       GPL     R/O      2  Ext. Comprehensive SMART error log
0x04       GPL,SL  R/O      5  Device Statistics log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x30       GPL,SL  R/O      8  IDENTIFY DEVICE data log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (2 sectors)
Device Error Count: 15545 (device log contains only the most recent 8 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 15545 [7] occurred at disk power-on lifetime: 14967 hours (623 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 00 00 00 00 00  Error: UNC at LBA = 0x00000000 = 0

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 40 d0 0f f0 d0 0f e8 ea 00 22d+05:44:12.887  READ DMA
  c8 00 00 00 80 d0 0f f0 d0 0f a8 ea 00 22d+05:44:12.093  READ DMA
  c8 00 00 00 00 d0 0f f0 d0 0f 28 ea 00 22d+05:44:11.304  READ DMA
  c8 00 00 00 00 d0 0f f0 d0 0f 28 ea 00 22d+05:44:10.569  READ DMA
  c8 00 00 00 00 d0 0f f0 d0 0f 28 ea 00 22d+05:44:09.792  READ DMA

Error 15544 [6] occurred at disk power-on lifetime: 14967 hours (623 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 00 00 00 00 00  Error: UNC at LBA = 0x00000000 = 0

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 40 d0 0f f0 d0 0f e8 ea 00 22d+05:44:12.827  READ DMA
  c8 00 00 00 80 d0 0f f0 d0 0f a8 ea 00 22d+05:44:12.033  READ DMA
  c8 00 00 00 00 d0 0f f0 d0 0f 28 ea 00 22d+05:44:11.244  READ DMA
  c8 00 00 00 00 d0 0f f0 d0 0f 28 ea 00 22d+05:44:10.509  READ DMA
  c8 00 00 00 00 d0 0f f0 d0 0f 28 ea 00 22d+05:44:09.732  READ DMA

Error 15543 [5] occurred at disk power-on lifetime: 14967 hours (623 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 00 00 00 00 00  Error: UNC at LBA = 0x00000000 = 0

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 40 d0 0f f0 d0 0f e8 ea 00 22d+05:44:12.768  READ DMA
  c8 00 00 00 80 d0 0f f0 d0 0f a8 ea 00 22d+05:44:11.973  READ DMA
  c8 00 00 00 00 d0 0f f0 d0 0f 28 ea 00 22d+05:44:11.184  READ DMA
  c8 00 00 00 00 d0 0f f0 d0 0f 28 ea 00 22d+05:44:10.449  READ DMA
  c8 00 00 00 00 d0 0f f0 d0 0f 28 ea 00 22d+05:44:09.673  READ DMA

Error 15542 [4] occurred at disk power-on lifetime: 14967 hours (623 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 00 00 00 00 00  Error: UNC at LBA = 0x00000000 = 0

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 40 d0 0f f0 d0 0f e8 ea 00 22d+05:44:12.709  READ DMA
  c8 00 00 00 80 d0 0f f0 d0 0f a8 ea 00 22d+05:44:11.914  READ DMA
  c8 00 00 00 00 d0 0f f0 d0 0f 28 ea 00 22d+05:44:11.124  READ DMA
  c8 00 00 00 00 d0 0f f0 d0 0f 28 ea 00 22d+05:44:10.389  READ DMA
  c8 00 00 00 00 d0 0f f0 d0 0f 28 ea 00 22d+05:44:09.613  READ DMA

Error 15541 [3] occurred at disk power-on lifetime: 14967 hours (623 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 00 00 00 00 00  Error: UNC at LBA = 0x00000000 = 0

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 40 7d 04 3f d0 0f e8 ea 00 22d+05:44:12.649  READ DMA
  c8 00 00 00 40 d0 0f f0 7d 04 68 ea 00 22d+05:44:12.509  READ DMA
  c8 00 00 00 80 d0 0f 3f d0 0f a8 ea 00 22d+05:44:11.854  READ DMA
  c8 00 00 00 40 d0 0f f0 d0 0f 68 ea 00 22d+05:44:11.800  READ DMA
  c8 00 00 00 00 79 92 3f d0 0f 28 ea 00 22d+05:44:11.064  READ DMA

Error 15540 [2] occurred at disk power-on lifetime: 14967 hours (623 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 00 00 00 00 00  Error: UNC at LBA = 0x00000000 = 0

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 40 d0 0f f0 d0 0f e8 ea 00 22d+05:44:12.495  READ DMA
  c8 00 00 00 c0 d0 0f f0 d0 0f 68 ea 00 22d+05:44:11.669  READ DMA
  c8 00 00 00 00 d0 0f f0 d0 0f 28 ea 00 22d+05:44:10.931  READ DMA
  c8 00 00 00 00 d0 0f f0 d0 0f 28 ea 00 22d+05:44:10.205  READ DMA
  c8 00 00 00 00 d0 0f f0 d0 0f 28 ea 00 22d+05:44:09.409  READ DMA

Error 15539 [1] occurred at disk power-on lifetime: 14967 hours (623 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 00 00 00 00 00  Error: UNC at LBA = 0x00000000 = 0

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 40 d0 0f f0 d0 0f e8 ea 00 22d+05:44:12.435  READ DMA
  c8 00 00 00 c0 d0 0f f0 d0 0f 68 ea 00 22d+05:44:11.609  READ DMA
  c8 00 00 00 00 d0 0f f0 d0 0f 28 ea 00 22d+05:44:10.871  READ DMA
  c8 00 00 00 00 d0 0f f0 d0 0f 28 ea 00 22d+05:44:10.142  READ DMA
  c8 00 00 00 00 d0 0f f0 d0 0f 28 ea 00 22d+05:44:09.350  READ DMA

Error 15538 [0] occurred at disk power-on lifetime: 14967 hours (623 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 00 00 00 00 00  Error: UNC at LBA = 0x00000000 = 0

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 40 d0 0f f0 d0 0f e8 ea 00 22d+05:44:12.376  READ DMA
  c8 00 00 00 c0 d0 0f f0 d0 0f 68 ea 00 22d+05:44:11.550  READ DMA
  c8 00 00 00 00 d0 0f f0 d0 0f 28 ea 00 22d+05:44:10.811  READ DMA
  c8 00 00 00 00 d0 0f f0 d0 0f 28 ea 00 22d+05:44:10.076  READ DMA
  c8 00 00 00 00 d0 0f f0 d0 0f 28 ea 00 22d+05:44:09.290  READ DMA

SMART Extended Self-test Log Version: 1 (1 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 0
Note: revision number not 1 implies that no selective self-test has ever been run
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       0 (0x0000)
Device State:                        Active (0)
Current Temperature:                     0 Celsius
Power Cycle Min/Max Temperature:     28/28 Celsius
Lifetime    Min/Max Temperature:      0/36 Celsius
Specified Max Operating Temperature:   100 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Temperature History Version:     2
Temperature Sampling Period:         0 minutes
Temperature Logging Interval:        0 minutes
Min/Max recommended Temperature:      0/100 Celsius
Min/Max Temperature Limit:           -10/125 Celsius
Temperature History Size (Index):    128 (1)

SCT Error Recovery Control:
           Read: Disabled
          Write: Disabled

Device Statistics (GP Log 0x04)
Page  Offset Size        Value Flags Description
0x01  =====  =               =  ===  == General Statistics (rev 1) ==
0x01  0x008  4             119  ---  Lifetime Power-On Resets
0x01  0x010  4           14977  ---  Power-on Hours
0x01  0x018  6      7501688966  ---  Logical Sectors Written
0x01  0x020  6       100376461  ---  Number of Write Commands
0x01  0x028  6      1705867405  ---  Logical Sectors Read
0x01  0x030  6        55144531  ---  Number of Read Commands
0x01  0x038  6     53918343630  ---  Date and Time TimeStamp
0x04  =====  =               =  ===  == General Errors Statistics (rev 1) ==
0x04  0x008  4           15545  ---  Number of Reported Uncorrectable Errors
0x04  0x010  4               0  ---  Resets Between Cmd Acceptance and Completion
0x06  =====  =               =  ===  == Transport Statistics (rev 1) ==
0x06  0x008  4             581  ---  Number of Hardware Resets
0x06  0x018  4               0  ---  Number of Interface CRC Errors
0x07  =====  =               =  ===  == Solid State Device Statistics (rev 1) ==
0x07  0x008  1              86  ---  Percentage Used Endurance Indicator
                                |||_ C monitored condition met
                                ||__ D supports DSN
                                |___ N normalized value

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  4            0  Command failed due to ICRC error
0x000a  4           66  Device-to-host register FISes sent due to a COMRESET

