smartctl 7.4 2023-08-01 r5530 [FreeBSD 13.2-RELEASE-p3 amd64] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Number:                       SAMSUNG MZVLW512HMJP-000L7
Serial Number:                      --
Firmware Version:                   6L7QCXY7
PCI Vendor/Subsystem ID:            0x144d
IEEE OUI Identifier:                0x002538
Total NVM Capacity:                 512,110,190,592 [512 GB]
Unallocated NVM Capacity:           0
Controller ID:                      2
NVMe Version:                       1.2
Number of Namespaces:               1
Namespace 1 Size/Capacity:          512,110,190,592 [512 GB]
Namespace 1 Utilization:            121,469,755,392 [121 GB]
Namespace 1 Formatted LBA Size:     512
Namespace 1 IEEE EUI-64:            002538 ...
Local Time is:                      Wed Nov  8 13:51:49 2023 CET
Firmware Updates (0x16):            3 Slots, no Reset required
Optional Admin Commands (0x0017):   Security Format Frmw_DL Self_Test
Optional NVM Commands (0x001f):     Comp Wr_Unc DS_Mngmt Wr_Zero Sav/Sel_Feat
Log Page Attributes (0x03):         S/H_per_NS Cmd_Eff_Lg
Warning  Comp. Temp. Threshold:     69 Celsius
Critical Comp. Temp. Threshold:     72 Celsius

Supported Power States
St Op     Max   Active     Idle   RL RT WL WT  Ent_Lat  Ex_Lat
 0 +     7.60W       -        -    0  0  0  0        0       0
 1 +     6.00W       -        -    1  1  1  1        0       0
 2 +     5.10W       -        -    2  2  2  2        0       0
 3 -   0.0400W       -        -    3  3  3  3      210    1500
 4 -   0.0050W       -        -    4  4  4  4     2200    6000

Supported LBA Sizes (NSID 0x1)
Id Fmt  Data  Metadt  Rel_Perf
 0 +     512       0         0

=== START OF SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

SMART/Health Information (NVMe Log 0x02)
Critical Warning:                   0x00
Temperature:                        45 Celsius
Available Spare:                    100%
Available Spare Threshold:          10%
Percentage Used:                    8%
Data Units Read:                    100,265,012 [51.3 TB]
Data Units Written:                 125,359,145 [64.1 TB]
Host Read Commands:                 860,968,102
Host Write Commands:                1,141,586,135
Controller Busy Time:               9,589
Power Cycles:                       1,984
Power On Hours:                     7,593
Unsafe Shutdowns:                   756
Media and Data Integrity Errors:    0
Error Information Log Entries:      4,949
Warning  Comp. Temperature Time:    0
Critical Comp. Temperature Time:    0
Temperature Sensor 1:               45 Celsius
Temperature Sensor 2:               75 Celsius

Error Information (NVMe Log 0x01, 16 of 64 entries)
Num   ErrCount  SQId   CmdId  Status  PELoc          LBA  NSID    VS  Message
  0       4949     0  0x0018  0x4004  0x02c            0     0     -  Invalid Field in Command
  1       4948     0  0x0017  0x4004  0x02c            0     0     -  Invalid Field in Command
  2       4947     0  0x0015  0x4212  0x028            0     -     -  Invalid Log Page
  3       4946     0  0x0002  0x4004  0x028            0     0     -  Invalid Field in Command
  4       4945     0  0x0018  0x4004  0x02c            0     0     -  Invalid Field in Command
  5       4944     0  0x0017  0x4004  0x02c            0     0     -  Invalid Field in Command
  6       4943     0  0x0015  0x4212  0x028            0     -     -  Invalid Log Page
  7       4942     0  0x0002  0x4004  0x028            0     0     -  Invalid Field in Command
  8       4941     0  0x0018  0x4004  0x02c            0     0     -  Invalid Field in Command
  9       4940     0  0x0017  0x4004  0x02c            0     0     -  Invalid Field in Command
 10       4939     0  0x0015  0x4212  0x028            0     -     -  Invalid Log Page
 11       4938     0  0x0002  0x4004  0x028            0     0     -  Invalid Field in Command
 12       4937     0  0x0018  0x4004  0x02c            0     0     -  Invalid Field in Command
 13       4936     0  0x0017  0x4004  0x02c            0     0     -  Invalid Field in Command
 14       4935     0  0x0015  0x4212  0x028            0     -     -  Invalid Log Page
 15       4934     0  0x0002  0x4004  0x028            0     0     -  Invalid Field in Command
... (48 entries not read)

Self-test Log (NVMe Log 0x06)
Self-test status: Short self-test in progress (78% completed)
No Self-tests Logged

