smartctl 7.4 2023-08-01 r5530 [FreeBSD 14.1-RELEASE-p3 amd64] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Western Digital Red (SMR)
Device Model:     WDC WD40EFAX-68JH4N1
Serial Number:    --
LU WWN Device Id: 5 0014ee ...
Firmware Version: 83.00A83
User Capacity:    4,000,787,030,016 bytes [4.00 TB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Rotation Rate:    5400 rpm
Form Factor:      3.5 inches
TRIM Command:     Available, deterministic, zeroed
Device is:        In smartctl database 7.3/5528
ATA Version is:   ACS-3 T13/2161-D revision 5
SATA Version is:  SATA 3.1, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Sun Nov 24 11:32:48 2024 GMT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(46844) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 ( 504) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x3039)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR-K   200   200   051    -    0
  3 Spin_Up_Time            POS--K   202   202   021    -    2883
  4 Start_Stop_Count        -O--CK   100   100   000    -    59
  5 Reallocated_Sector_Ct   PO--CK   200   200   140    -    0
  7 Seek_Error_Rate         -OSR-K   200   200   000    -    0
  9 Power_On_Hours          -O--CK   056   056   000    -    32798
 10 Spin_Retry_Count        -O--CK   100   253   000    -    0
 11 Calibration_Retry_Count -O--CK   100   253   000    -    0
 12 Power_Cycle_Count       -O--CK   100   100   000    -    39
192 Power-Off_Retract_Count -O--CK   200   200   000    -    4
193 Load_Cycle_Count        -O--CK   200   200   000    -    86
194 Temperature_Celsius     -O---K   118   106   000    -    29
196 Reallocated_Event_Count -O--CK   200   200   000    -    0
197 Current_Pending_Sector  -O--CK   200   200   000    -    0
198 Offline_Uncorrectable   ----CK   100   253   000    -    0
199 UDMA_CRC_Error_Count    -O--CK   200   200   000    -    0
200 Multi_Zone_Error_Rate   ---R--   100   253   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      6  Ext. Comprehensive SMART error log
0x04       GPL     R/O    256  Device Statistics log
0x04       SL      R/O      8  Device Statistics log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x0c       GPL     R/O   2048  Pending Defects log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x24       GPL     R/O    294  Current Device Internal Status Data log
0x30       GPL,SL  R/O      9  IDENTIFY DEVICE data log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa0-0xa7  GPL,SL  VS      16  Device vendor specific log
0xa8-0xb6  GPL,SL  VS       1  Device vendor specific log
0xb7       GPL,SL  VS      78  Device vendor specific log
0xb9       GPL,SL  VS       4  Device vendor specific log
0xbd       GPL,SL  VS       1  Device vendor specific log
0xc0       GPL,SL  VS       1  Device vendor specific log
0xc1       GPL     VS      93  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (6 sectors)
Device Error Count: 14
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 14 [13] occurred at disk power-on lifetime: 24350 hours (1014 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 08 00 00 6c bb fc 48 e0 00  Error: IDNF 8 sectors at LBA = 0x6cbbfc48 = 1824259144

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  35 00 03 00 08 00 00 6c bb fc 48 e0 00 11d+14:38:55.985  WRITE DMA EXT
  35 00 03 00 08 00 00 6c bb fc 30 e0 00 11d+14:38:55.977  WRITE DMA EXT
  35 00 03 00 08 00 00 6c bb fc 18 e0 00 11d+14:38:55.975  WRITE DMA EXT
  35 00 03 00 10 00 00 6c bb fc 00 e0 00 11d+14:38:55.974  WRITE DMA EXT
  25 00 03 00 08 00 00 f0 ca 94 88 e0 00 11d+14:38:55.973  READ DMA EXT

Error 13 [12] occurred at disk power-on lifetime: 24350 hours (1014 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 10 00 00 6c ba 8f c8 e0 00  Error: IDNF 16 sectors at LBA = 0x6cba8fc8 = 1824165832

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  35 00 03 00 10 00 00 6c ba 8f c8 e0 00 11d+14:38:20.864  WRITE DMA EXT
  25 00 03 00 08 00 00 f0 ca 90 50 e0 00 11d+14:38:20.863  READ DMA EXT
  35 00 03 00 08 00 00 6c ba 8f b0 e0 00 11d+14:38:20.857  WRITE DMA EXT
  35 00 03 00 08 00 00 6c ba 8f 98 e0 00 11d+14:38:20.855  WRITE DMA EXT
  35 00 03 00 08 00 00 6c ba 8f 80 e0 00 11d+14:38:20.854  WRITE DMA EXT

Error 12 [11] occurred at disk power-on lifetime: 24350 hours (1014 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 08 00 00 6c b9 15 c8 e0 00  Error: IDNF 8 sectors at LBA = 0x6cb915c8 = 1824069064

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  35 00 03 00 08 00 00 6c b9 15 c8 e0 00 11d+14:37:49.616  WRITE DMA EXT
  35 00 03 00 08 00 00 6c b9 15 b0 e0 00 11d+14:37:49.615  WRITE DMA EXT
  35 00 03 00 08 00 00 6c b9 15 98 e0 00 11d+14:37:49.613  WRITE DMA EXT
  35 00 03 00 10 00 00 6c b9 15 80 e0 00 11d+14:37:49.602  WRITE DMA EXT
  35 00 03 00 08 00 00 6c b9 15 68 e0 00 11d+14:37:49.589  WRITE DMA EXT

Error 11 [10] occurred at disk power-on lifetime: 24350 hours (1014 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 08 00 00 6c b7 a3 00 e0 00  Error: IDNF 8 sectors at LBA = 0x6cb7a300 = 1823974144

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  35 00 03 00 08 00 00 6c b7 a3 00 e0 00 11d+14:37:05.250  WRITE DMA EXT
  35 00 03 00 08 00 00 6c b7 a2 e8 e0 00 11d+14:37:05.244  WRITE DMA EXT
  35 00 03 00 08 00 00 6c b7 a2 d0 e0 00 11d+14:37:05.243  WRITE DMA EXT
  35 00 03 00 10 00 00 6c b7 a2 b8 e0 00 11d+14:37:05.241  WRITE DMA EXT
  35 00 03 00 08 00 00 6c b7 a2 a0 e0 00 11d+14:37:05.238  WRITE DMA EXT

Error 10 [9] occurred at disk power-on lifetime: 24350 hours (1014 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 08 00 00 6c b6 66 68 e0 00  Error: IDNF 8 sectors at LBA = 0x6cb66668 = 1823893096

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  35 00 03 00 08 00 00 6c b6 66 68 e0 00 11d+14:36:35.822  WRITE DMA EXT
  35 00 03 00 08 00 00 6c b6 66 50 e0 00 11d+14:36:35.815  WRITE DMA EXT
  35 00 03 00 08 00 00 6c b6 66 38 e0 00 11d+14:36:35.813  WRITE DMA EXT
  35 00 03 00 10 00 00 6c b6 66 20 e0 00 11d+14:36:35.811  WRITE DMA EXT
  25 00 03 00 08 00 01 44 ab 31 d8 e0 00 11d+14:36:35.811  READ DMA EXT

Error 9 [8] occurred at disk power-on lifetime: 24350 hours (1014 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 58 00 00 9a dc 4b 90 e0 00  Error: IDNF 88 sectors at LBA = 0x9adc4b90 = 2598128528

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  35 00 03 00 58 00 00 9a dc 4b 90 e0 00 11d+14:32:41.308  WRITE DMA EXT
  35 00 03 00 08 00 00 6c ac d2 78 e0 00 11d+14:32:41.306  WRITE DMA EXT
  35 00 03 00 08 00 00 63 58 3d 58 e0 00 11d+14:32:41.300  WRITE DMA EXT
  35 00 03 03 20 00 00 10 be cb c0 e0 00 11d+14:32:41.297  WRITE DMA EXT
  35 00 03 01 40 00 00 85 9e c6 b0 e0 00 11d+14:32:41.294  WRITE DMA EXT

Error 8 [7] occurred at disk power-on lifetime: 24350 hours (1014 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 10 00 01 d1 c0 b4 10 e0 00  Error: IDNF 16 sectors at LBA = 0x1d1c0b410 = 7814034448

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  35 00 03 00 10 00 01 d1 c0 b4 10 e0 00 11d+14:32:18.213  WRITE DMA EXT
  35 00 03 00 10 00 00 00 00 0a 10 e0 00 11d+14:32:17.542  WRITE DMA EXT
  25 00 03 00 10 00 01 d1 c0 b6 10 e0 00 11d+14:32:16.830  READ DMA EXT
  25 00 03 00 10 00 01 d1 c0 b4 10 e0 00 11d+14:32:16.809  READ DMA EXT
  25 00 03 00 10 00 00 00 00 0a 10 e0 00 11d+14:32:16.797  READ DMA EXT

Error 7 [6] occurred at disk power-on lifetime: 24350 hours (1014 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 08 00 00 6c ab 90 a0 e0 00  Error: IDNF 8 sectors at LBA = 0x6cab90a0 = 1823183008

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  35 00 03 00 08 00 00 6c ab 90 a0 e0 00 11d+14:32:09.212  WRITE DMA EXT
  35 00 03 00 10 00 00 6c ab 90 88 e0 00 11d+14:32:09.207  WRITE DMA EXT
  25 00 03 00 08 00 01 1e ee 28 00 e0 00 11d+14:32:09.206  READ DMA EXT
  35 00 03 00 08 00 00 6c ab 90 70 e0 00 11d+14:32:09.205  WRITE DMA EXT
  35 00 03 00 08 00 00 6c ab 90 58 e0 00 11d+14:32:09.203  WRITE DMA EXT

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%      9711         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       258 (0x0102)
Device State:                        Active (0)
Current Temperature:                    29 Celsius
Power Cycle Min/Max Temperature:     23/34 Celsius
Lifetime    Min/Max Temperature:     15/41 Celsius
Under/Over Temperature Limit Count:   0/0
Vendor specific:
01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      0/65 Celsius
Min/Max Temperature Limit:           -41/85 Celsius
Temperature History Size (Index):    478 (451)

SCT Error Recovery Control:
           Read:     70 (7.0 seconds)
          Write:     70 (7.0 seconds)

Device Statistics (GP Log 0x04)
Page  Offset Size        Value Flags Description
0x01  =====  =               =  ===  == General Statistics (rev 1) ==
0x01  0x008  4              39  ---  Lifetime Power-On Resets
0x01  0x010  4           32798  ---  Power-on Hours
0x01  0x018  6    140549006038  ---  Logical Sectors Written
0x01  0x020  6      2454158366  ---  Number of Write Commands
0x01  0x028  6     54128282309  ---  Logical Sectors Read
0x01  0x030  6       660856513  ---  Number of Read Commands
0x01  0x038  6      2108683008  ---  Date and Time TimeStamp
0x03  =====  =               =  ===  == Rotating Media Statistics (rev 1) ==
0x03  0x008  4           32635  ---  Spindle Motor Power-on Hours
0x03  0x010  4           32568  ---  Head Flying Hours
0x03  0x018  4              91  ---  Head Load Events
0x03  0x020  4               0  ---  Number of Reallocated Logical Sectors
0x03  0x028  4               1  ---  Read Recovery Attempts
0x03  0x030  4               0  ---  Number of Mechanical Start Failures
0x03  0x038  4               0  ---  Number of Realloc. Candidate Logical Sectors
0x03  0x040  4               4  ---  Number of High Priority Unload Events
0x04  =====  =               =  ===  == General Errors Statistics (rev 1) ==
0x04  0x008  4              14  ---  Number of Reported Uncorrectable Errors
0x04  0x010  4               1  ---  Resets Between Cmd Acceptance and Completion
0x05  =====  =               =  ===  == Temperature Statistics (rev 1) ==
0x05  0x008  1              29  ---  Current Temperature
0x05  0x010  1              29  ---  Average Short Term Temperature
0x05  0x018  1              30  ---  Average Long Term Temperature
0x05  0x020  1              41  ---  Highest Temperature
0x05  0x028  1              21  ---  Lowest Temperature
0x05  0x030  1              40  ---  Highest Average Short Term Temperature
0x05  0x038  1              26  ---  Lowest Average Short Term Temperature
0x05  0x040  1              37  ---  Highest Average Long Term Temperature
0x05  0x048  1              27  ---  Lowest Average Long Term Temperature
0x05  0x050  4               0  ---  Time in Over-Temperature
0x05  0x058  1              65  ---  Specified Maximum Operating Temperature
0x05  0x060  4               0  ---  Time in Under-Temperature
0x05  0x068  1               0  ---  Specified Minimum Operating Temperature
0x06  =====  =               =  ===  == Transport Statistics (rev 1) ==
0x06  0x008  4             219  ---  Number of Hardware Resets
0x06  0x010  4             180  ---  Number of ASR Events
0x06  0x018  4               0  ---  Number of Interface CRC Errors
0xff  =====  =               =  ===  == Vendor Specific Statistics (rev 1) ==
0xff  0x008  7               0  ---  Vendor Specific
0xff  0x010  7               0  ---  Vendor Specific
0xff  0x018  7               0  ---  Vendor Specific
                                |||_ C monitored condition met
                                ||__ D supports DSN
                                |___ N normalized value

Pending Defects log (GP Log 0x0c)
No Defects Logged

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x0002  2            0  R_ERR response for data FIS
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0005  2            0  R_ERR response for non-data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x0008  2            0  Device-to-host non-data FIS retries
0x0009  2            4  Transition from drive PhyRdy to drive PhyNRdy
0x000a  2            5  Device-to-host register FISes sent due to a COMRESET
0x000b  2            0  CRC errors within host-to-device FIS
0x000d  2            0  Non-CRC errors within host-to-device FIS
0x000f  2            0  R_ERR response for host-to-device data FIS, CRC
0x0012  2            0  R_ERR response for host-to-device non-data FIS, CRC
0x8000  4      9833588  Vendor specific



