smartctl 7.4 2023-08-01 r5530 [FreeBSD 13.2-RELEASE-p4 amd64] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Laptop HDD
Device Model:     ST320LT012-1DG14C
Serial Number:    --
LU WWN Device Id: 5 000c50 ...
Firmware Version: 0001SDM1
User Capacity:    320,072,933,376 bytes [320 GB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Rotation Rate:    5400 rpm
Form Factor:      2.5 inches
Device is:        In smartctl database 7.3/5528
ATA Version is:   ATA8-ACS T13/1699-D revision 4
SATA Version is:  SATA 3.0, 6.0 Gb/s (current: 3.0 Gb/s)
Local Time is:    Sun Dec  3 04:02:56 2023 -04
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     128 (minimum power consumption without standby)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(    0) seconds.
Offline data collection
capabilities: 			 (0x73) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (  81) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x1035)	SCT Status supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   115   085   006    -    91376648
  3 Spin_Up_Time            PO----   099   099   000    -    0
  4 Start_Stop_Count        -O--CK   098   098   020    -    2152
  5 Reallocated_Sector_Ct   PO--CK   100   100   036    -    0
  7 Seek_Error_Rate         POSR--   063   060   030    -    120332523454
  9 Power_On_Hours          -O--CK   096   096   000    -    4026 (86 25 0)
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   099   099   020    -    1469
184 End-to-End_Error        -O--CK   100   100   099    -    0
187 Reported_Uncorrect      -O--CK   001   001   000    -    3224
188 Command_Timeout         -O--CK   100   099   000    -    8
189 High_Fly_Writes         -O-RCK   100   100   000    -    0
190 Airflow_Temperature_Cel -O---K   071   050   045    -    29 (Min/Max 29/29)
191 G-Sense_Error_Rate      -O--CK   100   100   000    -    749
192 Power-Off_Retract_Count -O--CK   100   100   000    -    275
193 Load_Cycle_Count        -O--CK   073   073   000    -    55061
194 Temperature_Celsius     -O---K   029   050   000    -    29 (0 22 0 0 0)
197 Current_Pending_Sector  -O--C-   100   099   000    -    0
198 Offline_Uncorrectable   ----C-   100   099   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    0
240 Head_Flying_Hours       ------   097   097   000    -    3341 (20 49 0)
241 Total_LBAs_Written      ------   100   253   000    -    7518725224
242 Total_LBAs_Read         ------   100   253   000    -    11546483427
254 Free_Fall_Sensor        -O--CK   100   100   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      5  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x21       GPL     R/O      1  Write stream error log
0x22       GPL     R/O      1  Read stream error log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS      20  Device vendor specific log
0xa2       GPL     VS    2248  Device vendor specific log
0xa8       GPL,SL  VS      65  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xab       GPL     VS       1  Device vendor specific log
0xb0       GPL     VS    2864  Device vendor specific log
0xbd-0xbf  GPL     VS   65535  Device vendor specific log
0xc0       GPL,SL  VS       1  Device vendor specific log
0xc1       GPL,SL  VS      10  Device vendor specific log
0xc3       GPL,SL  VS       8  Device vendor specific log
0xc4       GPL,SL  VS      18  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 3247 (device log contains only the most recent 20 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 3247 [6] occurred at disk power-on lifetime: 3791 hours (157 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 02 21 62 00 00 00  Error: UNC at LBA = 0x02216200 = 35742208

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 01 00 00 00 02 21 61 88 e0 00     00:02:04.198  READ DMA EXT
  25 00 00 01 00 00 00 02 21 60 88 e0 00     00:02:04.196  READ DMA EXT
  25 00 00 00 08 00 00 02 21 60 08 e0 00     00:02:04.196  READ DMA EXT
  35 00 00 00 01 00 00 01 f9 0e 8e e0 00     00:02:04.195  WRITE DMA EXT
  25 00 00 00 40 00 00 01 e0 b3 70 e0 00     00:02:04.195  READ DMA EXT

Error 3246 [5] occurred at disk power-on lifetime: 3791 hours (157 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 02 21 62 00 00 00  Error: UNC at LBA = 0x02216200 = 35742208

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 01 00 00 00 02 21 5f 88 e0 00     00:02:01.085  READ DMA EXT
  25 00 00 01 00 00 00 02 21 5e 88 e0 00     00:02:01.081  READ DMA EXT
  25 00 00 00 08 00 00 02 21 5e 48 e0 00     00:02:01.080  READ DMA EXT
  25 00 00 00 08 00 00 01 e0 b2 e0 e0 00     00:02:01.080  READ DMA EXT
  35 00 00 01 00 00 00 00 4c f2 c0 e0 00     00:02:01.079  WRITE DMA EXT

Error 3245 [4] occurred at disk power-on lifetime: 3791 hours (157 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 02 21 62 00 00 00  Error: UNC at LBA = 0x02216200 = 35742208

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 01 00 00 00 02 21 61 10 e0 00     00:01:57.558  READ DMA EXT
  25 00 00 01 00 00 00 02 21 60 10 e0 00     00:01:57.535  READ DMA EXT
  25 00 00 01 00 00 00 02 21 5f 10 e0 00     00:01:57.513  READ DMA EXT
  25 00 00 01 00 00 00 02 21 5e 10 e0 00     00:01:57.489  READ DMA EXT
  25 00 00 01 00 00 00 02 21 5d 10 e0 00     00:01:57.465  READ DMA EXT

Error 3244 [3] occurred at disk power-on lifetime: 3791 hours (157 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 02 21 62 00 00 00  Error: UNC at LBA = 0x02216200 = 35742208

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 01 00 00 00 02 21 5e 10 e0 00     00:01:54.204  READ DMA EXT
  25 00 00 01 00 00 00 02 21 5d 10 e0 00     00:01:54.198  READ DMA EXT
  25 00 00 00 08 00 00 01 e0 b1 d8 e0 00     00:01:54.197  READ DMA EXT
  25 00 00 01 00 00 00 01 8c 66 a8 e0 00     00:01:54.194  READ DMA EXT
  25 00 00 01 00 00 00 01 8c 65 a8 e0 00     00:01:54.182  READ DMA EXT

Error 3243 [2] occurred at disk power-on lifetime: 3791 hours (157 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 02 21 62 00 00 00  Error: UNC at LBA = 0x02216200 = 35742208

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 01 00 00 00 02 21 5e 10 e0 00     00:01:51.053  READ DMA EXT
  25 00 00 01 00 00 00 02 21 5d 10 e0 00     00:01:51.046  READ DMA EXT
  25 00 00 01 00 00 00 01 8c 65 88 e0 00     00:01:51.041  READ DMA EXT
  25 00 00 01 00 00 00 01 8c 64 88 e0 00     00:01:51.025  READ DMA EXT
  25 00 00 00 40 00 00 01 28 2b 48 e0 00     00:01:51.015  READ DMA EXT

Error 3242 [1] occurred at disk power-on lifetime: 3791 hours (157 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 02 21 62 00 00 00  Error: UNC at LBA = 0x02216200 = 35742208

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 01 00 00 00 02 21 61 10 e0 00     00:01:47.864  READ DMA EXT
  25 00 00 01 00 00 00 02 21 60 10 e0 00     00:01:47.864  READ DMA EXT
  25 00 00 01 00 00 00 02 21 5f 10 e0 00     00:01:47.858  READ DMA EXT
  25 00 00 01 00 00 00 02 21 5e 10 e0 00     00:01:47.836  READ DMA EXT
  25 00 00 01 00 00 00 02 21 5d 10 e0 00     00:01:47.816  READ DMA EXT

Error 3241 [0] occurred at disk power-on lifetime: 3791 hours (157 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 02 21 62 00 00 00  Error: UNC at LBA = 0x02216200 = 35742208

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 01 00 00 00 02 21 5e 10 e0 00     00:01:44.662  READ DMA EXT
  25 00 00 01 00 00 00 02 21 5d 10 e0 00     00:01:44.652  READ DMA EXT
  25 00 00 00 98 00 00 01 fb 19 88 e0 00     00:01:44.651  READ DMA EXT
  25 00 00 00 08 00 00 01 fb 19 48 e0 00     00:01:44.645  READ DMA EXT
  25 00 00 00 a8 00 00 01 8c 67 88 e0 00     00:01:44.643  READ DMA EXT

Error 3240 [19] occurred at disk power-on lifetime: 3791 hours (157 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 02 21 62 00 00 00  Error: UNC at LBA = 0x02216200 = 35742208

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 01 00 00 00 02 21 61 10 e0 00     00:01:41.136  READ DMA EXT
  25 00 00 01 00 00 00 02 21 60 10 e0 00     00:01:41.136  READ DMA EXT
  25 00 00 01 00 00 00 02 21 5f 10 e0 00     00:01:40.957  READ DMA EXT
  25 00 00 01 00 00 00 02 21 5e 10 e0 00     00:01:40.924  READ DMA EXT
  25 00 00 01 00 00 00 02 21 5d 10 e0 00     00:01:40.907  READ DMA EXT

SMART Extended Self-test Log Version: 1 (1 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       522 (0x020a)
Device State:                        Active (0)
Current Temperature:                    29 Celsius
Power Cycle Min/Max Temperature:     29/29 Celsius
Lifetime    Min/Max Temperature:     21/50 Celsius
Specified Max Operating Temperature:    39 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        30 minutes
Min/Max recommended Temperature:     14/55 Celsius
Min/Max Temperature Limit:           10/60 Celsius
Temperature History Size (Index):    128 (87)

SCT Error Recovery Control command not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2            4  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS

