smartctl 7.2 2020-12-30 r5155 [FreeBSD 12.2-STABLE amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Hitachi Ultrastar A7K1000
Device Model:     HUA721010KLA330
Serial Number:    --
Firmware Version: GKAOA94A
User Capacity:    1,000,204,886,016 bytes [1.00 TB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA/ATAPI-7 T13/1532D revision 1
Local Time is:    Sat Mar  6 04:47:43 2021 UTC
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM level is:     254 (maximum performance), recommended: 128
APM feature is:   Disabled
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x84)	Offline data collection activity
					was suspended by an interrupting command from host.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(15354) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 ( 255) minutes.
SCT capabilities: 	       (0x003f)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     PO-R--   100   100   016    -    0
  2 Throughput_Performance  P-S---   100   100   054    -    76
  3 Spin_Up_Time            POS---   102   102   024    -    683 (Average 680)
  4 Start_Stop_Count        -O--C-   100   100   000    -    1488
  5 Reallocated_Sector_Ct   PO--CK   100   100   005    -    0
  7 Seek_Error_Rate         PO-R--   100   100   067    -    0
  8 Seek_Time_Performance   P-S---   134   134   020    -    32
  9 Power_On_Hours          -O--C-   100   100   000    -    4813
 10 Spin_Retry_Count        PO--C-   100   100   060    -    0
 12 Power_Cycle_Count       -O--CK   100   100   000    -    1488
192 Power-Off_Retract_Count -O--CK   099   099   000    -    1488
193 Load_Cycle_Count        -O--C-   099   099   000    -    1488
194 Temperature_Celsius     -O----   130   130   000    -    46 (Min/Max 15/54)
196 Reallocated_Event_Count -O--CK   100   100   000    -    0
197 Current_Pending_Sector  -O---K   100   100   000    -    0
198 Offline_Uncorrectable   ---R--   100   100   000    -    0
199 UDMA_CRC_Error_Count    -O-R--   200   200   000    -    651
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x03       GPL     R/O      1  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x24       GPL     R/O     60  Current Device Internal Status Data log
0x80       GPL     R/W     60  Host vendor specific log
0x81-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (1 sectors)
Device Error Count: 12 (device log contains only the most recent 4 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 12 [3] occurred at disk power-on lifetime: 12743 hours (530 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 08 00 00 15 7c cc 77 45 00  Error: ICRC, ABRT at LBA = 0x157ccc77 = 360500343

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 68 00 80 00 00 15 7c cc 18 40 00 43d+16:41:39.848  READ FPDMA QUEUED
  60 00 08 00 80 00 00 15 80 cf 30 40 00 43d+16:41:39.848  READ FPDMA QUEUED
  60 00 08 00 80 00 00 15 7f 07 c8 40 00 43d+16:41:39.848  READ FPDMA QUEUED
  60 00 08 00 80 00 00 15 7f 07 c0 40 00 43d+16:41:39.848  READ FPDMA QUEUED
  60 00 08 00 80 00 00 15 7c 08 98 40 00 43d+16:41:39.848  READ FPDMA QUEUED

Error 11 [2] occurred at disk power-on lifetime: 12482 hours (520 days + 2 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 00 00 00 35 32 23 8f 45 00  Error: ICRC, ABRT at LBA = 0x3532238f = 892478351

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 08 00 80 00 00 35 32 23 88 40 00 32d+19:47:51.348  READ FPDMA QUEUED
  60 00 08 00 80 00 00 35 32 23 80 40 00 32d+19:47:51.348  READ FPDMA QUEUED
  60 00 08 00 80 00 00 35 30 08 90 40 00 32d+19:47:51.348  READ FPDMA QUEUED
  60 00 10 00 80 00 00 27 7a 42 90 40 00 32d+19:47:45.848  READ FPDMA QUEUED
  60 00 68 00 80 00 00 27 7a 42 28 40 00 32d+19:47:45.848  READ FPDMA QUEUED

Error 10 [1] occurred at disk power-on lifetime: 11803 hours (491 days + 19 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 03 10 00 00 63 65 32 8f 43 00  Error: ICRC, ABRT at LBA = 0x6365328f = 1667576463

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 04 00 00 80 00 00 63 65 31 a0 40 00  4d+12:28:21.148  READ FPDMA QUEUED
  60 00 10 00 80 00 00 6c 68 4f 58 40 00  4d+12:28:21.148  READ FPDMA QUEUED
  60 00 08 00 80 00 00 6c 68 c9 40 40 00  4d+12:28:21.148  READ FPDMA QUEUED
  60 00 08 00 80 00 00 6c 68 08 a8 40 00  4d+12:28:21.048  READ FPDMA QUEUED
  60 00 08 00 80 00 00 6c 69 ca f0 40 00  4d+12:28:21.048  READ FPDMA QUEUED

Error 9 [0] occurred at disk power-on lifetime: 11369 hours (473 days + 17 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 58 00 00 26 9f 01 c7 46 00  Error: ICRC, ABRT at LBA = 0x269f01c7 = 647954887

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 08 00 88 00 00 48 50 08 50 40 00 36d+04:28:11.644  READ FPDMA QUEUED
  60 00 68 00 80 00 00 26 9f 01 b8 40 00 36d+04:28:11.644  READ FPDMA QUEUED
  60 00 08 00 80 00 00 49 bb a1 30 40 00 36d+04:28:11.644  READ FPDMA QUEUED
  60 00 08 00 80 00 00 49 b8 0a a0 40 00 36d+04:28:11.644  READ FPDMA QUEUED
  60 00 08 00 88 00 00 26 9c d4 40 40 00 36d+04:28:11.644  READ FPDMA QUEUED

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%      3810         -
# 2  Short offline       Completed without error       00%      3806         -
# 3  Short offline       Completed without error       00%         0         -
# 4  Extended offline    Completed without error       00%     15110         -
# 5  Extended offline    Completed without error       00%     13646         -
# 6  Extended offline    Completed without error       00%     12182         -
# 7  Extended offline    Completed without error       00%     10722         -
# 8  Extended offline    Completed without error       00%      7310         -
# 9  Extended offline    Completed without error       00%      5846         -
#10  Extended offline    Completed without error       00%      4381         -
#11  Extended offline    Completed without error       00%      2917         -
#12  Extended offline    Completed without error       00%      1453         -
#13  Extended offline    Completed without error       00%     65525         -
#14  Extended offline    Completed without error       00%     64061         -
#15  Extended offline    Completed without error       00%     62597         -
#16  Extended offline    Completed without error       00%     61133         -
#17  Extended offline    Completed without error       00%     59668         -
#18  Extended offline    Completed without error       00%     58204         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  2
SCT Version (vendor specific):       256 (0x0100)
Device State:                        SMART Off-line Data Collection executing in background (4)
Current Temperature:                    46 Celsius
Power Cycle Min/Max Temperature:     --/49 Celsius
Lifetime    Min/Max Temperature:     --/54 Celsius

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      5/60 Celsius
Min/Max Temperature Limit:           -40/65 Celsius
Temperature History Size (Index):    128 (59)

SCT Error Recovery Control:
           Read:    250 (25.0 seconds)
          Write:    250 (25.0 seconds)

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x0009  2            2  Transition from drive PhyRdy to drive PhyNRdy
0x000a  2            2  Device-to-host register FISes sent due to a COMRESET
0x000b  2            0  CRC errors within host-to-device FIS
0x000d  2            0  Non-CRC errors within host-to-device FIS

