Innodisk Solid State Drives
===========================

This is a list of all tested Innodisk solid state drive models and their MTBFs. See
more info on reliability test in the [README](https://github.com/bsdhw/SMART).

Contents
--------

1. [ SSD by Model  ](#ssd-by-model)
2. [ SSD by Family ](#ssd-by-family)

SSD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| Innodisk  | DEMSR- 08GB mSA... | 8 GB   | 3       | 876   | 0     | 2.40   |
| Innodisk  | DEMSR- 16GB mSA... | 16 GB  | 6       | 492   | 0     | 1.35   |
| Innodisk  | Corp. - mSATA 3ME3 | 32 GB  | 3       | 215   | 0     | 0.59   |
| Innodisk  | DEM24-16GM41BC1... | 16 GB  | 2       | 202   | 0     | 0.55   |
| Innodisk  | DEMSR- 08GB mSA... | 8 GB   | 15      | 188   | 0     | 0.52   |
| Innodisk  | M.2 (S80) 3MG2-P   | 992 GB | 2       | 5     | 0     | 0.02   |

SSD by Family
-------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Family                 | Models | Samples | Days  | Err   | MTBF |
|-----------|------------------------|--------|---------|-------|-------|------|
| Innodisk  | 1IE3/3IE3/3ME3/3IE4... | 1      | 3       | 215   | 0     | 0.59   |
| Innodisk  | 3IE2/3ME2/3MG2/3SE2... | 1      | 2       | 5     | 0     | 0.02   |
