smartctl 7.3 2022-02-28 r5338 [FreeBSD 13.2-RELEASE amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Laptop HDD
Device Model:     ST500LT012-9WS142
Serial Number:    --
LU WWN Device Id: 5 000c50 ...
Firmware Version: 0001YAM1
User Capacity:    500,107,862,016 bytes [500 GB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Rotation Rate:    5400 rpm
Form Factor:      2.5 inches
Device is:        In smartctl database 7.3/5319
ATA Version is:   ATA8-ACS T13/1699-D revision 4
SATA Version is:  SATA 2.6, 3.0 Gb/s (current: 3.0 Gb/s)
Local Time is:    Sat Jun 10 08:21:14 2023 -03
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     128 (minimum power consumption without standby)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(    0) seconds.
Offline data collection
capabilities: 			 (0x53) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 ( 102) minutes.
SCT capabilities: 	       (0x103d)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR-K   114   092   006    -    74828760
  3 Spin_Up_Time            PO---K   099   099   000    -    0
  4 Start_Stop_Count        -O--CK   094   094   000    -    7115
  5 Reallocated_Sector_Ct   PO--CK   099   099   036    -    224
  7 Seek_Error_Rate         POSR-K   072   060   030    -    77563216120
  9 Power_On_Hours          -O--CK   092   092   000    -    7755
 10 Spin_Retry_Count        PO--CK   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   095   095   000    -    5789
183 Runtime_Bad_Block       -O--CK   100   100   000    -    0
184 End-to-End_Error        PO--CK   100   100   097    -    0
187 Reported_Uncorrect      -O--CK   001   001   000    -    1138
188 Command_Timeout         -O--CK   100   092   000    -    167506280510
189 High_Fly_Writes         -O-RCK   100   100   000    -    0
190 Airflow_Temperature_Cel -O---K   062   048   045    -    38 (Min/Max 38/40)
191 G-Sense_Error_Rate      -O--CK   100   100   000    -    1380
192 Power-Off_Retract_Count -O---K   100   100   000    -    924
193 Load_Cycle_Count        -O--CK   054   054   000    -    92129
194 Temperature_Celsius     -O---K   038   052   000    -    38 (0 12 0 0 0)
196 Reallocated_Event_Count -O--CK   099   099   000    -    224
197 Current_Pending_Sector  -O--CK   100   099   000    -    0
198 Offline_Uncorrectable   ----CK   100   100   000    -    0
199 UDMA_CRC_Error_Count    -O--CK   200   200   000    -    23
254 Free_Fall_Sensor        -O--CK   100   100   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      5  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x21       GPL     R/O      1  Write stream error log
0x22       GPL     R/O      1  Read stream error log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS      20  Device vendor specific log
0xa2       GPL     VS    2248  Device vendor specific log
0xa8       GPL,SL  VS      65  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xab       GPL     VS       1  Device vendor specific log
0xb0       GPL     VS    2864  Device vendor specific log
0xbd-0xbf  GPL     VS   65535  Device vendor specific log
0xc0       GPL,SL  VS       1  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 1135 (device log contains only the most recent 20 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 1135 [14] occurred at disk power-on lifetime: 6320 hours (263 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 02 05 79 10 00 00  Error: WP at LBA = 0x02057910 = 33913104

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 20 00 00 1d 28 dd 00 40 00     00:52:56.916  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 00 6b 76 10 40 00     00:52:56.916  WRITE FPDMA QUEUED
  60 00 00 00 08 00 00 02 05 79 10 40 00     00:52:56.916  READ FPDMA QUEUED
  61 00 00 00 40 00 00 00 6b dc 00 40 00     00:52:56.915  WRITE FPDMA QUEUED
  60 00 00 00 08 00 00 00 92 60 30 40 00     00:52:56.913  READ FPDMA QUEUED

Error 1134 [13] occurred at disk power-on lifetime: 6320 hours (263 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 02 05 79 10 00 00  Error: UNC at LBA = 0x02057910 = 33913104

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 00 00 37 ec 60 40 00     00:52:54.189  READ FPDMA QUEUED
  60 00 00 00 06 00 00 00 dc a4 30 40 00     00:52:54.189  READ FPDMA QUEUED
  60 00 00 00 20 00 00 00 51 e4 40 40 00     00:52:54.188  READ FPDMA QUEUED
  60 00 00 00 08 00 00 00 3b 49 ea 40 00     00:52:54.188  READ FPDMA QUEUED
  60 00 00 00 05 00 00 00 c9 b8 24 40 00     00:52:54.188  READ FPDMA QUEUED

Error 1133 [12] occurred at disk power-on lifetime: 6320 hours (263 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 02 05 79 10 00 00  Error: UNC at LBA = 0x02057910 = 33913104

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 00 00 3b 49 ea 40 00     00:52:51.447  READ FPDMA QUEUED
  60 00 00 00 20 00 00 00 51 e4 40 40 00     00:52:51.430  READ FPDMA QUEUED
  61 00 00 00 10 00 00 00 51 e3 68 40 00     00:52:51.429  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 00 51 e3 28 40 00     00:52:51.429  WRITE FPDMA QUEUED
  61 00 00 00 10 00 00 00 51 e3 00 40 00     00:52:51.428  WRITE FPDMA QUEUED

Error 1132 [11] occurred at disk power-on lifetime: 6320 hours (263 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 02 05 79 10 00 00  Error: WP at LBA = 0x02057910 = 33913104

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 18 00 00 00 51 de 38 40 00     00:52:48.661  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 00 51 de 20 40 00     00:52:48.644  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 00 51 dd 20 40 00     00:52:48.644  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 00 51 dc f0 40 00     00:52:48.643  WRITE FPDMA QUEUED
  61 00 00 00 10 00 00 00 51 dc b0 40 00     00:52:48.643  WRITE FPDMA QUEUED

Error 1131 [10] occurred at disk power-on lifetime: 6320 hours (263 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 02 05 79 10 00 00  Error: WP at LBA = 0x02057910 = 33913104

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 10 00 00 00 51 dc 40 40 00     00:52:45.899  WRITE FPDMA QUEUED
  60 00 00 00 08 00 00 00 b4 f3 f8 40 00     00:52:45.899  READ FPDMA QUEUED
  60 00 00 00 08 00 00 00 70 f1 b8 40 00     00:52:45.882  READ FPDMA QUEUED
  60 00 00 00 08 00 00 00 4d bb 00 40 00     00:52:45.880  READ FPDMA QUEUED
  61 00 00 00 08 00 00 00 6b 76 90 40 00     00:52:45.868  WRITE FPDMA QUEUED

Error 1130 [9] occurred at disk power-on lifetime: 6320 hours (263 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 02 05 79 10 00 00  Error: WP at LBA = 0x02057910 = 33913104

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 18 00 00 00 3f 0d 90 40 00     00:52:43.091  WRITE FPDMA QUEUED
  61 00 00 00 10 00 00 00 3f 0d 70 40 00     00:52:43.091  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 00 3f 0d 60 40 00     00:52:43.090  WRITE FPDMA QUEUED
  61 00 00 00 10 00 00 00 3f 0d 30 40 00     00:52:43.090  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 00 3f 0d 20 40 00     00:52:43.090  WRITE FPDMA QUEUED

Error 1129 [8] occurred at disk power-on lifetime: 6320 hours (263 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 02 05 79 10 00 00  Error: UNC at LBA = 0x02057910 = 33913104

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 01 00 00 00 02 05 7b 10 40 00     00:52:40.238  READ FPDMA QUEUED
  61 00 00 00 08 00 00 00 3f 0c 70 40 00     00:52:40.238  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 00 6b 76 10 40 00     00:52:40.238  WRITE FPDMA QUEUED
  60 00 00 01 00 00 00 02 05 7a 10 40 00     00:52:40.238  READ FPDMA QUEUED
  60 00 00 01 00 00 00 02 05 79 10 40 00     00:52:40.238  READ FPDMA QUEUED

Error 1128 [7] occurred at disk power-on lifetime: 6320 hours (263 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 02 05 79 10 00 00  Error: WP at LBA = 0x02057910 = 33913104

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 20 00 00 00 3f 0b d8 40 00     00:52:37.533  WRITE FPDMA QUEUED
  60 00 00 00 08 00 00 01 87 25 00 40 00     00:52:37.514  READ FPDMA QUEUED
  61 00 00 00 08 00 00 00 3f 0b c8 40 00     00:52:37.513  WRITE FPDMA QUEUED
  60 00 00 00 20 00 00 00 b3 b7 65 40 00     00:52:37.513  READ FPDMA QUEUED
  61 00 00 00 20 00 00 00 3f 0b a0 40 00     00:52:37.513  WRITE FPDMA QUEUED

SMART Extended Self-test Log Version: 1 (1 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       522 (0x020a)
Device State:                        Active (0)
Current Temperature:                    38 Celsius
Power Cycle Min/Max Temperature:     37/41 Celsius
Lifetime    Min/Max Temperature:     12/50 Celsius
Under/Over Temperature Limit Count:   0/3

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        30 minutes
Min/Max recommended Temperature:      0/ 0 Celsius
Min/Max Temperature Limit:            0/ 0 Celsius
Temperature History Size (Index):    128 (52)

SCT Error Recovery Control:
           Read: Disabled
          Write: Disabled

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2           23  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS

