smartctl 7.4 2023-08-01 r5530 [FreeBSD 13.2-RELEASE-p2 amd64] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Western Digital VelociRaptor
Device Model:     WDC WD1600HLFS-75G6U1
Serial Number:    --
LU WWN Device Id: 5 0014ee ...
Firmware Version: 04.04V04
User Capacity:    160,000,000,000 bytes [160 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    10000 rpm
Device is:        In smartctl database 7.3/5528
ATA Version is:   ATA8-ACS (minor revision not indicated)
SATA Version is:  SATA 2.5, 3.0 Gb/s
Local Time is:    Wed Sep 13 22:27:40 2023 PKT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Disabled
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x84)	Offline data collection activity
					was suspended by an interrupting command from host.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		( 2700) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  36) minutes.
Conveyance self-test routine
recommended polling time: 	 (   5) minutes.
SCT capabilities: 	       (0x303f)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   200   200   051    -    1284
  3 Spin_Up_Time            PO----   195   193   021    -    3216
  4 Start_Stop_Count        -O--CK   093   093   000    -    7037
  5 Reallocated_Sector_Ct   PO--CK   200   200   140    -    0
  7 Seek_Error_Rate         -OSR--   200   200   000    -    0
  9 Power_On_Hours          -O--CK   075   075   000    -    18276
 10 Spin_Retry_Count        -O--C-   100   100   000    -    0
 11 Calibration_Retry_Count -O--C-   100   100   000    -    0
 12 Power_Cycle_Count       -O--CK   093   093   000    -    7000
192 Power-Off_Retract_Count -O--CK   197   197   000    -    2904
193 Load_Cycle_Count        -O--CK   198   198   000    -    7067
194 Temperature_Celsius     -O---K   103   095   000    -    44
196 Reallocated_Event_Count -O--CK   200   200   000    -    0
197 Current_Pending_Sector  -O--C-   200   200   000    -    0
198 Offline_Uncorrectable   ----C-   200   200   000    -    10
200 Multi_Zone_Error_Rate   ---R--   200   200   000    -    0
240 Head_Flying_Hours       -O--CK   077   077   000    -    17082
241 Total_LBAs_Written      -O--CK   200   200   000    -    49636850624
242 Total_LBAs_Read         -O--CK   200   200   000    -    30379027030
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      6  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa0-0xa7  GPL,SL  VS      16  Device vendor specific log
0xa8-0xb7  GPL,SL  VS       1  Device vendor specific log
0xbd       GPL,SL  VS       1  Device vendor specific log
0xc0       GPL,SL  VS       1  Device vendor specific log
0xc1       GPL     VS      24  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (6 sectors)
Device Error Count: 1284 (device log contains only the most recent 24 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 1284 [11] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 00 01 01 00 51 00 00 40 01 00 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  00 bf 25 13 39 00 00 00 00 00 00 00 0f     00:00:00.000  NOP [Reserved subcommand] [OBS-ACS-2]
  08 46 03 00 0d 13 bf 00 39 ef 00 00 08     00:00:03.329  DEVICE RESET
  00 ba ec 13 39 00 0c 08 0d 03 00 00 00     00:20:59.967  NOP [Reserved subcommand] [OBS-ACS-2]
  08 01 03 00 0d 13 96 0f 20 25 00 00 08     00:00:03.329  DEVICE RESET

Error 1283 [10] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 00 01 01 00 51 00 00 40 01 00 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  00 96 25 13 20 00 00 00 00 00 00 00 0f     00:00:00.000  NOP [Reserved subcommand] [OBS-ACS-2]
  08 46 03 00 0b 13 96 00 20 ef 00 00 08     00:00:03.329  DEVICE RESET
  00 91 ec 13 20 00 0c 08 0b 03 00 00 00     00:20:53.526  NOP [Reserved subcommand] [OBS-ACS-2]
  08 00 01 00 0c 13 71 0f 07 60 00 00 08     00:00:02.816  DEVICE RESET

Error 1282 [9] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 00 01 00 00 51 00 00 40 01 00 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  00 71 60 13 07 00 00 00 00 00 00 00 0f     00:00:00.000  NOP [Reserved subcommand] [OBS-ACS-2]
  08 01 03 00 12 13 1a 0f 07 25 00 00 08     00:00:03.072  DEVICE RESET
  00 1a ef 13 07 00 46 08 ba 03 00 00 00     00:20:47.002  NOP [Reserved subcommand] [OBS-ACS-2]
  08 00 e8 00 ba 13 14 00 07 ec 00 00 08     00:00:47.628  DEVICE RESET

Error 1281 [8] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 00 01 00 00 51 00 00 40 01 00 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  00 68 60 10 6e 00 00 00 00 00 00 00 0d     00:00:00.000  NOP [Reserved subcommand] [OBS-ACS-2]
  08 01 d0 00 01 0f 71 00 9b b0 00 00 08     00:00:33.024  DEVICE RESET
  00 4e 60 0d 94 00 00 08 00 00 00 00 0b     00:17:02.827  NOP [Reserved subcommand] [OBS-ACS-2]
  08 00 e8 00 92 0d 17 0b 5f 60 00 00 08     00:00:46.336  DEVICE RESET

Error 1280 [7] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 00 01 01 00 51 00 00 40 01 00 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  00 f1 25 08 f1 00 00 00 00 00 00 00 0f     00:00:00.000  NOP [Reserved subcommand] [OBS-ACS-2]
  08 46 03 00 95 08 f1 00 f1 ef 00 00 08     00:00:38.145  DEVICE RESET
  00 eb ec 08 f1 00 0c 08 95 03 00 00 00     00:09:46.225  NOP [Reserved subcommand] [OBS-ACS-2]
  08 01 03 00 95 08 cd 0f d8 25 00 00 08     00:00:38.145  DEVICE RESET

Error 1279 [6] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 00 01 01 00 51 00 00 40 01 00 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  00 cd 25 08 d8 00 00 00 00 00 00 00 0f     00:00:00.000  NOP [Reserved subcommand] [OBS-ACS-2]
  08 46 03 00 91 08 cd 00 d8 ef 00 00 08     00:00:38.145  DEVICE RESET
  00 c8 ec 08 d8 00 0c 08 91 03 00 00 00     00:09:39.789  NOP [Reserved subcommand] [OBS-ACS-2]
  08 00 01 00 94 08 66 0f bf 60 00 00 08     00:00:37.120  DEVICE RESET

Error 1278 [5] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 00 01 e8 00 51 00 00 40 01 00 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  00 66 60 08 bf 00 00 00 00 00 00 00 0f     00:00:00.000  NOP [Reserved subcommand] [OBS-ACS-2]
  08 01 03 00 a7 08 14 0f bf 25 00 00 08     00:00:37.888  DEVICE RESET
  00 14 ef 08 bf 00 46 08 a7 03 00 00 00     00:09:33.204  NOP [Reserved subcommand] [OBS-ACS-2]
  08 e8 03 00 a7 08 0f 00 bf ec 00 00 08     00:00:42.764  DEVICE RESET

Error 1277 [4] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 00 01 e8 00 51 00 00 40 01 00 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  00 d5 25 08 a5 00 00 00 00 00 00 00 0f     00:00:00.000  NOP [Reserved subcommand] [OBS-ACS-2]
  08 46 03 00 a0 08 d5 00 a5 ef 00 00 08     00:00:42.984  DEVICE RESET
  00 d0 ec 08 a5 00 0c 08 a0 03 00 00 00     00:09:26.741  NOP [Reserved subcommand] [OBS-ACS-2]
  08 00 e8 00 a7 08 64 0f 8c 60 00 00 08     00:00:40.960  DEVICE RESET

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Aborted by host               90%     12568         -
# 2  Short offline       Completed without error       00%         0         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  2
SCT Version (vendor specific):       258 (0x0102)
Device State:                        SMART Off-line Data Collection executing in background (4)
Current Temperature:                    44 Celsius
Power Cycle Min/Max Temperature:     44/45 Celsius
Lifetime    Min/Max Temperature:     32/52 Celsius
Specified Max Operating Temperature:    36 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      5/60 Celsius
Min/Max Temperature Limit:           -40/70 Celsius
Temperature History Size (Index):    128 (11)

SCT Error Recovery Control:
           Read: Disabled
          Write: Disabled

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x0002  2            0  R_ERR response for data FIS
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0005  2            0  R_ERR response for non-data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x000a  2            3  Device-to-host register FISes sent due to a COMRESET
0x8000  4         4863  Vendor specific

