smartctl 7.3 2022-02-28 r5338 [FreeBSD 13.1-RELEASE amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Toshiba 2.5" HDD MK..34GSX
Device Model:     TOSHIBA MK8034GSX
Serial Number:    --
Firmware Version: AH301D
User Capacity:    80,026,361,856 bytes [80.0 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database 7.3/5319
ATA Version is:   ATA/ATAPI-7 (minor revision not indicated)
Local Time is:    Thu May 11 15:40:41 2023 UTC
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Disabled
APM level is:     128 (minimum power consumption without standby)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  120) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  61) minutes.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     PO-R--   100   100   050    -    0
  2 Throughput_Performance  --S---   100   100   000    -    0
  3 Spin_Up_Time            POS--K   100   100   001    -    1889
  4 Start_Stop_Count        -O--CK   100   100   000    -    5138
  5 Reallocated_Sector_Ct   PO--CK   100   100   050    -    0
  7 Seek_Error_Rate         -O-R--   100   100   000    -    0
  8 Seek_Time_Performance   --S---   100   100   000    -    0
  9 Power_On_Hours          -O--CK   068   068   000    -    13057
 10 Spin_Retry_Count        -O--CK   202   100   000    -    0
 12 Power_Cycle_Count       -O--CK   100   100   000    -    4274
192 Power-Off_Retract_Count -O--CK   100   100   000    -    186
193 Load_Cycle_Count        -O--CK   042   042   000    -    580895
194 Temperature_Celsius     -O---K   100   100   000    -    30 (Min/Max 2/60)
196 Reallocated_Event_Count -O--CK   100   100   000    -    0
197 Current_Pending_Sector  -O--CK   100   100   000    -    0
198 Offline_Uncorrectable   ----CK   100   100   000    -    0
199 UDMA_CRC_Error_Count    -O--CK   200   200   000    -    17
220 Disk_Shift              -O----   100   100   000    -    4328
222 Loaded_Hours            -O--CK   079   079   000    -    8620
223 Load_Retry_Count        -O--CK   100   100   000    -    0
224 Load_Friction           -O---K   100   100   000    -    0
226 Load-in_Time            -OS--K   100   100   000    -    410
240 Head_Flying_Hours       ------   100   100   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O     51  Comprehensive SMART error log
0x03       GPL     R/O     64  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log

SMART Extended Comprehensive Error Log Version: 1 (64 sectors)
Device Error Count: 265 (device log contains only the most recent 256 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 265 [8] occurred at disk power-on lifetime: 12598 hours (524 days + 22 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 41 00 b2 00 00 00 00 80 00 40 00  Error: ICRC, ABRT at LBA = 0x00008000 = 32768

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 01 00 00 b0 00 00 00 00 80 00 40 00     02:42:47.277  READ FPDMA QUEUED
  60 01 00 00 a8 00 00 00 00 00 22 40 00     02:42:47.277  READ FPDMA QUEUED
  60 01 00 00 a0 00 00 00 00 00 00 40 00     02:42:47.277  READ FPDMA QUEUED
  e7 00 00 00 00 00 80 ff 00 00 00 a0 00     02:42:47.271  FLUSH CACHE
  60 01 00 00 b0 00 00 00 00 80 00 40 00     02:42:47.123  READ FPDMA QUEUED

Error 264 [7] occurred at disk power-on lifetime: 12598 hours (524 days + 22 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 41 00 b2 00 00 00 00 80 00 40 00  Error: ICRC, ABRT at LBA = 0x00008000 = 32768

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 01 00 00 b0 00 00 00 00 80 00 40 00     02:42:47.277  READ FPDMA QUEUED
  60 01 00 00 a8 00 00 00 00 00 22 40 00     02:42:47.277  READ FPDMA QUEUED
  60 01 00 00 a0 00 00 00 00 00 00 40 00     02:42:47.277  READ FPDMA QUEUED
  e7 00 00 00 00 00 80 ff 00 00 00 a0 00     02:42:47.271  FLUSH CACHE
  60 01 00 00 b0 00 00 00 00 80 00 40 00     02:42:47.123  READ FPDMA QUEUED

Error 263 [6] occurred at disk power-on lifetime: 12555 hours (523 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 41 00 ba 00 00 00 0e 81 cf 40 00  Error: ICRC, ABRT at LBA = 0x000e81cf = 950735

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 7f ff 00 b8 00 00 00 0e 81 cf 40 00     00:10:11.152  READ FPDMA QUEUED
  60 00 10 00 c0 00 00 00 0e 81 c0 40 00     00:10:11.141  READ FPDMA QUEUED
  60 00 10 00 b0 00 00 00 10 98 90 40 00     00:10:11.130  READ FPDMA QUEUED
  60 1c 08 00 a8 00 00 00 10 7c 97 40 00     00:10:11.017  READ FPDMA QUEUED
  60 18 24 00 98 00 00 00 10 64 73 40 00     00:10:10.917  READ FPDMA QUEUED

Error 262 [5] occurred at disk power-on lifetime: 12555 hours (523 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 41 00 ba 00 00 00 0e 81 cf 40 00  Error: ICRC, ABRT at LBA = 0x000e81cf = 950735

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 7f ff 00 b8 00 00 00 0e 81 cf 40 00     00:10:11.152  READ FPDMA QUEUED
  60 00 10 00 c0 00 00 00 0e 81 c0 40 00     00:10:11.141  READ FPDMA QUEUED
  60 00 10 00 b0 00 00 00 10 98 90 40 00     00:10:11.130  READ FPDMA QUEUED
  60 1c 08 00 a8 00 00 00 10 7c 97 40 00     00:10:11.017  READ FPDMA QUEUED
  60 18 24 00 98 00 00 00 10 64 73 40 00     00:10:10.917  READ FPDMA QUEUED

Error 261 [4] occurred at disk power-on lifetime: 12522 hours (521 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 01 00 00 03 d3 b3 ff e0 00  Error: ICRC, ABRT 1 sectors at LBA = 0x03d3b3ff = 64205823

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  35 00 00 00 80 00 00 03 d3 b3 80 e0 00     00:19:50.441  WRITE DMA EXT
  35 00 00 00 80 00 00 03 d3 b3 00 e0 00     00:19:50.439  WRITE DMA EXT
  35 00 00 00 80 00 00 03 d3 b2 80 e0 00     00:19:50.437  WRITE DMA EXT
  35 00 00 00 80 00 00 03 d3 b2 00 e0 00     00:19:50.434  WRITE DMA EXT
  35 00 00 00 80 00 00 03 d3 b1 80 e0 00     00:19:50.432  WRITE DMA EXT

Error 260 [3] occurred at disk power-on lifetime: 4031 hours (167 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 01 00 00 01 53 e9 aa e1 00  Error: ICRC, ABRT 1 sectors at LBA = 0x0153e9aa = 22276522

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 40 26 f1 2f 53 e7 b2 e1 00     00:00:07.672  READ DMA
  c8 00 00 00 80 47 6b 7f 26 f0 b0 e9 00     00:00:07.648  READ DMA
  c8 00 00 00 08 47 6b 77 47 6b 78 e1 00     00:00:07.571  READ DMA
  c8 00 00 00 08 00 00 00 47 6b 70 e1 00     00:00:07.570  READ DMA
  e7 00 00 00 00 a1 70 0f 00 00 00 a0 00     00:00:07.465  FLUSH CACHE

Error 259 [2] occurred at disk power-on lifetime: 3416 hours (142 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 01 00 00 02 61 58 1f e2 00  Error: ICRC, ABRT 1 sectors at LBA = 0x0261581f = 39933983

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 08 67 3c 2f 61 56 70 e2 00     00:39:21.370  READ DMA
  c8 00 00 00 08 6c 08 b7 67 3c 28 e2 00     00:39:21.356  READ DMA
  c8 00 00 00 08 69 7d 7f 6c 08 b0 e2 00     00:39:21.355  READ DMA
  c8 00 00 00 08 44 1b 51 69 7d 78 e2 00     00:39:21.341  READ DMA
  c8 00 00 00 08 6c 08 a7 44 1b 4a e1 00     00:39:21.332  READ DMA

Error 258 [1] occurred at disk power-on lifetime: 2551 hours (106 days + 7 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 01 00 00 08 c5 d3 39 e8 00  Error: ICRC, ABRT 1 sectors at LBA = 0x08c5d339 = 147182393

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 48 c5 d1 57 c5 d2 d8 e8 00     00:00:10.028  READ DMA
  c8 00 00 00 38 58 f7 89 c5 d1 20 e8 00     00:00:10.016  READ DMA
  c8 00 00 00 40 c5 d2 d7 58 f7 4a e1 00     00:00:10.015  READ DMA
  c8 00 00 00 18 c5 d2 b7 c5 d2 c0 e8 00     00:00:10.015  READ DMA
  c8 00 00 00 68 58 f9 39 c5 d2 50 e8 00     00:00:10.014  READ DMA

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%         0         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Commands not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  4            0  Command failed due to ICRC error
0x0002  4            0  R_ERR response for data FIS
0x0003  4            0  R_ERR response for device-to-host data FIS
0x0004  4            0  R_ERR response for host-to-device data FIS
0x0005  4            0  R_ERR response for non-data FIS
0x0006  4            0  R_ERR response for device-to-host non-data FIS
0x0007  4            0  R_ERR response for host-to-device non-data FIS
0x0008  4            0  Device-to-host non-data FIS retries
0x0009  4            1  Transition from drive PhyRdy to drive PhyNRdy
0x000a  4            1  Device-to-host register FISes sent due to a COMRESET
0x000b  4            0  CRC errors within host-to-device FIS
0x000d  4            0  Non-CRC errors within host-to-device FIS
0x000f  4            0  R_ERR response for host-to-device data FIS, CRC
0x0010  4            0  R_ERR response for host-to-device data FIS, non-CRC
0x0012  4            0  R_ERR response for host-to-device non-data FIS, CRC
0x0013  4            0  R_ERR response for host-to-device non-data FIS, non-CRC



