smartctl 7.4 2023-08-01 r5530 [FreeBSD 14.0-BETA5 amd64] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Constellation.2 (SATA)
Device Model:     MM1000GBKAL
Serial Number:    --
LU WWN Device Id: 5 000c50 ...
Firmware Version: HPGE
User Capacity:    1,000,204,886,016 bytes [1.00 TB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    7200 rpm
Form Factor:      2.5 inches
Device is:        In smartctl database 7.3/5528
ATA Version is:   ATA8-ACS T13/1699-D revision 6
SATA Version is:  SATA 3.0, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Fri Nov 24 21:41:33 2023 CET
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Disabled
DSN feature is:   Unavailable
ATA Security is:  Unavailable
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  642) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 ( 204) minutes.
Conveyance self-test routine
recommended polling time: 	 (   3) minutes.
SCT capabilities: 	       (0x103d)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   082   063   044    -    182229588
  3 Spin_Up_Time            PO----   094   094   070    -    0
  4 Start_Stop_Count        -O--CK   100   100   020    -    127
  5 Reallocated_Sector_Ct   PO--CK   095   095   036    -    237
  7 Seek_Error_Rate         POSR--   081   060   030    -    140946336
  9 Power_On_Hours          -O--CK   049   049   000    -    45207
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   100   100   020    -    126
180 Unknown_HDD_Attribute   PO-RCK   100   100   030    -    189036646
184 End-to-End_Error        -O--CK   100   100   003    -    0
187 Reported_Uncorrect      -O--CK   100   100   000    -    0
188 Command_Timeout         -O--CK   100   100   000    -    0
189 High_Fly_Writes         -O-RCK   100   100   000    -    0
190 Airflow_Temperature_Cel -O---K   076   051   045    -    24 (Min/Max 13/25)
191 G-Sense_Error_Rate      -O--CK   100   100   000    -    0
192 Power-Off_Retract_Count -O--CK   100   100   000    -    125
193 Load_Cycle_Count        -O--CK   100   100   000    -    1990
194 Temperature_Celsius     -O---K   024   049   000    -    24 (0 11 0 0 0)
195 Hardware_ECC_Recovered  -O-RC-   118   099   000    -    182229588
196 Reallocated_Event_Count PO--CK   095   095   036    -    237
197 Current_Pending_Sector  -O--C-   100   100   000    -    0
198 Offline_Uncorrectable   ----C-   100   100   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      5  Ext. Comprehensive SMART error log
0x04       GPL,SL  R/O      8  Device Statistics log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x12       GPL,SL  R/O      1  SATA NCQ Non-Data log
0x21       GPL     R/O      1  Write stream error log
0x22       GPL     R/O      1  Read stream error log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS      20  Device vendor specific log
0xa2       GPL     VS    4496  Device vendor specific log
0xa8       GPL,SL  VS     129  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xb0       GPL     VS    5176  Device vendor specific log
0xb6       GPL     VS    1918  Device vendor specific log
0xbd       GPL     VS     252  Device vendor specific log
0xbe-0xbf  GPL     VS   65535  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 33 (device log contains only the most recent 20 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 33 [12] occurred at disk power-on lifetime: 44764 hours (1865 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 00 00 00 18 1e 12 c8 00 00  Error: IDNF at LBA = 0x181e12c8 = 404624072

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 08 00 00 18 1e 12 c8 40 00  3d+15:56:32.197  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 05 80 28 f0 40 00  3d+15:56:32.185  WRITE FPDMA QUEUED
  60 00 00 00 60 00 00 23 23 b6 f0 40 00  3d+15:56:32.162  READ FPDMA QUEUED
  60 00 00 00 18 00 00 23 23 b6 d8 40 00  3d+15:56:32.162  READ FPDMA QUEUED
  61 00 00 00 08 00 00 22 82 54 80 40 00  3d+15:56:32.141  WRITE FPDMA QUEUED

Error 32 [11] occurred at disk power-on lifetime: 44764 hours (1865 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 00 00 00 05 80 28 d0 00 00  Error: IDNF at LBA = 0x058028d0 = 92285136

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 08 00 00 05 80 28 d0 40 00  3d+15:56:05.463  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 18 00 57 30 40 00  3d+15:56:05.441  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 05 80 28 d0 40 00  3d+15:56:05.435  WRITE FPDMA QUEUED
  61 00 00 00 18 00 00 02 94 5d 80 40 00  3d+15:56:05.429  WRITE FPDMA QUEUED
  61 00 00 00 30 00 00 02 94 3a 08 40 00  3d+15:56:05.412  WRITE FPDMA QUEUED

Error 31 [10] occurred at disk power-on lifetime: 44764 hours (1865 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 00 00 00 18 1e 5f f8 00 00  Error: IDNF at LBA = 0x181e5ff8 = 404643832

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 28 00 00 18 1e 5f f8 40 00  3d+15:49:58.221  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 02 9f 8b 78 40 00  3d+15:49:58.211  WRITE FPDMA QUEUED
  61 00 00 00 50 00 00 24 80 79 a8 40 00  3d+15:49:58.204  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 24 00 31 b8 40 00  3d+15:49:58.196  WRITE FPDMA QUEUED
  61 00 00 00 28 00 00 23 80 63 30 40 00  3d+15:49:58.188  WRITE FPDMA QUEUED

Error 30 [9] occurred at disk power-on lifetime: 44764 hours (1865 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 00 00 00 18 1e 5f 00 00 00  Error: IDNF at LBA = 0x181e5f00 = 404643584

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 08 00 00 18 1e 5f 00 40 00  3d+15:49:38.462  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 18 1e 5e f8 40 00  3d+15:49:38.456  WRITE FPDMA QUEUED
  60 00 00 01 c0 00 00 23 19 e2 18 40 00  3d+15:49:38.453  READ FPDMA QUEUED
  60 00 00 02 00 00 00 23 19 e0 18 40 00  3d+15:49:38.449  READ FPDMA QUEUED
  60 00 00 01 78 00 00 23 19 de 10 40 00  3d+15:49:38.447  READ FPDMA QUEUED

Error 29 [8] occurred at disk power-on lifetime: 44764 hours (1865 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 00 00 00 18 1e 58 40 00 00  Error: IDNF at LBA = 0x181e5840 = 404641856

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 08 00 00 18 1e 58 40 40 00  3d+15:47:16.912  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 21 30 6e c8 40 00  3d+15:47:16.903  WRITE FPDMA QUEUED
  60 00 00 00 c8 00 00 23 30 5b b0 40 00  3d+15:47:16.898  READ FPDMA QUEUED
  60 00 00 01 40 00 00 23 30 5a 18 40 00  3d+15:47:16.888  READ FPDMA QUEUED
  60 00 00 02 00 00 00 23 30 58 18 40 00  3d+15:47:16.887  READ FPDMA QUEUED

Error 28 [7] occurred at disk power-on lifetime: 44764 hours (1865 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 00 00 00 18 1e 57 b8 00 00  Error: IDNF at LBA = 0x181e57b8 = 404641720

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 08 00 00 18 1e 57 b8 40 00  3d+15:47:03.849  WRITE FPDMA QUEUED
  61 00 00 00 20 00 00 24 80 6d 10 40 00  3d+15:47:03.840  WRITE FPDMA QUEUED
  61 00 00 00 10 00 00 24 80 6c f8 40 00  3d+15:47:03.832  WRITE FPDMA QUEUED
  61 00 00 00 10 00 00 24 80 6c d8 40 00  3d+15:47:03.821  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 24 00 30 50 40 00  3d+15:47:03.814  WRITE FPDMA QUEUED

Error 27 [6] occurred at disk power-on lifetime: 44764 hours (1865 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 00 00 00 23 80 52 d8 00 00  Error: IDNF at LBA = 0x238052d8 = 595612376

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 08 00 00 23 80 52 d8 40 00  3d+15:44:02.266  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 23 33 d0 f8 40 00  3d+15:44:02.260  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 22 83 61 30 40 00  3d+15:44:02.251  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 21 86 d7 c0 40 00  3d+15:44:02.242  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 24 80 5f b8 40 00  3d+15:44:02.213  WRITE FPDMA QUEUED

Error 26 [5] occurred at disk power-on lifetime: 44764 hours (1865 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 00 00 00 18 1e 4d d8 00 00  Error: IDNF at LBA = 0x181e4dd8 = 404639192

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 08 00 00 18 1e 4d d8 40 00  3d+15:43:21.352  WRITE FPDMA QUEUED
  60 00 00 00 48 00 00 23 24 7b a8 40 00  3d+15:43:21.352  READ FPDMA QUEUED
  60 00 00 00 20 00 00 23 24 7b f0 40 00  3d+15:43:21.351  READ FPDMA QUEUED
  61 00 00 00 08 00 00 22 82 66 08 40 00  3d+15:43:21.343  WRITE FPDMA QUEUED
  60 00 00 00 20 00 00 23 24 7a c8 40 00  3d+15:43:21.328  READ FPDMA QUEUED

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%     44780         -
# 2  Short offline       Completed without error       00%     44756         -
# 3  Short offline       Completed without error       00%     44733         -
# 4  Short offline       Completed without error       00%     44708         -
# 5  Short offline       Completed without error       00%     44430         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       522 (0x020a)
Device State:                        Active (0)
Current Temperature:                    24 Celsius
Power Cycle Min/Max Temperature:     13/25 Celsius
Lifetime    Min/Max Temperature:     11/48 Celsius
Specified Max Operating Temperature:    60 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        10 minutes
Min/Max recommended Temperature:      5/60 Celsius
Min/Max Temperature Limit:           -40/70 Celsius
Temperature History Size (Index):    128 (121)

SCT Error Recovery Control:
           Read:    100 (10.0 seconds)
          Write:    100 (10.0 seconds)

Device Statistics (GP Log 0x04)
Page  Offset Size        Value Flags Description
0x01  =====  =               =  ===  == General Statistics (rev 2) ==
0x01  0x008  4             126  ---  Lifetime Power-On Resets
0x01  0x010  4           45207  ---  Power-on Hours
0x01  0x018  6     12607431482  ---  Logical Sectors Written
0x01  0x020  6        84209927  ---  Number of Write Commands
0x01  0x028  6     55042730696  ---  Logical Sectors Read
0x01  0x030  6       200988889  ---  Number of Read Commands
0x03  =====  =               =  ===  == Rotating Media Statistics (rev 1) ==
0x03  0x008  4           45210  ---  Spindle Motor Power-on Hours
0x03  0x010  4           45210  ---  Head Flying Hours
0x03  0x018  4            1990  ---  Head Load Events
0x03  0x020  4             237  ---  Number of Reallocated Logical Sectors
0x03  0x028  4               0  ---  Read Recovery Attempts
0x03  0x030  4               0  ---  Number of Mechanical Start Failures
0x04  =====  =               =  ===  == General Errors Statistics (rev 1) ==
0x04  0x008  4               0  ---  Number of Reported Uncorrectable Errors
0x04  0x010  4               0  ---  Resets Between Cmd Acceptance and Completion
                                |||_ C monitored condition met
                                ||__ D supports DSN
                                |___ N normalized value

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2           18  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS



