smartctl 7.4 2023-08-01 r5530 [FreeBSD 14.0-RELEASE-p6 amd64] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Momentus 5400.6
Device Model:     ST9500325AS
Serial Number:    --
LU WWN Device Id: 5 000c50 ...
Firmware Version: 0001SDM1
User Capacity:    500,107,862,016 bytes [500 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    5400 rpm
Device is:        In smartctl database 7.3/5528
ATA Version is:   ATA8-ACS T13/1699-D revision 4
SATA Version is:  SATA 2.6, 3.0 Gb/s
Local Time is:    Thu Apr 11 19:15:03 2024 CDT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     128 (minimum power consumption without standby)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unknown

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(    0) seconds.
Offline data collection
capabilities: 			 (0x73) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 ( 144) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x103b)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   108   088   006    -    17131496
  3 Spin_Up_Time            PO----   099   099   000    -    0
  4 Start_Stop_Count        -O--CK   100   100   020    -    914
  5 Reallocated_Sector_Ct   PO--CK   097   097   036    -    68
  7 Seek_Error_Rate         POSR--   086   060   030    -    443018788
  9 Power_On_Hours          -O--CK   032   032   000    -    60285
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   100   100   020    -    366
184 End-to-End_Error        -O--CK   100   100   099    -    0
187 Reported_Uncorrect      -O--CK   001   001   000    -    488
188 Command_Timeout         -O--CK   100   099   000    -    8590065667
189 High_Fly_Writes         -O-RCK   100   100   000    -    0
190 Airflow_Temperature_Cel -O---K   065   055   045    -    35 (Min/Max 33/35)
191 G-Sense_Error_Rate      -O--CK   100   100   000    -    57
192 Power-Off_Retract_Count -O--CK   100   100   000    -    0
193 Load_Cycle_Count        -O--CK   001   001   000    -    914274
194 Temperature_Celsius     -O---K   035   045   000    -    35 (0 9 0 0 0)
195 Hardware_ECC_Recovered  -O-RC-   048   038   000    -    17131496
197 Current_Pending_Sector  -O--C-   100   100   000    -    1
198 Offline_Uncorrectable   ----C-   100   100   000    -    1
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    0
254 Free_Fall_Sensor        -O--CK   100   100   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01       GPL,SL  R/O      1  Summary SMART error log
0x02       GPL,SL  R/O      5  Comprehensive SMART error log
0x03       GPL,SL  R/O      5  Ext. Comprehensive SMART error log
0x06       GPL,SL  R/O      1  SMART self-test log
0x07       GPL,SL  R/O      1  Extended self-test log
0x09       GPL,SL  R/W      1  Selective self-test log
0x10       GPL,SL  R/O      1  NCQ Command Error log
0x11       GPL,SL  R/O      1  SATA Phy Event Counters log
0x21       GPL,SL  R/O      1  Write stream error log
0x22       GPL,SL  R/O      1  Read stream error log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS      20  Device vendor specific log
0xa2       GPL     VS    2248  Device vendor specific log
0xa8       GPL,SL  VS      65  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xb0       GPL     VS    2864  Device vendor specific log
0xbe-0xbf  GPL     VS   65535  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 356 (device log contains only the most recent 20 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 356 [15] occurred at disk power-on lifetime: 57463 hours (2394 days + 7 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 8c 00 e3 39 bb 00 00  Error: UNC at LBA = 0x8c00e339bb = 601310312891

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 8c 00 e0 39 58 40 00     04:29:19.877  READ FPDMA QUEUED
  60 00 00 00 08 00 8c 00 d5 39 b0 40 00     04:29:19.393  READ FPDMA QUEUED
  60 00 00 00 08 00 8c 00 ba 39 18 40 00     04:29:18.534  READ FPDMA QUEUED
  60 00 00 00 08 00 8c 00 b6 39 b8 40 00     04:29:17.742  READ FPDMA QUEUED
  60 00 00 00 08 00 8c 00 a2 39 60 40 00     04:29:16.245  READ FPDMA QUEUED

Error 355 [14] occurred at disk power-on lifetime: 57461 hours (2394 days + 5 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 1d 00 07 1d eb 00 00  Error: UNC at LBA = 0x1d00071deb = 124554517995

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 1d 00 07 1d e8 40 00     02:09:09.177  READ FPDMA QUEUED
  60 00 00 00 08 00 1d 00 07 1d e0 40 00     02:09:07.746  READ FPDMA QUEUED
  60 00 00 00 08 00 1d 00 07 1d d8 40 00     02:09:06.394  READ FPDMA QUEUED
  60 00 00 00 08 00 12 00 a1 1d 20 40 00     02:08:52.287  READ FPDMA QUEUED
  60 00 00 00 08 00 12 00 a1 1d 18 40 00     02:08:51.109  READ FPDMA QUEUED

Error 354 [13] occurred at disk power-on lifetime: 57461 hours (2394 days + 5 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 12 00 a0 1d f1 00 00  Error: UNC at LBA = 0x1200a01df1 = 77319904753

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 05 00 4b 1d 58 40 00     02:08:29.191  READ FPDMA QUEUED
  60 00 00 00 08 00 05 00 4b 1d 50 40 00     02:08:29.188  READ FPDMA QUEUED
  60 00 00 00 08 00 f5 00 54 1c c0 40 00     02:08:11.054  READ FPDMA QUEUED
  60 00 00 00 08 00 f5 00 54 1c b8 40 00     02:08:11.044  READ FPDMA QUEUED
  60 00 00 00 08 00 e5 00 5f 1c 38 40 00     02:07:52.915  READ FPDMA QUEUED

Error 353 [12] occurred at disk power-on lifetime: 57460 hours (2394 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 c5 00 bc 12 01 00 00  Error: UNC at LBA = 0xc500bc1201 = 846120882689

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 c5 00 bb 12 b8 40 00     01:18:55.235  READ FPDMA QUEUED
  60 00 00 00 08 00 c5 00 bb 12 b0 40 00     01:18:55.169  READ FPDMA QUEUED
  60 00 00 00 08 00 c5 00 bb 12 a8 40 00     01:18:55.137  READ FPDMA QUEUED
  27 00 00 00 00 00 00 00 00 00 00 e0 00     01:18:55.136  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 00 00 00 00 00 00 00 00 00 00 a0 00     01:18:55.135  IDENTIFY DEVICE

Error 352 [11] occurred at disk power-on lifetime: 57460 hours (2394 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 c5 00 bb 12 a3 00 00  Error: UNC at LBA = 0xc500bb12a3 = 846120817315

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 c5 00 ba 12 a8 40 00     01:18:52.746  READ FPDMA QUEUED
  60 00 00 00 08 00 c5 00 ba 12 a0 40 00     01:18:52.629  READ FPDMA QUEUED
  27 00 00 00 00 00 00 00 00 00 00 e0 00     01:18:52.629  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 00 00 00 00 00 00 00 00 00 00 a0 00     01:18:52.627  IDENTIFY DEVICE
  ef 00 03 00 46 00 00 00 00 00 00 a0 00     01:18:52.627  SET FEATURES [Set transfer mode]

Error 351 [10] occurred at disk power-on lifetime: 57460 hours (2394 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 c5 00 69 12 11 00 00  Error: UNC at LBA = 0xc500691211 = 846115443217

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 c5 00 68 12 d0 40 00     01:18:44.107  READ FPDMA QUEUED
  60 00 00 00 08 00 c5 00 68 12 c8 40 00     01:18:43.989  READ FPDMA QUEUED
  27 00 00 00 00 00 00 00 00 00 00 e0 00     01:18:43.988  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 00 00 00 00 00 00 00 00 00 00 a0 00     01:18:43.987  IDENTIFY DEVICE
  ef 00 03 00 46 00 00 00 00 00 00 a0 00     01:18:43.986  SET FEATURES [Set transfer mode]

Error 350 [9] occurred at disk power-on lifetime: 57460 hours (2394 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 c5 00 68 12 c0 00 00  Error: UNC at LBA = 0xc5006812c0 = 846115377856

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 c1 00 a4 12 20 40 00     01:18:37.442  READ FPDMA QUEUED
  60 00 00 00 08 00 c1 00 a4 12 18 40 00     01:18:37.434  READ FPDMA QUEUED
  60 00 00 00 08 00 b1 00 ae 12 98 40 00     01:18:19.327  READ FPDMA QUEUED
  60 00 00 00 08 00 b1 00 ae 12 90 40 00     01:18:19.321  READ FPDMA QUEUED
  60 00 00 00 08 00 a1 00 ba 12 a0 40 00     01:18:01.339  READ FPDMA QUEUED

Error 349 [8] occurred at disk power-on lifetime: 57459 hours (2394 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 45 00 da 08 40 00 00  Error: UNC at LBA = 0x4500da0840 = 296367032384

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 45 00 da 08 40 40 00     00:26:54.047  READ FPDMA QUEUED
  60 00 00 00 08 00 45 00 da 08 38 40 00     00:26:54.046  READ FPDMA QUEUED
  60 00 00 00 08 00 45 00 da 08 30 40 00     00:26:54.046  READ FPDMA QUEUED
  60 00 00 00 08 00 45 00 da 08 28 40 00     00:26:54.045  READ FPDMA QUEUED
  60 00 00 00 08 00 45 00 da 08 20 40 00     00:26:54.045  READ FPDMA QUEUED

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%      2350         -
# 2  Extended offline    Aborted by host               30%      2349         -
# 3  Conveyance offline  Completed without error       00%      1015         -
# 4  Short offline       Completed without error       00%      1015         -
# 5  Extended offline    Aborted by host               70%      1015         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       522 (0x020a)
Device State:                        Active (0)
Current Temperature:                    35 Celsius
Power Cycle Min/Max Temperature:     33/35 Celsius
Lifetime    Min/Max Temperature:      9/45 Celsius
Under/Over Temperature Limit Count:   0/14

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      0/ 0 Celsius
Min/Max Temperature Limit:            0/ 0 Celsius
Temperature History Size (Index):    128 (80)

SCT Error Recovery Control:
           Read: Disabled
          Write: Disabled

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2            3  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS

