ADATA Solid State Drives
========================

This is a list of all tested ADATA solid state drive models and their MTBFs. See
more info on reliability test in the [README](https://github.com/bsdhw/SMART).

Contents
--------

1. [ SSD by Model  ](#ssd-by-model)
2. [ SSD by Family ](#ssd-by-family)

SSD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| ADATA     | SP310              | 32 GB  | 2       | 1914  | 0     | 5.25   |
| ADATA     | SP900              | 64 GB  | 3       | 1342  | 0     | 3.68   |
| ADATA     | SP600              | 32 GB  | 2       | 1097  | 0     | 3.01   |
| ADATA     | SSD S510           | 64 GB  | 2       | 839   | 0     | 2.30   |
| ADATA     | SP920SS            | 128 GB | 2       | 816   | 0     | 2.24   |
| ADATA     | SP600              | 64 GB  | 2       | 683   | 0     | 1.87   |
| ADATA     | SP600              | 128 GB | 2       | 673   | 0     | 1.84   |
| ADATA     | IM2S3134N-064GM    | 64 GB  | 23      | 660   | 0     | 1.81   |
| ADATA     | SP900              | 128 GB | 7       | 493   | 0     | 1.35   |
| ADATA     | SU750              | 256 GB | 3       | 381   | 0     | 1.04   |
| ADATA     | SP900              | 256 GB | 2       | 614   | 212   | 0.85   |
| ADATA     | SU650              | 960 GB | 2       | 358   | 145   | 0.76   |
| ADATA     | SU650              | 480 GB | 3       | 248   | 0     | 0.68   |
| ADATA     | SU800              | 256 GB | 10      | 219   | 201   | 0.59   |
| ADATA     | SU800NS38          | 256 GB | 2       | 204   | 0     | 0.56   |
| ADATA     | SU650              | 120 GB | 37      | 257   | 37    | 0.56   |
| ADATA     | SU800              | 1 TB   | 3       | 344   | 15    | 0.49   |
| ADATA     | SU630              | 480 GB | 3       | 177   | 0     | 0.49   |
| ADATA     | SU630              | 240 GB | 17      | 199   | 2     | 0.48   |
| ADATA     | SU655              | 120 GB | 4       | 164   | 0     | 0.45   |
| ADATA     | SU800              | 128 GB | 11      | 173   | 1     | 0.43   |
| ADATA     | SU650              | 240 GB | 14      | 147   | 0     | 0.40   |
| ADATA     | SU635              | 240 GB | 4       | 97    | 0     | 0.27   |
| ADATA     | SU800              | 512 GB | 4       | 65    | 0     | 0.18   |
| ADATA     | ASU800SS-128GT     | 128 GB | 2       | 39    | 0     | 0.11   |
| ADATA     | SU760              | 1 TB   | 2       | 8     | 0     | 0.02   |
| ADATA     | SX300              | 128 GB | 2       | 24    | 525   | 0.00   |

SSD by Family
-------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Family                 | Models | Samples | Days  | Err   | MTBF |
|-----------|------------------------|--------|---------|-------|-------|------|
| ADATA     | JMicron based SSDs     | 2      | 4       | 1299  | 0     | 3.56   |
| ADATA     | JMicron/Maxiotek ba... | 2      | 4       | 885   | 0     | 2.43   |
| ADATA     | SandForce Driven SSDs  | 4      | 14      | 742   | 31    | 1.92   |
| ADATA     | Silicon Motion base... | 9      | 88      | 216   | 42    | 0.50   |
