smartctl 7.3 2022-02-28 r5338 [FreeBSD 14.0-CURRENT amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     SAMSUNG SpinPoint T166
Device Model:     SAMSUNG HD501LJ
Serial Number:    --
LU WWN Device Id: 5 0000f0 ...
Firmware Version: CR100-10
User Capacity:    500,107,862,016 bytes [500 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database 7.3/5319
ATA Version is:   ATA8-ACS T13/1699-D revision 3b
SATA Version is:  SATA 2.5, 3.0 Gb/s
Local Time is:    Sun Jul 17 18:36:01 2022 EDT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Disabled
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		( 8961) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 ( 153) minutes.
SCT capabilities: 	       (0x003f)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   253   100   051    -    1
  3 Spin_Up_Time            POS---   100   100   015    -    7616
  4 Start_Stop_Count        -O--CK   074   074   000    -    26593
  5 Reallocated_Sector_Ct   PO--CK   100   100   010    -    2
  7 Seek_Error_Rate         POSR--   253   253   051    -    0
  8 Seek_Time_Performance   P-S--K   253   253   015    -    0
  9 Power_On_Hours          -O--CK   100   100   000    -    26239
 10 Spin_Retry_Count        PO--CK   253   253   051    -    0
 11 Calibration_Retry_Count -O--C-   253   100   000    -    0
 12 Power_Cycle_Count       -O--CK   093   093   000    -    7255
187 Reported_Uncorrect      -O--CK   043   043   000    -    393274
188 Command_Timeout         -O--CK   253   253   000    -    0
190 Airflow_Temperature_Cel -O---K   072   053   000    -    28
194 Temperature_Celsius     -O---K   154   097   000    -    28
195 Hardware_ECC_Recovered  -O-RC-   100   100   000    -    32482
196 Reallocated_Event_Count -O--CK   100   100   000    -    2
197 Total_Pending_Sectors   -O--C-   253   100   000    -    0
198 Offline_Uncorrectable   ----CK   253   253   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    0
200 Multi_Zone_Error_Rate   -O-R--   253   100   000    -    0
201 Soft_Read_Error_Rate    -O-R--   253   100   000    -    0
202 Data_Address_Mark_Errs  -O--CK   098   098   000    -    699
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      2  Comprehensive SMART error log
0x03       GPL     R/O      2  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log

SMART Extended Comprehensive Error Log Version: 1 (2 sectors)
Invalid Error Log index = 0x0000, trying reserved byte (0x05) instead
Device Error Count: 77 (device log contains only the most recent 8 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 77 [4] occurred at disk power-on lifetime: 11731 hours (488 days + 19 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 08 00 00 18 fc 00 b8 e0 00  Error: UNC 8 sectors at LBA = 0x18fc00b8 = 419168440

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 08 00 00 00 18 fc b8 e0 00     00:55:09.563  READ DMA
  c8 00 00 00 08 00 00 00 18 fc b0 e0 00     00:55:06.938  READ DMA
  c8 00 00 00 08 00 00 00 18 fc a8 e0 00     00:55:06.938  READ DMA
  c8 00 00 00 08 00 00 00 18 fc a0 e0 00     00:55:06.938  READ DMA
  c8 00 00 00 08 00 00 00 18 fc 98 e0 00     00:55:06.938  READ DMA

Error 76 [3] occurred at disk power-on lifetime: 11642 hours (485 days + 2 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 01 00 00 00 18 fc b8 e0 00  Error: UNC 1 sectors at LBA = 0x0018fcb8 = 1637560

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 01 00 00 00 18 fc b8 e0 00     02:32:21.625  READ DMA EXT
  25 00 00 00 01 00 00 00 18 fc b7 e0 00     02:32:18.813  READ DMA EXT
  25 00 00 00 01 00 00 00 18 fc b6 e0 00     02:32:18.813  READ DMA EXT
  25 00 00 00 01 00 00 00 18 fc b5 e0 00     02:32:18.813  READ DMA EXT
  25 00 00 00 01 00 00 00 18 fc b4 e0 00     02:32:18.813  READ DMA EXT

Error 75 [2] occurred at disk power-on lifetime: 11642 hours (485 days + 2 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 20 00 00 00 18 fc a0 e0 00  Error: UNC 32 sectors at LBA = 0x0018fca0 = 1637536

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 20 00 00 00 18 fc a0 e0 00     02:32:18.500  READ DMA EXT
  35 00 00 00 18 00 00 01 56 af 30 e0 00     02:32:15.688  WRITE DMA EXT
  25 00 00 00 18 00 00 00 16 f2 20 e0 00     02:32:15.688  READ DMA EXT
  35 00 00 00 20 00 00 13 24 b8 a0 e0 00     02:32:15.688  WRITE DMA EXT
  35 00 00 00 20 00 00 13 27 3d 80 e0 00     02:32:15.688  WRITE DMA EXT

Error 74 [1] occurred at disk power-on lifetime: 11641 hours (485 days + 1 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 01 00 00 00 18 fc b8 e0 00  Error: UNC 1 sectors at LBA = 0x0018fcb8 = 1637560

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 01 00 00 00 18 fc b8 e0 00     01:47:52.563  READ DMA EXT
  25 00 00 00 01 00 00 00 18 fc b7 e0 00     01:47:49.750  READ DMA EXT
  25 00 00 00 01 00 00 00 18 fc b6 e0 00     01:47:49.750  READ DMA EXT
  25 00 00 00 01 00 00 00 18 fc b5 e0 00     01:47:49.750  READ DMA EXT
  25 00 00 00 01 00 00 00 18 fc b4 e0 00     01:47:49.750  READ DMA EXT

Error 73 [0] occurred at disk power-on lifetime: 11641 hours (485 days + 1 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 20 00 00 00 18 fc a0 e0 00  Error: UNC 32 sectors at LBA = 0x0018fca0 = 1637536

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 20 00 00 00 18 fc a0 e0 00     01:47:49.625  READ DMA EXT
  25 00 00 00 08 00 00 0e df 91 e0 e0 00     01:47:46.813  READ DMA EXT
  35 00 00 00 18 00 00 00 f1 c1 88 e0 00     01:47:46.750  WRITE DMA EXT
  25 00 00 00 18 00 00 01 e9 27 50 e0 00     01:47:46.750  READ DMA EXT
  35 00 00 00 10 00 00 00 f1 c1 78 e0 00     01:47:46.750  WRITE DMA EXT

Error 72 [7] occurred at disk power-on lifetime: 11623 hours (484 days + 7 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 01 00 00 00 18 fc b8 e0 00  Error: UNC 1 sectors at LBA = 0x0018fcb8 = 1637560

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 01 00 00 00 18 fc b8 e0 00     05:40:00.938  READ DMA EXT
  25 00 00 00 01 00 00 00 18 fc b7 e0 00     05:39:58.125  READ DMA EXT
  25 00 00 00 01 00 00 00 18 fc b6 e0 00     05:39:58.125  READ DMA EXT
  25 00 00 00 01 00 00 00 18 fc b5 e0 00     05:39:58.125  READ DMA EXT
  25 00 00 00 01 00 00 00 18 fc b4 e0 00     05:39:58.125  READ DMA EXT

Error 71 [6] occurred at disk power-on lifetime: 11623 hours (484 days + 7 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 20 00 00 00 18 fc a0 e0 00  Error: UNC 32 sectors at LBA = 0x0018fca0 = 1637536

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 20 00 00 00 18 fc a0 e0 00     05:39:57.813  READ DMA EXT
  25 00 00 00 08 00 00 01 56 5e 58 e0 00     05:39:54.938  READ DMA EXT
  25 00 00 00 08 00 00 22 e1 ff 68 e0 00     05:39:54.938  READ DMA EXT
  35 00 00 00 18 00 00 01 05 85 c0 e0 00     05:39:54.938  WRITE DMA EXT
  25 00 00 00 18 00 00 00 32 44 08 e0 00     05:39:54.938  READ DMA EXT

Error 70 [5] occurred at disk power-on lifetime: 11599 hours (483 days + 7 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 01 00 00 00 18 fc b8 e0 00  Error: UNC 1 sectors at LBA = 0x0018fcb8 = 1637560

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 01 00 00 00 18 fc b8 e0 00     02:50:02.938  READ DMA EXT
  25 00 00 00 01 00 00 00 18 fc b7 e0 00     02:50:00.125  READ DMA EXT
  25 00 00 00 01 00 00 00 18 fc b6 e0 00     02:50:00.125  READ DMA EXT
  25 00 00 00 01 00 00 00 18 fc b5 e0 00     02:50:00.125  READ DMA EXT
  25 00 00 00 01 00 00 00 18 fc b4 e0 00     02:50:00.125  READ DMA EXT

SMART Extended Self-test Log (GP Log 0x07) not supported

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%      7720         -

SMART Selective self-test log data structure revision number 0
Note: revision number not 1 implies that no selective self-test has ever been run
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       256 (0x0100)
Device State:                        Active (0)
Current Temperature:                    29 Celsius
Power Cycle Min/Max Temperature:     20/28 Celsius
Lifetime    Min/Max Temperature:      7/47 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:     -4/72 Celsius
Min/Max Temperature Limit:           -9/77 Celsius
Temperature History Size (Index):    128 (94)

SCT Error Recovery Control:
           Read: Disabled
          Write: Disabled

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x0002  2            0  R_ERR response for data FIS
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0005  2            0  R_ERR response for non-data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x0008  2            0  Device-to-host non-data FIS retries
0x0009  2            0  Transition from drive PhyRdy to drive PhyNRdy
0x000a  2            5  Device-to-host register FISes sent due to a COMRESET
0x000b  2            0  CRC errors within host-to-device FIS
0x000d  2            0  Non-CRC errors within host-to-device FIS
0x000f  2            0  R_ERR response for host-to-device data FIS, CRC
0x0010  2            0  R_ERR response for host-to-device data FIS, non-CRC
0x0012  2            0  R_ERR response for host-to-device non-data FIS, CRC
0x0013  2            0  R_ERR response for host-to-device non-data FIS, non-CRC
0x8001  2            0  Vendor specific



