smartctl 7.1 2019-12-30 r5022 [FreeBSD 12.1-RELEASE amd64] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Apple SD/SM/TS...E/F/G SSDs
Device Model:     APPLE SSD SM256E
Serial Number:    --
LU WWN Device Id: 5 002538 ...
Firmware Version: CXM09A1Q
User Capacity:    251,000,193,024 bytes [251 GB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Rotation Rate:    Solid State Device
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA8-ACS T13/1699-D revision 4c
SATA Version is:  SATA 3.0, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Wed Sep 23 04:17:00 2020 AEST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Disabled
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x02)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  960) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  16) minutes.

SMART Attributes Data Structure revision number: 1
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     -O-RC-   198   198   000    -    64
  5 Reallocated_Sector_Ct   PO--CK   098   098   000    -    122
  9 Power_On_Hours          -O--CK   096   096   000    -    19437
 12 Power_Cycle_Count       -O--CK   094   094   000    -    5921
169 Unknown_Apple_Attrib    PO--C-   253   253   010    -    2319710165248
173 Wear_Leveling_Count     -O--CK   184   184   100    -    1172558446982
192 Power-Off_Retract_Count -O--C-   098   098   000    -    5652
194 Temperature_Celsius     -O---K   060   035   000    -    40 (Min/Max 14/70)
197 Current_Pending_Sector  -O---K   100   100   000    -    0
199 UDMA_CRC_Error_Count    -O-RC-   200   200   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01       GPL,SL  R/O      1  Summary SMART error log
0x02       GPL,SL  R/O      2  Comprehensive SMART error log
0x03       GPL,SL  R/O      2  Ext. Comprehensive SMART error log
0x06       GPL,SL  R/O      1  SMART self-test log
0x07       GPL,SL  R/O      2  Extended self-test log
0x09       GPL,SL  R/W      1  Selective self-test log
0x10       GPL,SL  R/O      1  NCQ Command Error log
0x11       GPL,SL  R/O      1  SATA Phy Event Counters log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log

SMART Extended Comprehensive Error Log Version: 1 (2 sectors)
Device Error Count: 65535 (device log contains only the most recent 8 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Warning! SMART Extended Comprehensive Error Log Structure error: invalid SMART checksum.
Error 65535 [5] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 80 00 08 00 00 00 00 00 00 00 00   8 sectors at LBA = 0x00000000 = 0

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT

Error 65534 [4] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 80 00 08 00 00 00 00 00 00 00 00   8 sectors at LBA = 0x00000000 = 0

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT

Error 65533 [3] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 80 00 08 00 00 00 00 00 00 00 00   8 sectors at LBA = 0x00000000 = 0

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT

Error 65532 [2] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 80 00 08 00 00 00 00 00 00 00 00   8 sectors at LBA = 0x00000000 = 0

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT

Error 65531 [1] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 80 00 08 00 00 00 00 00 00 00 00   8 sectors at LBA = 0x00000000 = 0

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 0c 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT

Error 65530 [0] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 80 00 08 00 00 00 00 00 00 00 00   8 sectors at LBA = 0x00000000 = 0

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 0c 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 0c 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT

Error 65529 [7] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 80 00 08 00 00 00 00 00 00 00 00   8 sectors at LBA = 0x00000000 = 0

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 0c 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 0c 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 0c 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT

Error 65528 [6] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 80 00 08 00 00 00 00 00 00 00 00   8 sectors at LBA = 0x00000000 = 0

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 0c 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 08 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 0c 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 0c 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT
  25 00 00 00 0c 00 00 00 00 00 00 00 00     00:06:45.000  READ DMA EXT

SMART Extended Self-test Log Version: 1 (2 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Commands not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x0002  2        49152  R_ERR response for data FIS
0x0003  2        53248  R_ERR response for device-to-host data FIS
0x0004  2        57344  R_ERR response for host-to-device data FIS
0x0005  2         7952  R_ERR response for non-data FIS
0x0006  2         2562  R_ERR response for device-to-host non-data FIS
0x0007  2         4096  R_ERR response for host-to-device non-data FIS
0x0008  2         7952  Device-to-host non-data FIS retries
0x0009  2         7953  Transition from drive PhyRdy to drive PhyNRdy
0x000a  2         4268  Device-to-host register FISes sent due to a COMRESET
0x000b  2         6145  CRC errors within host-to-device FIS
0x000d  2         7953  Non-CRC errors within host-to-device FIS
0x000f  2         8176  R_ERR response for host-to-device data FIS, CRC
0x0010  2           15  R_ERR response for host-to-device data FIS, non-CRC
0x0012  2        49153  R_ERR response for host-to-device non-data FIS, CRC
0x0013  2        12112  R_ERR response for host-to-device non-data FIS, non-CRC

