smartctl 7.2 2020-12-30 r5155 [FreeBSD 13.0-RELEASE amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Western Digital Scorpio Blue Serial ATA
Device Model:     WDC WD3200BEVT-60A23T0
Serial Number:    --
LU WWN Device Id: 5 0014ee ...
Firmware Version: 02.01A02
User Capacity:    320,072,933,376 bytes [320 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    5400 rpm
Form Factor:      2.5 inches
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA8-ACS (minor revision not indicated)
SATA Version is:  SATA 2.6, 3.0 Gb/s
Local Time is:    Fri Dec 23 10:24:32 2022 EST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     128 (minimum power consumption without standby)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		( 8160) seconds.
Offline data collection
capabilities: 			 (0x51) SMART execute Offline immediate.
					No Auto Offline data collection support.
					Suspend Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  97) minutes.
SCT capabilities: 	       (0x703f)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR-K   200   200   051    -    0
  3 Spin_Up_Time            POS--K   154   145   021    -    1291
  4 Start_Stop_Count        -O--CK   094   094   000    -    6186
  5 Reallocated_Sector_Ct   PO--CK   200   200   140    -    0
  7 Seek_Error_Rate         POSR-K   100   253   051    -    0
  9 Power_On_Hours          -O--CK   087   087   000    -    9719
 10 Spin_Retry_Count        PO--CK   100   100   051    -    0
 11 Calibration_Retry_Count -O--CK   100   100   000    -    0
 12 Power_Cycle_Count       -O--CK   094   094   000    -    6158
183 Runtime_Bad_Block       -O--CK   100   100   000    -    0
187 Reported_Uncorrect      -O--CK   100   095   000    -    7
188 Command_Timeout         -O--CK   100   094   000    -    8590065677
190 Airflow_Temperature_Cel -O---K   065   048   040    -    35 (Min/Max 17/35)
191 G-Sense_Error_Rate      -O--CK   001   001   000    -    4372
192 Power-Off_Retract_Count -O--CK   200   200   000    -    714
193 Load_Cycle_Count        -O--CK   001   001   000    -    1055709
194 Temperature_Celsius     -O---K   108   091   000    -    35
196 Reallocated_Event_Count -O--CK   200   200   000    -    0
197 Current_Pending_Sector  -O--CK   200   200   000    -    0
198 Offline_Uncorrectable   ----CK   100   253   000    -    0
199 UDMA_CRC_Error_Count    -O--CK   200   200   000    -    0
200 Multi_Zone_Error_Rate   P--R--   100   253   051    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      6  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa0-0xa7  GPL,SL  VS      16  Device vendor specific log
0xa8-0xb7  GPL,SL  VS       1  Device vendor specific log
0xbd       GPL,SL  VS       1  Device vendor specific log
0xc0       GPL,SL  VS       1  Device vendor specific log
0xc1       GPL     VS      24  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (6 sectors)
Device Error Count: 9
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 9 [8] occurred at disk power-on lifetime: 3246 hours (135 days + 6 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 08 00 00 06 6e 54 60 40 00  Error: WP at LBA = 0x066e5460 = 107893856

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 08 00 c8 00 00 00 0c ea 78 40 00     00:16:10.456  WRITE FPDMA QUEUED
  61 00 01 00 c0 00 00 08 89 7d 09 40 00     00:16:10.456  WRITE FPDMA QUEUED
  60 00 08 00 b8 00 00 00 6d 13 58 40 00     00:16:10.456  READ FPDMA QUEUED
  60 00 08 00 b0 00 00 06 6e 54 60 40 00     00:16:10.456  READ FPDMA QUEUED
  61 00 30 00 a8 00 00 01 db fa a0 40 00     00:16:10.456  WRITE FPDMA QUEUED

Error 8 [7] occurred at disk power-on lifetime: 3246 hours (135 days + 6 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 00 00 00 00 a7 f7 df 38 a7 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  ea 00 00 00 00 00 00 00 00 00 00 e0 00     00:16:01.709  FLUSH CACHE EXT
  61 00 08 00 90 00 00 00 46 93 00 40 00     00:16:01.653  WRITE FPDMA QUEUED
  61 00 08 00 88 00 00 00 66 e6 30 40 00     00:16:01.652  WRITE FPDMA QUEUED
  60 00 01 00 80 00 00 08 89 7d 09 40 00     00:16:01.652  READ FPDMA QUEUED
  60 00 01 00 78 00 00 02 60 9a 80 40 00     00:16:01.652  READ FPDMA QUEUED

Error 7 [6] occurred at disk power-on lifetime: 3246 hours (135 days + 6 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 01 00 00 00 15 46 f8 40 00  Error: UNC at LBA = 0x001546f8 = 1394424

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 01 00 28 00 00 02 60 0d 68 40 00     00:15:52.859  READ FPDMA QUEUED
  60 00 01 00 20 00 00 00 15 46 f8 40 00     00:15:52.854  READ FPDMA QUEUED
  60 00 01 00 f8 00 00 00 0c 88 00 40 00     00:15:52.792  READ FPDMA QUEUED
  60 00 01 00 f0 00 00 01 f9 32 78 40 00     00:15:52.792  READ FPDMA QUEUED
  61 00 08 00 18 00 00 00 0c ea 80 40 00     00:15:52.792  WRITE FPDMA QUEUED

Error 6 [5] occurred at disk power-on lifetime: 3246 hours (135 days + 6 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 00 00 00 00 a7 f7 df 38 a7 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  ea 00 00 00 00 00 00 00 00 00 00 e0 00     00:15:44.297  FLUSH CACHE EXT
  61 00 10 00 e0 00 00 00 66 e5 b0 40 00     00:15:44.287  WRITE FPDMA QUEUED
  61 00 08 00 d8 00 00 00 46 9c 90 40 00     00:15:44.286  WRITE FPDMA QUEUED
  61 00 08 00 d0 00 00 00 46 9c 60 40 00     00:15:44.286  WRITE FPDMA QUEUED
  61 00 08 00 c8 00 00 00 46 9b c0 40 00     00:15:44.286  WRITE FPDMA QUEUED

Error 5 [4] occurred at disk power-on lifetime: 3246 hours (135 days + 6 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 40 00 00 00 6d a4 08 40 00  Error: WP at LBA = 0x006da408 = 7185416

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 08 00 f8 00 00 03 69 b2 08 40 00     00:15:31.828  WRITE FPDMA QUEUED
  61 00 08 00 f0 00 00 00 43 6a 18 40 00     00:15:31.828  WRITE FPDMA QUEUED
  60 00 28 00 38 00 00 00 16 8d c2 40 00     00:15:31.828  READ FPDMA QUEUED
  60 00 08 00 30 00 00 06 cf c9 50 40 00     00:15:31.828  READ FPDMA QUEUED
  60 00 08 00 28 00 00 00 6d a4 08 40 00     00:15:31.828  READ FPDMA QUEUED

Error 4 [3] occurred at disk power-on lifetime: 3246 hours (135 days + 6 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 10 00 00 07 34 27 38 40 00  Error: UNC at LBA = 0x07342738 = 120858424

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 08 00 e8 00 00 06 cf c9 50 40 00     00:14:45.733  READ FPDMA QUEUED
  61 00 10 00 e0 00 00 00 7c 1b e0 40 00     00:14:45.733  WRITE FPDMA QUEUED
  61 00 20 00 d8 00 00 00 7e 26 00 40 00     00:14:45.733  WRITE FPDMA QUEUED
  60 00 01 00 d0 00 00 00 0b 66 80 40 00     00:14:45.733  READ FPDMA QUEUED
  60 00 10 00 c8 00 00 02 4f 97 10 40 00     00:14:45.733  READ FPDMA QUEUED

Error 3 [2] occurred at disk power-on lifetime: 3246 hours (135 days + 6 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 c8 00 00 00 0b 66 80 40 00  Error: UNC at LBA = 0x000b6680 = 747136

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 10 00 40 00 00 02 4f 97 10 40 00     00:14:15.874  READ FPDMA QUEUED
  60 00 01 00 38 00 00 00 0b 66 80 40 00     00:14:15.874  READ FPDMA QUEUED
  60 00 c8 00 30 00 00 04 2d 38 e8 40 00     00:14:15.874  READ FPDMA QUEUED
  61 00 08 00 28 00 00 00 66 e5 b8 40 00     00:14:15.874  WRITE FPDMA QUEUED
  ea 00 00 00 00 00 00 00 00 00 00 e0 00     00:14:15.681  FLUSH CACHE EXT

Error 2 [1] occurred at disk power-on lifetime: 1288 hours (53 days + 16 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 08 00 00 00 81 f6 40 40 00  Error: UNC at LBA = 0x0081f640 = 8517184

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 01 00 00 30 00 00 00 81 f6 40 40 00     00:05:27.979  READ FPDMA QUEUED
  60 00 08 00 28 00 00 00 b7 fc e0 40 00     00:05:25.751  READ FPDMA QUEUED
  ea 00 00 00 00 00 00 00 00 00 00 e0 00     00:05:24.228  FLUSH CACHE EXT
  61 00 08 00 18 00 00 00 53 4a d8 40 00     00:05:24.151  WRITE FPDMA QUEUED
  ea 00 00 00 00 00 00 00 00 00 00 e0 00     00:05:23.449  FLUSH CACHE EXT

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%      3319         -
# 2  Short offline       Completed without error       00%      3319         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       258 (0x0102)
Device State:                        Active (0)
Current Temperature:                    34 Celsius
Power Cycle Min/Max Temperature:     17/34 Celsius
Lifetime    Min/Max Temperature:     18/52 Celsius
Under/Over Temperature Limit Count:   0/0
Vendor specific:
01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      0/60 Celsius
Min/Max Temperature Limit:           -41/85 Celsius
Temperature History Size (Index):    128 (15)

SCT Error Recovery Control:
           Read:     85 (8.5 seconds)
          Write:     85 (8.5 seconds)

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x0002  2            0  R_ERR response for data FIS
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0005  2            0  R_ERR response for non-data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x000a  2            4  Device-to-host register FISes sent due to a COMRESET
0x000b  2            0  CRC errors within host-to-device FIS
0x8000  4         2312  Vendor specific

