smartctl 7.3 2022-02-28 r5338 [FreeBSD 13.1-RELEASE amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     SAMSUNG SpinPoint F2 EG
Device Model:     SAMSUNG HD154UI
Serial Number:    --
LU WWN Device Id: 5 0024e9 ...
Firmware Version: 1AG01118
User Capacity:    1,500,301,910,016 bytes [1.50 TB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database 7.3/5319
ATA Version is:   ATA/ATAPI-7, ATA8-ACS T13/1699-D revision 3b
Local Time is:    Tue Jun 21 11:33:50 2022 CEST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Disabled
APM feature is:   Disabled
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(18645) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 ( 312) minutes.
Conveyance self-test routine
recommended polling time: 	 (  33) minutes.
SCT capabilities: 	       (0x003f)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   100   100   051    -    11
  3 Spin_Up_Time            POS---   063   063   011    -    11860
  4 Start_Stop_Count        -O--CK   100   100   000    -    110
  5 Reallocated_Sector_Ct   PO--CK   064   064   010    -    1582
  7 Seek_Error_Rate         POSR--   100   100   051    -    0
  8 Seek_Time_Performance   P-S--K   100   100   015    -    11352
  9 Power_On_Hours          -O--CK   083   083   000    -    87013
 10 Spin_Retry_Count        PO--CK   100   100   051    -    0
 11 Calibration_Retry_Count -O--C-   100   100   000    -    0
 12 Power_Cycle_Count       -O--CK   100   100   000    -    110
 13 Read_Soft_Error_Rate    -OSR--   100   100   000    -    11
183 Runtime_Bad_Block       -O--CK   100   100   000    -    0
184 End-to-End_Error        PO--CK   100   100   000    -    0
187 Reported_Uncorrect      -O--CK   100   100   000    -    36
188 Command_Timeout         -O--CK   100   100   000    -    0
190 Airflow_Temperature_Cel -O---K   068   065   000    -    32 (Min/Max 17/32)
194 Temperature_Celsius     -O---K   066   064   000    -    34 (Min/Max 8/44)
195 Hardware_ECC_Recovered  -O-RC-   100   100   000    -    1260382509
196 Reallocated_Event_Count -O--CK   062   062   000    -    1582
197 Current_Pending_Sector  -O--C-   100   100   000    -    0
198 Offline_Uncorrectable   ----CK   100   100   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   099   099   000    -    658
200 Multi_Zone_Error_Rate   -O-R--   099   099   000    -    512
201 Soft_Read_Error_Rate    -O-R--   100   100   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      2  Comprehensive SMART error log
0x03       GPL     R/O      2  Ext. Comprehensive SMART error log
0x04       GPL     R/O      2  Device Statistics log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      2  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x20       GPL     R/O      2  Streaming performance log [OBS-8]
0x21       GPL     R/O      1  Write stream error log
0x22       GPL     R/O      1  Read stream error log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (2 sectors)
Device Error Count: 663 (device log contains only the most recent 8 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 663 [6] occurred at disk power-on lifetime: 57077 hours (2378 days + 5 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  00 -- 80 00 01 00 00 00 00 00 01 a0 00   1 sectors at LBA = 0x00000001 = 1

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  35 00 00 00 ab 00 00 8e 15 6f 86 40 08 10d+01:48:58.564  WRITE DMA EXT
  61 00 00 00 1c 00 00 ff 02 a4 9c 40 00 10d+01:48:58.554  WRITE FPDMA QUEUED
  61 00 00 00 0f 00 00 00 39 0d 2d 40 00 10d+01:48:58.554  WRITE FPDMA QUEUED
  61 00 00 00 01 00 00 00 05 78 21 40 00 10d+01:48:58.554  WRITE FPDMA QUEUED
  61 00 00 00 02 00 00 00 05 65 01 40 00 10d+01:48:58.554  WRITE FPDMA QUEUED

Error 662 [5] occurred at disk power-on lifetime: 57077 hours (2378 days + 5 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  00 -- 80 00 01 00 00 00 00 00 01 a0 00   1 sectors at LBA = 0x00000001 = 1

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  35 00 00 00 ab 00 00 30 4c 40 78 40 08 10d+01:47:15.884  WRITE DMA EXT
  61 00 00 00 1e 00 00 00 40 c7 ae 40 00 10d+01:47:15.874  WRITE FPDMA QUEUED
  61 00 00 00 02 00 00 00 40 72 ab 40 00 10d+01:47:15.874  WRITE FPDMA QUEUED
  61 00 00 00 1c 00 00 00 03 20 5a 40 00 10d+01:47:15.874  WRITE FPDMA QUEUED
  61 00 00 00 02 00 00 00 3d 14 75 40 00 10d+01:47:15.874  WRITE FPDMA QUEUED

Error 661 [4] occurred at disk power-on lifetime: 47573 hours (1982 days + 5 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  00 -- 48 00 32 00 00 6f 01 e8 8b 40 00   at LBA = 0x6f01e88b = 1862396043

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 ab 00 00 00 01 e8 12 40 00     00:14:29.670  WRITE FPDMA QUEUED
  61 00 00 01 00 00 00 00 01 e7 12 40 00     00:14:29.660  WRITE FPDMA QUEUED
  61 00 00 00 56 00 00 00 01 c4 3c 40 00     00:14:29.650  WRITE FPDMA QUEUED
  ea 00 00 00 00 00 00 00 00 00 00 40 08     00:14:24.950  FLUSH CACHE EXT
  61 00 00 00 02 00 00 ff a8 3a a2 40 00     00:14:24.950  WRITE FPDMA QUEUED

Error 660 [3] occurred at disk power-on lifetime: 47573 hours (1982 days + 5 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  00 -- 4a 00 00 00 00 75 04 c1 6d 40 00   at LBA = 0x7504c16d = 1963245933

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 21 00 00 00 05 bc 0a 40 00  6d+15:14:52.004  READ FPDMA QUEUED
  60 00 00 00 0b 00 00 00 04 c1 64 40 00  6d+15:14:52.004  READ FPDMA QUEUED
  60 00 00 00 08 00 00 00 04 bc 56 40 00  6d+15:14:51.984  READ FPDMA QUEUED
  60 00 00 00 02 00 00 00 03 fc f4 40 00  6d+15:14:51.984  READ FPDMA QUEUED
  60 00 00 00 02 00 00 00 03 7b aa 40 00  6d+15:14:51.984  READ FPDMA QUEUED

Error 659 [2] occurred at disk power-on lifetime: 45144 hours (1881 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  00 -- 4a 00 34 00 00 56 05 6c 23 40 00   at LBA = 0x56056c23 = 1443195939

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 55 00 00 00 05 6c 02 40 00 37d+18:12:36.188  READ FPDMA QUEUED
  60 00 00 00 55 00 00 00 05 6a ac 40 00 37d+18:12:36.168  READ FPDMA QUEUED
  60 00 00 00 55 00 00 00 05 6a 01 40 00 37d+18:12:36.168  READ FPDMA QUEUED
  60 00 00 00 56 00 00 00 05 69 00 40 00 37d+18:12:36.158  READ FPDMA QUEUED
  60 00 00 00 55 00 00 00 05 67 55 40 00 37d+18:12:36.148  READ FPDMA QUEUED

Error 658 [1] occurred at disk power-on lifetime: 41051 hours (1710 days + 11 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  00 -- 4a 00 35 00 00 45 16 f6 ef 40 00   at LBA = 0x4516f6ef = 1159132911

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 56 00 00 00 16 f6 ce 40 00 19d+13:37:44.670  READ FPDMA QUEUED
  60 00 00 00 56 00 00 00 16 f6 23 40 00 19d+13:37:44.670  READ FPDMA QUEUED
  60 00 00 00 55 00 00 00 16 f5 ce 40 00 19d+13:37:44.660  READ FPDMA QUEUED
  60 00 00 00 56 00 00 00 16 f5 78 40 00 19d+13:37:44.660  READ FPDMA QUEUED
  60 00 00 00 55 00 00 00 16 f5 23 40 00 19d+13:37:44.660  READ FPDMA QUEUED

Error 657 [0] occurred at disk power-on lifetime: 33362 hours (1390 days + 2 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  00 -- 4a 00 04 00 00 51 06 8e 5a 40 00   at LBA = 0x51068e5a = 1359384154

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 55 00 00 00 06 8e 09 40 00  1d+21:38:39.590  READ FPDMA QUEUED
  ea 00 00 00 00 00 00 00 00 00 00 40 08  1d+21:38:38.390  FLUSH CACHE EXT
  61 00 00 00 02 00 00 ff a8 3a a0 40 00  1d+21:38:38.390  WRITE FPDMA QUEUED
  61 00 00 00 02 00 00 ff a8 38 a0 40 00  1d+21:38:38.390  WRITE FPDMA QUEUED
  61 00 00 00 02 00 00 00 00 04 a0 40 00  1d+21:38:38.390  WRITE FPDMA QUEUED

Error 656 [7] occurred at disk power-on lifetime: 33361 hours (1390 days + 1 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  00 -- 4a 00 24 00 00 53 1a 35 33 40 00   at LBA = 0x531a3533 = 1394226483

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 55 00 00 00 1a 35 02 40 00  1d+20:58:07.160  READ FPDMA QUEUED
  ea 00 00 00 00 00 00 00 00 00 00 40 08  1d+20:58:05.460  FLUSH CACHE EXT
  61 00 00 00 02 00 00 ff a8 3a e0 40 00  1d+20:58:05.460  WRITE FPDMA QUEUED
  61 00 00 00 02 00 00 ff a8 38 e0 40 00  1d+20:58:05.460  WRITE FPDMA QUEUED
  61 00 00 00 02 00 00 00 00 04 e0 40 00  1d+20:58:05.460  WRITE FPDMA QUEUED

SMART Extended Self-test Log Version: 1 (2 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%     10942         -
# 2  Short offline       Completed without error       00%         5         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  2
SCT Version (vendor specific):       256 (0x0100)
Device State:                        Active (0)
Current Temperature:                    34 Celsius
Power Cycle Min/Max Temperature:     --/44 Celsius
Lifetime    Min/Max Temperature:     --/46 Celsius

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:     -4/72 Celsius
Min/Max Temperature Limit:           -9/77 Celsius
Temperature History Size (Index):    128 (126)

SCT Error Recovery Control:
           Read: Disabled
          Write: Disabled

ATA_READ_LOG_EXT (addr=0x04:0x00, page=0, n=1) failed: Input/output error
Read Device Statistics page 0x00 failed

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2           13  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0002  2            0  R_ERR response for data FIS
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0005  2            0  R_ERR response for non-data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x0008  2            0  Device-to-host non-data FIS retries
0x0009  2           19  Transition from drive PhyRdy to drive PhyNRdy
0x000b  2            0  CRC errors within host-to-device FIS
0x000d  2            0  Non-CRC errors within host-to-device FIS
0x000f  2            0  R_ERR response for host-to-device data FIS, CRC
0x0010  2            0  R_ERR response for host-to-device data FIS, non-CRC
0x0012  2            0  R_ERR response for host-to-device non-data FIS, CRC
0x0013  2            0  R_ERR response for host-to-device non-data FIS, non-CRC



