smartctl 7.3 2022-02-28 r5338 [FreeBSD 12.3-STABLE amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Laptop HDD
Device Model:     ST500LT012-1DG142
Serial Number:    --
LU WWN Device Id: 5 000c50 ...
Firmware Version: 0002LVM1
User Capacity:    500,107,862,016 bytes [500 GB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Rotation Rate:    5400 rpm
Form Factor:      2.5 inches
Device is:        In smartctl database 7.3/5319
ATA Version is:   ATA8-ACS T13/1699-D revision 4
SATA Version is:  SATA 3.0, 6.0 Gb/s (current: 3.0 Gb/s)
Local Time is:    Sat Apr 30 22:22:05 2022 UTC
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     128 (minimum power consumption without standby)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(    0) seconds.
Offline data collection
capabilities: 			 (0x73) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 ( 104) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x1031)	SCT Status supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   113   086   034    -    57963576
  3 Spin_Up_Time            PO----   099   099   000    -    0
  4 Start_Stop_Count        -O--CK   096   096   020    -    4102
  5 Reallocated_Sector_Ct   PO--CK   100   100   036    -    0
  7 Seek_Error_Rate         POSR--   077   060   030    -    52196193
  9 Power_On_Hours          -O--CK   095   095   000    -    4666
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   097   097   020    -    3506
184 End-to-End_Error        -O--CK   100   100   099    -    0
187 Reported_Uncorrect      -O--CK   001   001   000    -    1769
188 Command_Timeout         -O--CK   100   099   000    -    17180131345
189 High_Fly_Writes         -O-RCK   100   100   000    -    0
190 Airflow_Temperature_Cel -O---K   064   055   045    -    36 (Min/Max 24/40)
191 G-Sense_Error_Rate      -O--CK   100   100   000    -    104
192 Power-Off_Retract_Count -O--CK   100   100   000    -    2
193 Load_Cycle_Count        -O--CK   001   001   000    -    198851
194 Temperature_Celsius     -O---K   036   045   000    -    36 (0 14 0 0 0)
197 Current_Pending_Sector  -O--C-   100   100   000    -    0
198 Offline_Uncorrectable   ----C-   100   100   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    17
254 Free_Fall_Sensor        -O--CK   100   100   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      5  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x21       GPL     R/O      1  Write stream error log
0x22       GPL     R/O      1  Read stream error log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS      20  Device vendor specific log
0xa2       GPL     VS    2248  Device vendor specific log
0xa8       GPL,SL  VS      65  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xab       GPL     VS       1  Device vendor specific log
0xb0       GPL     VS    2864  Device vendor specific log
0xbd-0xbf  GPL     VS   65535  Device vendor specific log
0xc0       GPL,SL  VS       1  Device vendor specific log
0xc1       GPL,SL  VS      10  Device vendor specific log
0xc3       GPL,SL  VS       8  Device vendor specific log
0xc4       GPL,SL  VS      18  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 1769 (device log contains only the most recent 20 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 1769 [8] occurred at disk power-on lifetime: 3575 hours (148 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 0a d4 58 10 00 00  Error: WP at LBA = 0x0ad45810 = 181688336

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 08 00 00 13 59 7c b8 40 00     04:24:19.763  WRITE FPDMA QUEUED
  61 00 00 00 10 00 00 01 d4 fa 90 40 00     04:24:19.762  WRITE FPDMA QUEUED
  61 00 00 00 10 00 00 13 59 c0 50 40 00     04:24:19.762  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 02 d2 d8 c8 40 00     04:24:19.762  WRITE FPDMA QUEUED
  61 00 00 00 20 00 00 13 5a 84 e0 40 00     04:24:19.761  WRITE FPDMA QUEUED

Error 1768 [7] occurred at disk power-on lifetime: 3575 hours (148 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 0a d4 58 10 00 00  Error: UNC at LBA = 0x0ad45810 = 181688336

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 00 0a d4 58 10 40 00     04:24:16.874  READ FPDMA QUEUED
  60 00 00 00 08 00 00 0a d7 a0 48 40 00     04:24:16.860  READ FPDMA QUEUED
  60 00 00 00 10 00 00 0a e3 4d c0 40 00     04:24:16.834  READ FPDMA QUEUED
  60 00 00 00 08 00 00 0a d4 f2 e0 40 00     04:24:16.817  READ FPDMA QUEUED
  60 00 00 00 08 00 00 0a d5 db 58 40 00     04:24:16.795  READ FPDMA QUEUED

Error 1767 [6] occurred at disk power-on lifetime: 3575 hours (148 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 0a d4 58 10 00 00  Error: UNC at LBA = 0x0ad45810 = 181688336

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 00 0a d4 58 10 40 00     04:22:32.093  READ FPDMA QUEUED
  ef 00 10 00 03 00 00 00 00 00 00 a0 00     04:22:32.070  SET FEATURES [Enable SATA feature]
  27 00 00 00 00 00 00 00 00 00 00 e0 00     04:22:32.044  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 00 00 00 00 00 00 00 00 00 00 a0 00     04:22:32.043  IDENTIFY DEVICE
  ef 00 03 00 46 00 00 00 00 00 00 a0 00     04:22:32.031  SET FEATURES [Set transfer mode]

Error 1766 [5] occurred at disk power-on lifetime: 3575 hours (148 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 0a d4 58 10 00 00  Error: WP at LBA = 0x0ad45810 = 181688336

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 02 58 00 00 13 57 56 00 40 00     04:22:29.132  WRITE FPDMA QUEUED
  61 00 00 00 38 00 00 13 57 55 c0 40 00     04:22:29.132  WRITE FPDMA QUEUED
  61 00 00 01 70 00 00 13 57 54 40 40 00     04:22:29.131  WRITE FPDMA QUEUED
  61 00 00 00 78 00 00 13 57 53 c0 40 00     04:22:29.130  WRITE FPDMA QUEUED
  61 00 00 00 78 00 00 13 57 53 40 40 00     04:22:29.130  WRITE FPDMA QUEUED

Error 1765 [4] occurred at disk power-on lifetime: 3575 hours (148 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 0a d4 58 10 00 00  Error: WP at LBA = 0x0ad45810 = 181688336

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 08 00 00 1e 95 08 28 40 00     03:37:26.692  WRITE FPDMA QUEUED
  61 00 00 08 90 00 00 08 d1 53 70 40 00     03:37:26.692  WRITE FPDMA QUEUED
  60 00 00 00 08 00 00 0a d4 58 10 40 00     03:37:26.691  READ FPDMA QUEUED
  ea 00 00 00 00 00 00 00 00 00 00 a0 00     03:37:26.691  FLUSH CACHE EXT
  ef 00 10 00 03 00 00 00 00 00 00 a0 00     03:37:26.681  SET FEATURES [Enable SATA feature]

Error 1764 [3] occurred at disk power-on lifetime: 3575 hours (148 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 0a d4 58 10 00 00  Error: WP at LBA = 0x0ad45810 = 181688336

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 98 00 00 1e 95 07 90 40 00     03:37:23.710  WRITE FPDMA QUEUED
  61 00 00 0a 00 00 00 08 d1 49 70 40 00     03:37:23.710  WRITE FPDMA QUEUED
  60 00 00 00 08 00 00 0a d4 58 10 40 00     03:37:23.680  READ FPDMA QUEUED
  61 00 00 0a 00 00 00 08 d1 3f 70 40 00     03:37:23.680  WRITE FPDMA QUEUED
  61 00 00 06 30 00 00 08 d1 39 40 40 00     03:37:23.675  WRITE FPDMA QUEUED

Error 1763 [2] occurred at disk power-on lifetime: 3575 hours (148 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 0a d4 58 10 00 00  Error: WP at LBA = 0x0ad45810 = 181688336

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 08 b0 00 00 08 d1 27 60 40 00     03:37:20.722  WRITE FPDMA QUEUED
  61 00 00 00 28 00 00 11 94 c2 18 40 00     03:37:20.722  WRITE FPDMA QUEUED
  60 00 00 00 08 00 00 0a d4 58 10 40 00     03:37:20.722  READ FPDMA QUEUED
  ea 00 00 00 00 00 00 00 00 00 00 a0 00     03:37:20.721  FLUSH CACHE EXT
  ef 00 10 00 03 00 00 00 00 00 00 a0 00     03:37:20.712  SET FEATURES [Enable SATA feature]

Error 1762 [1] occurred at disk power-on lifetime: 3575 hours (148 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 0a d4 58 10 00 00  Error: UNC at LBA = 0x0ad45810 = 181688336

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 00 0a d4 58 10 40 00     03:37:17.858  READ FPDMA QUEUED
  61 00 00 00 08 00 00 1e 95 07 88 40 00     03:37:17.858  WRITE FPDMA QUEUED
  ea 00 00 00 00 00 00 00 00 00 00 a0 00     03:37:17.818  FLUSH CACHE EXT
  61 00 00 00 10 00 00 0a d4 62 70 40 00     03:37:17.818  WRITE FPDMA QUEUED
  61 00 00 01 48 00 00 1e 95 06 40 40 00     03:37:17.817  WRITE FPDMA QUEUED

SMART Extended Self-test Log Version: 1 (1 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       522 (0x020a)
Device State:                        Active (0)
Current Temperature:                    36 Celsius
Power Cycle Min/Max Temperature:     24/40 Celsius
Lifetime    Min/Max Temperature:     14/45 Celsius
Under/Over Temperature Limit Count:   0/42
Vendor specific:
00 00 00 00 00 00 00 00 00 00 02 00 00 00 00 00
00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        11 minutes
Min/Max recommended Temperature:      0/ 0 Celsius
Min/Max Temperature Limit:            0/ 0 Celsius
Temperature History Size (Index):    128 (4)

SCT Error Recovery Control command not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2           39  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS

