smartctl 7.1 2019-12-30 r5022 [FreeBSD 12.2-RELEASE amd64] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Fujitsu MHW BH
Device Model:     FUJITSU MHW2160BH
Serial Number:    --
LU WWN Device Id: 5 00000e ...
Firmware Version: 0000001C
User Capacity:    160,041,885,696 bytes [160 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA8-ACS T13/1699-D revision 3b
SATA Version is:  SATA 2.5, 1.5 Gb/s
Local Time is:    Thu Mar 11 10:32:54 2021 EST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM level is:     254 (maximum performance), recommended: 254
APM feature is:   Disabled
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  649) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  92) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x003d)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   100   079   046    -    65990
  2 Throughput_Performance  P-S---   100   100   030    -    39452672
  3 Spin_Up_Time            PO----   100   100   025    -    1
  4 Start_Stop_Count        -O--CK   098   098   000    -    9530
  5 Reallocated_Sector_Ct   PO--CK   090   090   024    -    386 (1749 251)
  7 Seek_Error_Rate         POSR--   100   100   047    -    1918
  8 Seek_Time_Performance   P-S---   100   100   019    -    0
  9 Power_On_Hours          -O--CK   078   078   000    -    11421
 10 Spin_Retry_Count        PO--C-   100   100   020    -    0
 12 Power_Cycle_Count       -O--CK   099   099   000    -    9244
192 Power-Off_Retract_Count -O--CK   092   092   000    -    2216
193 Load_Cycle_Count        -O--CK   093   093   000    -    156024
194 Temperature_Celsius     -O---K   100   060   000    -    34 (Min/Max -8/58)
195 Hardware_ECC_Recovered  -O-RC-   100   100   000    -    1073
196 Reallocated_Event_Count -O--CK   090   090   000    -    386 (9 6559)
197 Current_Pending_Sector  -O--C-   094   091   000    -    7
198 Offline_Uncorrectable   ----C-   015   015   000    -    170
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    0
200 Multi_Zone_Error_Rate   POSR--   100   100   060    -    32419
203 Run_Out_Cancel          -O----   100   100   000    -    3728286023068
240 Head_Flying_Hours       -OSRCK   200   200   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01       GPL,SL  R/O      1  Summary SMART error log
0x02       GPL,SL  R/O     51  Comprehensive SMART error log
0x03       GPL,SL  R/O     64  Ext. Comprehensive SMART error log
0x06       GPL,SL  R/O      1  SMART self-test log
0x07       GPL,SL  R/O      2  Extended self-test log
0x09       GPL,SL  R/W      1  Selective self-test log
0x10       GPL,SL  R/O      1  NCQ Command Error log
0x11       GPL,SL  R/O      1  SATA Phy Event Counters log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS       1  Device vendor specific log

SMART Extended Comprehensive Error Log Version: 1 (64 sectors)
Device Error Count: 33876 (device log contains only the most recent 256 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 33876 [83] occurred at disk power-on lifetime: 11322 hours (471 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 08 00 00 00 52 c1 28 e7 00  Error: UNC 8 sectors at LBA = 0x0752c128 = 122863912

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 08 00 00 00 52 c1 28 e7 00     02:34:25.050  READ DMA
  c8 00 00 00 10 00 00 00 3c c3 d8 e1 00     02:34:25.050  READ DMA
  c8 00 00 00 08 00 00 00 3c c3 c0 e1 00     02:34:25.050  READ DMA
  c8 00 00 00 08 00 00 00 3c c3 90 e1 00     02:34:25.050  READ DMA
  c8 00 00 00 08 00 00 00 3c c3 80 e1 00     02:34:25.018  READ DMA

Error 33875 [82] occurred at disk power-on lifetime: 11322 hours (471 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 08 00 00 00 52 c1 28 e7 00  Error: UNC 8 sectors at LBA = 0x0752c128 = 122863912

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 08 00 00 00 52 c1 28 e7 00     02:34:20.030  READ DMA
  c8 00 00 00 08 00 00 00 52 c1 20 e7 00     02:34:20.017  READ DMA
  c8 00 00 00 08 00 00 00 52 c1 18 e7 00     02:34:20.016  READ DMA
  c8 00 00 00 08 00 00 00 52 c1 10 e7 00     02:34:20.016  READ DMA
  c8 00 00 00 08 00 00 00 52 c1 08 e7 00     02:34:20.015  READ DMA

Error 33874 [81] occurred at disk power-on lifetime: 11322 hours (471 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 3a 00 00 07 52 cb c6 e0 00  Error: UNC 58 sectors at LBA = 0x0752cbc6 = 122866630

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 02 c0 00 00 07 52 c9 40 e0 00     02:34:14.625  READ DMA EXT
  ef 00 10 00 03 00 00 00 00 00 00 a0 00     02:34:14.624  SET FEATURES [Enable SATA feature]
  ef 00 10 00 02 00 00 00 00 00 00 a0 00     02:34:14.624  SET FEATURES [Enable SATA feature]
  27 00 00 00 00 00 00 00 00 00 00 e0 00     02:34:14.624  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  00 00 00 00 00 00 00 00 00 00 00 b0 00     02:34:14.622  NOP [Abort queued commands]

Error 33873 [80] occurred at disk power-on lifetime: 11322 hours (471 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 04 8e 00 00 07 52 c4 b2 e0 00  Error: UNC 1166 sectors at LBA = 0x0752c4b2 = 122864818

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 05 40 00 00 07 52 c4 00 e0 00     02:34:09.480  READ DMA EXT
  ef 00 10 00 03 00 00 00 00 00 00 a0 00     02:34:09.480  SET FEATURES [Enable SATA feature]
  ef 00 10 00 02 00 00 00 00 00 00 a0 00     02:34:09.480  SET FEATURES [Enable SATA feature]
  27 00 00 00 00 00 00 00 00 00 00 e0 00     02:34:09.480  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  00 00 00 00 00 00 00 00 00 00 00 b0 00     02:34:09.478  NOP [Abort queued commands]

Error 33872 [79] occurred at disk power-on lifetime: 11322 hours (471 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 02 d8 00 00 07 52 c1 28 e0 00  Error: UNC 728 sectors at LBA = 0x0752c128 = 122863912

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 04 00 00 00 07 52 c0 00 e0 00     02:34:04.503  READ DMA EXT
  25 00 00 05 10 00 00 07 52 ba f0 e0 00     02:34:04.484  READ DMA EXT
  25 00 00 06 f0 00 00 07 52 b4 00 e0 00     02:34:04.418  READ DMA EXT
  ca 00 00 00 30 00 00 00 06 dd e0 e0 00     02:34:04.418  WRITE DMA
  25 00 00 04 00 00 00 07 52 b0 00 e0 00     02:34:04.372  READ DMA EXT

Error 33871 [78] occurred at disk power-on lifetime: 11322 hours (471 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 05 00 00 00 12 e4 5b e7 00  Error: UNC 5 sectors at LBA = 0x0712e45b = 118678619

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 08 00 00 00 12 e4 58 e7 00     02:29:34.950  READ DMA
  ea 00 00 00 00 00 00 00 00 00 00 a0 00     02:29:34.939  FLUSH CACHE EXT
  ca 00 00 00 08 00 00 00 45 cc 08 e9 00     02:29:34.938  WRITE DMA
  ea 00 00 00 00 00 00 00 00 00 00 a0 00     02:29:34.922  FLUSH CACHE EXT
  ca 00 00 00 18 00 00 00 45 cb f0 e9 00     02:29:34.918  WRITE DMA

Error 33870 [77] occurred at disk power-on lifetime: 11322 hours (471 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 05 00 00 00 12 e4 5b e7 00  Error: UNC 5 sectors at LBA = 0x0712e45b = 118678619

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 08 00 00 00 12 e4 58 e7 00     02:29:29.888  READ DMA
  c8 00 00 00 08 00 00 00 12 e4 50 e7 00     02:29:29.869  READ DMA
  ea 00 00 00 00 00 00 00 00 00 00 a0 00     02:29:29.858  FLUSH CACHE EXT
  ca 00 00 00 08 00 00 00 45 cb e8 e9 00     02:29:29.858  WRITE DMA
  ea 00 00 00 00 00 00 00 00 00 00 a0 00     02:29:29.842  FLUSH CACHE EXT

Error 33869 [76] occurred at disk power-on lifetime: 11322 hours (471 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 45 00 00 00 12 e4 5b e7 00  Error: UNC 69 sectors at LBA = 0x0712e45b = 118678619

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 50 00 00 00 12 e4 50 e7 00     02:29:24.818  READ DMA
  c8 00 00 00 d8 00 00 00 12 e3 78 e7 00     02:29:24.695  READ DMA
  c8 00 00 00 58 00 00 00 12 e3 20 e7 00     02:29:24.588  READ DMA
  c8 00 00 00 48 00 00 00 12 e2 d8 e7 00     02:29:24.482  READ DMA
  c8 00 00 00 58 00 00 00 12 e2 80 e7 00     02:29:24.375  READ DMA

SMART Extended Self-test Log Version: 1 (2 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  2
SCT Version (vendor specific):       0 (0x0000)
Device State:                        Active (0)
Current Temperature:                    34 Celsius
Power Cycle Min/Max Temperature:     --/34 Celsius
Lifetime    Min/Max Temperature:     --/58 Celsius

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      5/60 Celsius
Min/Max Temperature Limit:           -40/65 Celsius
Temperature History Size (Index):    128 (75)

SCT Error Recovery Control:
           Read: Disabled
          Write: Disabled

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  4            0  Command failed due to ICRC error
0x0002  4            0  R_ERR response for data FIS
0x0003  4            0  R_ERR response for device-to-host data FIS
0x0004  4            0  R_ERR response for host-to-device data FIS
0x0005  4            0  R_ERR response for non-data FIS
0x0006  4            0  R_ERR response for device-to-host non-data FIS
0x0008  4            0  Device-to-host non-data FIS retries
0x0009  4         4943  Transition from drive PhyRdy to drive PhyNRdy
0x000a  4           20  Device-to-host register FISes sent due to a COMRESET
0x000b  4            0  CRC errors within host-to-device FIS
0x000d  4            0  Non-CRC errors within host-to-device FIS
0x000f  4            0  R_ERR response for host-to-device data FIS, CRC
0x0010  4            0  R_ERR response for host-to-device data FIS, non-CRC

