smartctl 7.2 2020-12-30 r5155 [FreeBSD 13.0-RELEASE amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Barracuda 7200.10
Device Model:     ST3250310AS
Serial Number:    --
Firmware Version: 3.AAD
User Capacity:    250,059,350,016 bytes [250 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA/ATAPI-7 (minor revision not indicated)
Local Time is:    Sat Mar 12 08:50:21 2022 EST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED
See vendor-specific Attribute list for marginal Attributes.

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  430) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (  92) minutes.
SCT capabilities: 	       (0x0001)	SCT Status supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   100   253   006    -    0
  3 Spin_Up_Time            PO----   097   097   000    -    0
  4 Start_Stop_Count        -O--CK   095   095   020    -    5949
  5 Reallocated_Sector_Ct   PO--CK   100   100   036    -    1
  7 Seek_Error_Rate         POSR--   086   060   030    -    9470021146
  9 Power_On_Hours          -O--CK   071   071   000    -    26116
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   095   095   020    -    5877
187 Reported_Uncorrect      -O--CK   001   001   000    -    1230
189 High_Fly_Writes         -O-RCK   100   100   000    -    0
190 Airflow_Temperature_Cel -O---K   066   039   045    Past 34 (Min/Max 27/34)
194 Temperature_Celsius     -O---K   034   061   000    -    34 (0 11 0 0 0)
195 Hardware_ECC_Recovered  -O-RC-   082   060   000    -    86804714
197 Current_Pending_Sector  -O--C-   100   093   000    -    18
198 Offline_Uncorrectable   ----C-   100   093   000    -    18
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    0
200 Multi_Zone_Error_Rate   ------   100   253   000    -    0
202 Data_Address_Mark_Errs  -O--CK   100   253   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01       GPL,SL  R/O      1  Summary SMART error log
0x02       GPL,SL  R/O      5  Comprehensive SMART error log
0x03       GPL,SL  R/O      5  Ext. Comprehensive SMART error log
0x06       GPL,SL  R/O      1  SMART self-test log
0x07       GPL,SL  R/O      1  Extended self-test log
0x09       GPL,SL  R/W      1  Selective self-test log
0x10       GPL,SL  R/O      1  NCQ Command Error log
0x11       GPL,SL  R/O      1  SATA Phy Event Counters log
0x20       GPL,SL  R/O      1  Streaming performance log [OBS-8]
0x21       GPL,SL  R/O      1  Write stream error log
0x22       GPL,SL  R/O      1  Read stream error log
0x23       GPL,SL  R/O      1  Delayed sector log [OBS-8]
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa0       GPL,SL  VS       1  Device vendor specific log
0xa1       GPL,SL  VS      20  Device vendor specific log
0xa2       GPL,SL  VS     101  Device vendor specific log
0xa8       GPL,SL  VS      20  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer
0xff       GPL     -    23040  Reserved

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 1289 (device log contains only the most recent 20 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 1289 [8] occurred at disk power-on lifetime: 25631 hours (1067 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 07 8d 00 ae 2d e7 00  Error: UNC at LBA = 0x78f00ae2d = 32463957549

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 08 00 07 8d 00 ae 28 e7 00     00:44:55.714  READ DMA
  ca 00 00 00 08 00 00 f8 00 0a a8 e0 00     00:44:55.714  WRITE DMA
  27 00 00 00 00 00 00 00 00 00 00 e0 00     00:44:55.713  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 00 00 01 00 00 ff ff 00 ff ff a0 00     00:44:55.711  IDENTIFY DEVICE
  ef 00 03 00 46 00 ff ff 00 ff ff a0 00     00:44:55.709  SET FEATURES [Set transfer mode]

Error 1288 [7] occurred at disk power-on lifetime: 25631 hours (1067 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 07 a5 00 af 71 e7 00  Error: UNC at LBA = 0x7a700af71 = 32866611057

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 08 00 07 a5 00 af 70 e7 00     00:45:06.404  READ DMA
  27 00 00 00 00 00 00 00 00 00 00 e0 00     00:45:02.349  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 00 00 01 00 00 ff ff 00 ff ff a0 00     00:45:02.349  IDENTIFY DEVICE
  ef 00 03 00 46 00 ff ff 00 ff ff a0 00     00:45:10.478  SET FEATURES [Set transfer mode]
  27 00 00 00 00 00 00 00 00 00 00 e0 00     00:45:10.477  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]

Error 1287 [6] occurred at disk power-on lifetime: 25631 hours (1067 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 07 a5 00 af 71 e7 00  Error: UNC at LBA = 0x7a700af71 = 32866611057

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 08 00 07 a5 00 af 70 e7 00     00:45:06.404  READ DMA
  c8 00 00 00 70 00 00 ba 00 48 10 e0 00     00:45:02.349  READ DMA
  27 00 00 00 00 00 00 00 00 00 00 e0 00     00:45:02.349  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 00 00 01 00 00 ff ff 00 ff ff a0 00     00:45:02.349  IDENTIFY DEVICE
  ef 00 03 00 46 00 ff ff 00 ff ff a0 00     00:45:02.348  SET FEATURES [Set transfer mode]

Error 1286 [5] occurred at disk power-on lifetime: 25631 hours (1067 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 07 a5 00 af 71 e7 00  Error: UNC at LBA = 0x7a700af71 = 32866611057

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 08 00 07 a5 00 af 70 e7 00     00:45:02.346  READ DMA
  c8 00 00 00 08 00 07 a5 00 af 68 e7 00     00:45:02.349  READ DMA
  c8 00 00 00 08 00 07 a5 00 af 60 e7 00     00:45:02.349  READ DMA
  c8 00 00 00 08 00 07 a5 00 af 58 e7 00     00:45:02.349  READ DMA
  c8 00 00 00 08 00 07 a5 00 af 50 e7 00     00:45:02.348  READ DMA

Error 1285 [4] occurred at disk power-on lifetime: 25631 hours (1067 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 07 8d 00 ae 2d e7 00  Error: UNC at LBA = 0x78f00ae2d = 32463957549

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 08 00 07 8d 00 ae 28 e7 00     00:44:55.714  READ DMA
  ca 00 00 00 08 00 00 f8 00 0a a8 e0 00     00:44:55.714  WRITE DMA
  27 00 00 00 00 00 00 00 00 00 00 e0 00     00:44:55.713  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 00 00 01 00 00 ff ff 00 ff ff a0 00     00:44:55.711  IDENTIFY DEVICE
  ef 00 03 00 46 00 ff ff 00 ff ff a0 00     00:44:55.709  SET FEATURES [Set transfer mode]

Error 1284 [3] occurred at disk power-on lifetime: 25631 hours (1067 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 07 a5 00 af 71 e7 00  Error: UNC at LBA = 0x7a700af71 = 32866611057

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 08 00 07 a5 00 af 70 e7 00     00:45:06.404  READ DMA
  27 00 00 00 00 00 00 00 00 00 00 e0 00     00:45:02.349  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 00 00 01 00 00 ff ff 00 ff ff a0 00     00:45:02.349  IDENTIFY DEVICE
  ef 00 03 00 46 00 ff ff 00 ff ff a0 00     00:45:10.478  SET FEATURES [Set transfer mode]
  27 00 00 00 00 00 00 00 00 00 00 e0 00     00:45:10.477  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]

Error 1283 [2] occurred at disk power-on lifetime: 25631 hours (1067 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 07 a5 00 af 71 e7 00  Error: UNC at LBA = 0x7a700af71 = 32866611057

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 08 00 07 a5 00 af 70 e7 00     00:45:06.404  READ DMA
  c8 00 00 00 70 00 00 ba 00 48 10 e0 00     00:45:02.349  READ DMA
  27 00 00 00 00 00 00 00 00 00 00 e0 00     00:45:02.349  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 00 00 01 00 00 ff ff 00 ff ff a0 00     00:45:02.349  IDENTIFY DEVICE
  ef 00 03 00 46 00 ff ff 00 ff ff a0 00     00:45:02.348  SET FEATURES [Set transfer mode]

Error 1282 [1] occurred at disk power-on lifetime: 25631 hours (1067 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 07 a5 00 af 71 e7 00  Error: UNC at LBA = 0x7a700af71 = 32866611057

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 08 00 07 a5 00 af 70 e7 00     00:45:02.346  READ DMA
  c8 00 00 00 08 00 07 a5 00 af 68 e7 00     00:45:02.349  READ DMA
  c8 00 00 00 08 00 07 a5 00 af 60 e7 00     00:45:02.349  READ DMA
  c8 00 00 00 08 00 07 a5 00 af 58 e7 00     00:45:02.349  READ DMA
  c8 00 00 00 08 00 07 a5 00 af 50 e7 00     00:45:02.348  READ DMA

SMART Extended Self-test Log Version: 1 (1 sectors)

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  2
SCT Version (vendor specific):       521 (0x0209)
Device State:                        Active (0)
Current Temperature:                    34 Celsius
Power Cycle Min/Max Temperature:     --/ 0 Celsius
Lifetime    Min/Max Temperature:     --/ 0 Celsius

SCT Data Table command not supported

SCT Error Recovery Control command not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2            3  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x0009  2            2  Transition from drive PhyRdy to drive PhyNRdy
0x8002  2            0  Vendor specific
0x8003  2            1  Vendor specific
0x8004  2            0  Vendor specific

