smartctl 7.0 2018-12-30 r4883 [FreeBSD 11.3-STABLE amd64] (local build)
Copyright (C) 2002-18, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     SAMSUNG SSD RBX Series 64GB M
Serial Number:    --
LU WWN Device Id: 5 0000f0 ...
Firmware Version: VAM05D1Q
User Capacity:    64,023,257,088 bytes [64.0 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
Device is:        Not in smartctl database [for details use: -P showall]
ATA Version is:   ATA/ATAPI-7 T13/1532D revision 1
Local Time is:    Sun Jul 26 12:37:38 2020 -03
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM level is:     254 (maximum performance), recommended: 128
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x02)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  120) seconds.
Offline data collection
capabilities: 			 (0x53) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  12) minutes.

SMART Attributes Data Structure revision number: 1
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  9 Power_On_Hours          -O--CK   094   094   000    -    28373
 12 Power_Cycle_Count       -O--CK   095   095   000    -    4327
175 Program_Fail_Count_Chip -O--CK   100   100   012    -    0
176 Erase_Fail_Count_Chip   -O--CK   100   100   012    -    0
177 Wear_Leveling_Count     PO--C-   100   100   023    -    0
178 Used_Rsvd_Blk_Cnt_Chip  PO--C-   093   093   012    -    4
179 Used_Rsvd_Blk_Cnt_Tot   PO--C-   099   099   010    -    30
180 Unused_Rsvd_Blk_Cnt_Tot PO--C-   050   050   010    -    1954
181 Program_Fail_Cnt_Total  -O--CK   100   100   010    -    0
182 Erase_Fail_Count_Total  -O--CK   100   100   010    -    0
183 Runtime_Bad_Block       PO--C-   100   100   010    -    0
187 Reported_Uncorrect      PO--CK   100   100   000    -    0
195 Hardware_ECC_Recovered  -O-RC-   200   200   000    -    0
198 Offline_Uncorrectable   ----CK   100   100   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   253   253   000    -    0
232 Available_Reservd_Space PO--C-   095   095   012    -    58
233 Media_Wearout_Indicator -O--CK   092   092   000    -    312564335
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 0
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01       GPL,SL  R/O      1  Summary SMART error log
0x02       GPL,SL  R/O      1  Comprehensive SMART error log
0x03       GPL,SL  R/O      1  Ext. Comprehensive SMART error log
0x06       GPL,SL  R/O      1  SMART self-test log
0x07       GPL,SL  R/O      1  Extended self-test log
0x09       GPL,SL  R/W      1  Selective self-test log
0x11       GPL,SL  R/O      1  SATA Phy Event Counters log
0x80-0x9f  GPL,SL  R/W      1  Host vendor specific log

Warning! SMART Extended Comprehensive Error Log Structure error: invalid SMART checksum.
SMART Extended Comprehensive Error Log Version: 1 (1 sectors)
Device Error Count: 28 (device log contains only the most recent 4 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 28 [3] occurred at disk power-on lifetime: 25404 hours (1058 days + 12 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 01 00 00 00 74 0a b0 47 00  Error: IDNF 1 sectors at LBA = 0x07740ab0 = 125045424

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 01 00 00 00 74 0a b0 47 00     00:00:09.000  READ DMA
  c8 00 00 00 01 00 00 00 00 00 01 40 00     00:00:09.000  READ DMA
  c8 00 00 00 01 00 00 00 00 00 00 40 00     00:00:09.000  READ DMA
  c8 00 00 00 01 00 00 00 00 00 00 40 00     00:00:09.000  READ DMA
  b0 00 da 00 00 00 00 00 c2 4f 00 40 00     00:00:08.000  SMART RETURN STATUS

Error 27 [2] occurred at disk power-on lifetime: 25404 hours (1058 days + 12 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 01 00 00 00 74 0a b0 47 00  Error: IDNF 1 sectors at LBA = 0x07740ab0 = 125045424

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 01 00 00 00 74 0a b0 47 00     00:00:11.000  READ DMA
  c8 00 00 00 01 00 00 00 00 00 01 40 00     00:00:11.000  READ DMA
  c8 00 00 00 01 00 00 00 00 00 00 40 00     00:00:11.000  READ DMA
  c8 00 00 00 01 00 00 00 00 00 00 40 00     00:00:11.000  READ DMA
  b0 00 da 00 00 00 00 00 c2 4f 00 40 00     00:00:10.000  SMART RETURN STATUS

Error 26 [1] occurred at disk power-on lifetime: 25402 hours (1058 days + 10 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 01 00 00 00 74 0a b0 47 00  Error: IDNF 1 sectors at LBA = 0x07740ab0 = 125045424

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 01 00 00 00 74 0a b0 47 00     00:00:10.000  READ DMA
  c8 00 00 00 01 00 00 00 00 00 01 40 00     00:00:10.000  READ DMA
  c8 00 00 00 01 00 00 00 00 00 00 40 00     00:00:10.000  READ DMA
  c8 00 00 00 01 00 00 00 00 00 00 40 00     00:00:10.000  READ DMA
  b0 00 da 00 00 00 00 00 c2 4f 00 40 00     00:00:08.000  SMART RETURN STATUS

Error 25 [0] occurred at disk power-on lifetime: 25399 hours (1058 days + 7 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 01 00 00 00 74 0a b0 47 00  Error: IDNF 1 sectors at LBA = 0x07740ab0 = 125045424

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 01 00 00 00 74 0a b0 47 00     00:00:10.000  READ DMA
  c8 00 00 00 01 00 00 00 00 00 01 40 00     00:00:10.000  READ DMA
  c8 00 00 00 01 00 00 00 00 00 00 40 00     00:00:10.000  READ DMA
  c8 00 00 00 01 00 00 00 00 00 00 40 00     00:00:10.000  READ DMA
  b0 00 da 00 00 00 00 00 c2 4f 00 40 00     00:00:09.000  SMART RETURN STATUS

Warning! SMART Extended Self-test Log Structure error: invalid SMART checksum.
SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%     27540         -
# 2  Short offline       Completed without error       00%     27493         -
# 3  Short offline       Completed without error       00%     23863         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Commands not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x0002  2            0  R_ERR response for data FIS
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0005  2            0  R_ERR response for non-data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x0008  2            0  Device-to-host non-data FIS retries
0x0009  2            1  Transition from drive PhyRdy to drive PhyNRdy
0x000a  2            1  Device-to-host register FISes sent due to a COMRESET
0x000b  2            0  CRC errors within host-to-device FIS
0x000d  2            0  Non-CRC errors within host-to-device FIS
0x000f  2            0  R_ERR response for host-to-device data FIS, CRC
0x0010  2            0  R_ERR response for host-to-device data FIS, non-CRC
0x0012  2            0  R_ERR response for host-to-device non-data FIS, CRC
0x0013  2            0  R_ERR response for host-to-device non-data FIS, non-CRC

