smartctl 7.2 2021-09-14 r5236 [FreeBSD 13.0-RELEASE-p5 amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Western Digital Caviar SE Serial ATA
Device Model:     WDC WD800JD-75MSA3
Serial Number:    --
Firmware Version: 10.01E04
User Capacity:    79,995,772,416 bytes [79.9 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA/ATAPI-7 (minor revision not indicated)
Local Time is:    Thu Nov 25 16:32:16 2021 WIB
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM level is:     128 (quiet), recommended: 128
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Unknown

=== START OF READ SMART DATA SECTION ===
SMART Status not supported: Incomplete response, ATA output registers missing
SMART overall-health self-assessment test result: PASSED
Warning: This result is based on an Attribute check.
See vendor-specific Attribute list for marginal Attributes.

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		( 2460) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  33) minutes.
Conveyance self-test routine
recommended polling time: 	 (   6) minutes.
SCT capabilities: 	       (0x103f)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   200   200   051    -    770
  3 Spin_Up_Time            PO----   161   159   021    -    2916
  4 Start_Stop_Count        -O--CK   094   094   000    -    6546
  5 Reallocated_Sector_Ct   PO--CK   200   200   140    -    0
  7 Seek_Error_Rate         POSR--   200   200   051    -    0
  9 Power_On_Hours          -O--CK   079   079   000    -    15753
 10 Spin_Retry_Count        PO--C-   100   100   051    -    0
 11 Calibration_Retry_Count -O--C-   100   100   051    -    0
 12 Power_Cycle_Count       -O--CK   095   095   000    -    5523
190 Airflow_Temperature_Cel -O---K   059   029   045    Past 41
194 Temperature_Celsius     -O---K   102   072   000    -    41
196 Reallocated_Event_Count -O--CK   200   200   000    -    0
197 Current_Pending_Sector  -O--C-   200   200   000    -    0
198 Offline_Uncorrectable   ----C-   200   200   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    13359
200 Multi_Zone_Error_Rate   P--R--   200   200   051    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      6  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa0-0xa7  GPL,SL  VS      16  Device vendor specific log
0xa8-0xb7  GPL,SL  VS       1  Device vendor specific log
0xc0       GPL,SL  VS       1  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (6 sectors)
Device Error Count: 2947 (device log contains only the most recent 24 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 2947 [18] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 00 01 01 00 51 00 00 40 01 00 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  00 99 29 87 9a 00 00 00 00 00 02 00 00     00:00:00.000  NOP [Reserved subcommand] [OBS-ACS-2]
  00 01 00 00 7a 87 99 00 9a 29 00 02 00     00:00:31.489  NOP [Abort queued commands]
  00 98 29 87 9a 00 01 00 79 00 02 00 00     11:47:21.368  NOP [Reserved subcommand] [OBS-ACS-2]
  00 01 00 00 77 87 98 00 9a 29 00 02 00     00:00:30.721  NOP [Abort queued commands]

Error 2946 [17] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 00 01 26 00 51 00 00 40 01 00 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  00 12 29 87 8d 00 00 00 00 00 02 00 00     00:00:00.000  NOP [Reserved subcommand] [OBS-ACS-2]
  00 26 00 00 4c 87 b6 00 8c 29 00 02 00     00:00:29.222  NOP [Abort queued commands]
  00 ff 29 87 8b 00 26 00 26 00 02 00 00     11:47:17.723  NOP [Reserved subcommand] [OBS-ACS-2]
  00 26 00 00 da 87 a4 00 8b 29 00 02 00     00:00:00.038  NOP [Abort queued commands]

Error 2945 [16] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 00 01 00 00 51 00 00 e0 01 00 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  00 7c c8 b1 ce 00 00 00 00 00 01 00 00     00:00:00.000  NOP [Reserved subcommand] [OBS-ACS-2]
  00 00 00 00 00 b1 63 00 ce 27 00 01 00     00:00:51.208  NOP [Abort queued commands]
  00 60 ef b1 ce 00 00 00 00 00 01 00 00     07:53:49.921  NOP [Reserved subcommand] [OBS-ACS-2]
  00 00 00 00 00 b1 60 00 ce 27 00 01 00     00:00:00.070  NOP [Abort queued commands]

Error 2944 [15] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 00 01 00 00 51 00 00 e0 01 00 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  00 9f c8 b1 c6 00 00 00 00 00 01 00 00     00:00:00.000  NOP [Reserved subcommand] [OBS-ACS-2]
  00 00 00 00 00 b1 af 00 5e 27 00 01 00     00:00:51.208  NOP [Abort queued commands]
  00 ac ef b1 5e 00 00 00 00 00 01 00 00     07:53:21.324  NOP [Reserved subcommand] [OBS-ACS-2]
  00 00 00 00 00 b1 ac 00 5e 27 00 01 00     00:00:00.070  NOP [Abort queued commands]

Error 2943 [14] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 00 01 00 00 51 00 00 e0 01 00 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  00 24 c8 b1 57 00 00 00 00 00 01 00 00     00:00:00.000  NOP [Reserved subcommand] [OBS-ACS-2]
  00 00 00 00 00 b1 1d 00 57 27 00 01 00     00:00:51.208  NOP [Abort queued commands]
  00 1a ef b1 57 00 00 00 00 00 01 00 00     07:53:19.386  NOP [Reserved subcommand] [OBS-ACS-2]
  00 00 00 00 00 b1 1a 00 57 27 00 01 00     00:00:00.070  NOP [Abort queued commands]

Error 2942 [13] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 00 01 00 00 51 00 00 e0 01 00 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  00 a8 c8 b1 4f 00 00 00 00 00 01 00 00     00:00:00.000  NOP [Reserved subcommand] [OBS-ACS-2]
  00 08 00 00 c0 b1 a8 00 4f c8 00 01 00     00:00:51.208  NOP [Abort queued commands]
  00 a7 c8 b1 4f 00 08 00 b8 00 01 00 00     07:53:17.479  NOP [Reserved subcommand] [OBS-ACS-2]
  00 08 00 00 a8 b1 a7 00 4f c8 00 01 00     00:00:45.064  NOP [Abort queued commands]

Error 2941 [12] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 00 01 00 00 51 00 00 e0 01 00 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  00 9a 25 b1 47 00 00 00 00 00 01 00 00     00:00:00.000  NOP [Reserved subcommand] [OBS-ACS-2]
  00 00 00 00 00 b1 95 00 47 25 00 01 00     00:00:00.000  NOP [Abort queued commands]
  00 89 25 b1 47 00 00 00 00 00 01 00 00     07:53:15.410  NOP [Reserved subcommand] [OBS-ACS-2]
  00 00 00 00 00 b1 7d 00 47 25 00 01 00     00:00:00.000  NOP [Abort queued commands]

Error 2940 [11] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 00 01 00 00 51 00 00 e4 01 00 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  00 13 c8 8e f6 00 00 00 00 00 00 00 04     00:00:00.000  NOP [Reserved subcommand] [OBS-ACS-2]
  00 00 00 00 00 8e 00 00 f6 27 00 00 00     00:00:35.585  NOP [Abort queued commands]
  00 f8 ef 8e f5 00 00 00 00 00 00 00 00     02:36:09.080  NOP [Reserved subcommand] [OBS-ACS-2]
  00 00 00 00 00 8e f8 00 f5 27 00 00 00     00:00:00.070  NOP [Abort queued commands]

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%     14297         -
# 2  Extended offline    Completed without error       00%     14245         -
# 3  Conveyance offline  Completed without error       00%     13758         -
# 4  Extended offline    Completed without error       00%     13758         -
# 5  Short offline       Completed without error       00%     13757         -
# 6  Extended offline    Completed: read failure       90%     12877         15890811
# 7  Short offline       Completed without error       00%     12877         -
# 8  Extended offline    Completed without error       00%     12647         -
# 9  Short offline       Completed without error       00%     12646         -
#10  Conveyance offline  Completed without error       00%     12457         -
#11  Short offline       Completed without error       00%     12457         -
#12  Short offline       Completed without error       00%     12426         -
#13  Short offline       Completed without error       00%     11935         -
#14  Extended offline    Completed without error       00%     11934         -
#15  Short offline       Completed: read failure       50%     11933         2397642
#16  Short offline       Completed: read failure       50%     11917         2397642
#17  Extended offline    Completed without error       00%     11699         -
#18  Short offline       Completed without error       00%     11344         -
3 of 3 failed self-tests are outdated by newer successful extended offline self-test # 2

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  2
SCT Version (vendor specific):       258 (0x0102)
Device State:                        Active (0)
Current Temperature:                    41 Celsius
Power Cycle Min/Max Temperature:     --/41 Celsius
Lifetime    Min/Max Temperature:     --/71 Celsius

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      5/65 Celsius
Min/Max Temperature Limit:            1/70 Celsius
Temperature History Size (Index):    128 (126)

SMART WRITE LOG does not return COUNT and LBA_LOW register
SCT (Get) Error Recovery Control command failed

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x000a  2            1  Device-to-host register FISes sent due to a COMRESET
0x8000  4       185701  Vendor specific

