smartctl 7.1 2019-12-30 r5022 [FreeBSD 12.1-RELEASE-p8 amd64] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Barracuda 7200.14 (AF)
Device Model:     ST1000DM003-1ER162
Serial Number:    --
LU WWN Device Id: 5 000c50 ...
Firmware Version: CC45
User Capacity:    1,000,204,886,016 bytes [1.00 TB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Rotation Rate:    7200 rpm
Form Factor:      3.5 inches
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ACS-2, ACS-3 T13/2161-D revision 3b
SATA Version is:  SATA 3.1, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Sun Aug 23 14:36:31 2020 CEST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     128 (minimum power consumption without standby)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(   80) seconds.
Offline data collection
capabilities: 			 (0x73) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 ( 105) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x1085)	SCT Status supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   118   099   006    -    181375400
  3 Spin_Up_Time            PO----   097   097   000    -    0
  4 Start_Stop_Count        -O--CK   095   095   020    -    5695
  5 Reallocated_Sector_Ct   PO--CK   100   100   010    -    8
  7 Seek_Error_Rate         POSR--   071   060   030    -    13537186
  9 Power_On_Hours          -O--CK   084   084   000    -    14163
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   095   095   020    -    5621
183 Runtime_Bad_Block       -O--CK   100   100   000    -    0
184 End-to-End_Error        -O--CK   100   100   099    -    0
187 Reported_Uncorrect      -O--CK   076   076   000    -    24
188 Command_Timeout         -O--CK   100   099   000    -    0 0 12
189 High_Fly_Writes         -O-RCK   098   098   000    -    2
190 Airflow_Temperature_Cel -O---K   056   054   045    -    44 (Min/Max 32/44)
191 G-Sense_Error_Rate      -O--CK   100   100   000    -    0
192 Power-Off_Retract_Count -O--CK   100   100   000    -    961
193 Load_Cycle_Count        -O--CK   070   070   000    -    60518
194 Temperature_Celsius     -O---K   044   046   000    -    44 (0 9 0 0 0)
197 Current_Pending_Sector  -O--C-   100   100   000    -    0
198 Offline_Uncorrectable   ----C-   100   100   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    0
240 Head_Flying_Hours       ------   100   253   000    -    10652h+57m+05.143s
241 Total_LBAs_Written      ------   100   253   000    -    5696639754
242 Total_LBAs_Read         ------   100   253   000    -    45352586891
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      5  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x21       GPL     R/O      1  Write stream error log
0x22       GPL     R/O      1  Read stream error log
0x30       GPL,SL  R/O      9  IDENTIFY DEVICE data log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS      20  Device vendor specific log
0xa2       GPL     VS    4496  Device vendor specific log
0xa8       GPL,SL  VS     129  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xab       GPL     VS       1  Device vendor specific log
0xb0       GPL     VS    5176  Device vendor specific log
0xbe-0xbf  GPL     VS   65535  Device vendor specific log
0xc0       GPL,SL  VS       1  Device vendor specific log
0xc1       GPL,SL  VS      10  Device vendor specific log
0xc3       GPL,SL  VS       8  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 24 (device log contains only the most recent 20 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 24 [3] occurred at disk power-on lifetime: 13308 hours (554 days + 12 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 17 06 93 77 00 00  Error: UNC at LBA = 0x17069377 = 386306935

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 20 20 00 01 00 00 17 06 93 77 e0 00     01:05:49.657  READ DMA EXT
  35 20 20 00 01 00 00 17 06 93 76 e0 00     01:05:49.657  WRITE DMA EXT
  25 20 20 00 01 00 00 17 06 93 76 e0 00     01:05:49.616  READ DMA EXT
  25 20 20 00 01 00 00 17 06 93 77 e0 00     01:05:49.050  READ DMA EXT
  25 20 20 00 01 00 00 17 06 93 76 e0 00     01:05:49.049  READ DMA EXT

Error 23 [2] occurred at disk power-on lifetime: 13308 hours (554 days + 12 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 17 06 93 77 00 00  Error: UNC at LBA = 0x17069377 = 386306935

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 20 20 00 01 00 00 17 06 93 77 e0 00     01:05:49.050  READ DMA EXT
  25 20 20 00 01 00 00 17 06 93 76 e0 00     01:05:49.049  READ DMA EXT
  35 20 20 00 01 00 00 17 06 93 76 e0 00     01:05:49.049  WRITE DMA EXT
  35 20 20 00 01 00 00 17 06 93 75 e0 00     01:05:49.049  WRITE DMA EXT
  35 20 20 00 01 00 00 17 06 93 76 e0 00     01:05:49.048  WRITE DMA EXT

Error 22 [1] occurred at disk power-on lifetime: 13308 hours (554 days + 12 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 17 06 93 76 00 00  Error: UNC at LBA = 0x17069376 = 386306934

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 20 20 00 01 00 00 17 06 93 76 e0 00     01:05:44.956  READ DMA EXT
  35 20 20 00 01 00 00 17 06 93 75 e0 00     01:05:44.956  WRITE DMA EXT
  25 20 20 00 01 00 00 17 06 93 75 e0 00     01:05:44.915  READ DMA EXT
  25 20 20 00 01 00 00 17 06 93 76 e0 00     01:05:44.349  READ DMA EXT
  25 20 20 00 01 00 00 17 06 93 75 e0 00     01:05:44.348  READ DMA EXT

Error 21 [0] occurred at disk power-on lifetime: 13308 hours (554 days + 12 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 17 06 93 76 00 00  Error: UNC at LBA = 0x17069376 = 386306934

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 20 20 00 01 00 00 17 06 93 76 e0 00     01:05:44.349  READ DMA EXT
  25 20 20 00 01 00 00 17 06 93 75 e0 00     01:05:44.348  READ DMA EXT
  35 20 20 00 01 00 00 17 06 93 75 e0 00     01:05:44.348  WRITE DMA EXT
  35 20 20 00 01 00 00 17 06 93 74 e0 00     01:05:44.348  WRITE DMA EXT
  35 20 20 00 01 00 00 17 06 93 75 e0 00     01:05:44.347  WRITE DMA EXT

Error 20 [19] occurred at disk power-on lifetime: 13308 hours (554 days + 12 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 17 06 93 75 00 00  Error: UNC at LBA = 0x17069375 = 386306933

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 20 20 00 01 00 00 17 06 93 75 e0 00     01:05:40.105  READ DMA EXT
  35 20 20 00 01 00 00 17 06 93 74 e0 00     01:05:40.105  WRITE DMA EXT
  25 20 20 00 01 00 00 17 06 93 74 e0 00     01:05:40.064  READ DMA EXT
  25 20 20 00 01 00 00 17 06 93 75 e0 00     01:05:39.499  READ DMA EXT
  25 20 20 00 01 00 00 17 06 93 74 e0 00     01:05:39.497  READ DMA EXT

Error 19 [18] occurred at disk power-on lifetime: 13308 hours (554 days + 12 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 17 06 93 75 00 00  Error: UNC at LBA = 0x17069375 = 386306933

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 20 20 00 01 00 00 17 06 93 75 e0 00     01:05:39.499  READ DMA EXT
  25 20 20 00 01 00 00 17 06 93 74 e0 00     01:05:39.497  READ DMA EXT
  35 20 20 00 01 00 00 17 06 93 74 e0 00     01:05:39.497  WRITE DMA EXT
  35 20 20 00 01 00 00 17 06 93 73 e0 00     01:05:39.497  WRITE DMA EXT
  35 20 20 00 01 00 00 17 06 93 74 e0 00     01:05:39.497  WRITE DMA EXT

Error 18 [17] occurred at disk power-on lifetime: 13308 hours (554 days + 12 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 17 06 93 74 00 00  Error: UNC at LBA = 0x17069374 = 386306932

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 20 20 00 01 00 00 17 06 93 74 e0 00     01:05:35.396  READ DMA EXT
  35 20 20 00 01 00 00 17 06 93 73 e0 00     01:05:35.396  WRITE DMA EXT
  25 20 20 00 01 00 00 17 06 93 73 e0 00     01:05:35.355  READ DMA EXT
  25 20 20 00 01 00 00 17 06 93 74 e0 00     01:05:34.789  READ DMA EXT
  25 20 20 00 01 00 00 17 06 93 73 e0 00     01:05:34.788  READ DMA EXT

Error 17 [16] occurred at disk power-on lifetime: 13308 hours (554 days + 12 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 17 06 93 74 00 00  Error: UNC at LBA = 0x17069374 = 386306932

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 20 20 00 01 00 00 17 06 93 74 e0 00     01:05:34.789  READ DMA EXT
  25 20 20 00 01 00 00 17 06 93 73 e0 00     01:05:34.788  READ DMA EXT
  35 20 20 00 01 00 00 17 06 93 73 e0 00     01:05:34.788  WRITE DMA EXT
  35 20 20 00 01 00 00 17 06 93 72 e0 00     01:05:34.788  WRITE DMA EXT
  35 20 20 00 01 00 00 17 06 93 73 e0 00     01:05:34.787  WRITE DMA EXT

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%     13308         -
# 2  Short offline       Completed: read failure       90%     13307         386306928
# 3  Short offline       Completed: read failure       90%     13307         386306928
# 4  Short offline       Completed: read failure       90%     13307         386306928
# 5  Short offline       Completed: read failure       90%     13306         386306928

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       522 (0x020a)
Device State:                        Active (0)
Current Temperature:                    43 Celsius
Power Cycle Min/Max Temperature:     32/43 Celsius
Lifetime    Min/Max Temperature:      9/46 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Data Table command not supported

SCT Error Recovery Control command not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2           15  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS

